-- Copyright(c) 2006-2007, LSI Logic Corporation
-- MIB file for MegaRAID SAS IR controllers
-- File: 1.11
-- Previous:1.10 
-- Date: 24-04-2007   
-- Revision : tParentIndex description has been updated
-- Revision : Temperature unit added in the description of enclosureTemperature, and spareType description has been updated
-- Revision : pdtInserted Trap description has been updated. Trap CATEGORY has been changed to "Error Events".
--				 ir Trap prefix has been inserted for Trap naming conflict with sas mib in HPOV.
-- Revision : Trap decsription has been modified and Trap ID has been changed from 9000 series to 7000 series
-- Revision : in pdtPredictiveThresholdExceed Trap, Trap Spelling Predictive corrected
-- Revision : Predictive Failure Trap inserted
-- Revision : Some MIB Description changed
-- Revision : Some MIB Description changed
-- Revision : SYNTAX  INTEGER (0..2) implemented for VDDiskCache Policy
-- Revision :  Add a new Trap pdtSMARTAlert
-- Revision : For LSI SAS IR support

LSI-megaRAID-SAS-IR-MIB DEFINITIONS ::= BEGIN
IMPORTS
    enterprises, Counter        FROM RFC1155-SMI
    Gauge                       FROM RFC1155-SMI
    PhysAddress                 FROM RFC1213-MIB
    DisplayString               FROM RFC1213-MIB
    OBJECT-TYPE                 FROM RFC-1212
    TRAP-TYPE                   FROM RFC-1215;

--
-- LSI specific object identifiers.
--
lsi   OBJECT IDENTIFIER ::= {enterprises 3582}
lsiStorageComponents    OBJECT IDENTIFIER ::= { lsi 5 }
lsiRAIDServer              OBJECT IDENTIFIER ::= { lsiStorageComponents 1 }

--------------------------------------------------------------------------------
--
-- Server Information group.
--
--------------------------------------------------------------------------------
hostName                     OBJECT-TYPE
    SYNTAX                     DisplayString (SIZE(0..63))
    ACCESS                     read-only
    STATUS                     mandatory
    DESCRIPTION                "Name of the host system wih IP address."
    ::= { lsiRAIDServer 1 }
hostOSInfo                     OBJECT-TYPE
    SYNTAX                     DisplayString (SIZE(0..63))
    ACCESS                     read-only
    STATUS                     mandatory
    DESCRIPTION                "Operating System description where SNMP agent is running."
    ::= { lsiRAIDServer 2 }
--------------------------------------------------------------------------------
--
-- Version Information group.
--
--------------------------------------------------------------------------------
versionInfo                     OBJECT IDENTIFIER ::= {lsiRAIDServer 3}

mibVersion                      OBJECT-TYPE
    SYNTAX                      DisplayString (SIZE(0..63))
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The MIB version no. (xx.yy.zz)"
    ::= { versionInfo 1 }

agentModuleName                 OBJECT-TYPE
    SYNTAX                      DisplayString (SIZE(0..63))
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The agent module name"
    ::= { versionInfo 2 }

agentModuleVersion              OBJECT-TYPE
    SYNTAX                      DisplayString (SIZE(0..63))
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The module version in xx.yy format. Where xx is the major version number and yy is the minor version number(without build information)."
    ::= { versionInfo 3 }

releaseDate                     OBJECT-TYPE
    SYNTAX                      DisplayString (SIZE(0..63))
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Module Release Date (DD/MM/YYYY)"
    ::= { versionInfo 4 }

--------------------------------------------------------------------------------

megaRAID-SAS-IR                           OBJECT IDENTIFIER ::= { lsiRAIDServer 4 }
--------------------------------------------------------------------------------
--
-- Management/monitoring MIB object groups.
--
--------------------------------------------------------------------------------

adapter                         OBJECT IDENTIFIER ::= {megaRAID-SAS-IR 1}
adapterDetails                         OBJECT IDENTIFIER ::= {adapter 1}

-- Adapter Table Definition----------------------------------------------------

adpNumber                       OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The total no of SAS adapters present."
    ::= { adapterDetails 1 }

adapterPropertiesTable               OBJECT-TYPE
    SYNTAX                      SEQUENCE OF AdapterPropertiesEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of adapter Entries containing Information/Properties about the adapters."
    ::= { adapterDetails 2 }

    adapterPropertiesEntry                OBJECT-TYPE
    SYNTAX                      AdapterPropertiesEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the adapter table."
    INDEX                       { adapterID }
    ::= { adapterPropertiesTable 1 }

    AdapterPropertiesEntry ::=
        SEQUENCE {
    adapterID               INTEGER,
    rebuildRate             INTEGER,
    reconstructionRate      INTEGER,
    alarmState              INTEGER,
    cacheFlushInteval       INTEGER,
    clusterState            INTEGER,
	predFailPollInterval    INTEGER,
	intThrottleCount        INTEGER,
	intThrottleTimeUs       INTEGER,
	patrolReadRate          INTEGER,
	bgiRate                 INTEGER,
	ccRate                  INTEGER,
	spinupDelay             INTEGER,
	spinupDriveCount        INTEGER,
	coercionMode            INTEGER,
	disableAutoRebuild       INTEGER,
	disableBatteryWarning    INTEGER
    }

-- defines for each attribute in AdapterEntry

adapterID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "AdapterID for this Adapter.(Unique)"
    ::= { adapterPropertiesEntry 1 }

rebuildRate                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Rebuild rate on this Adapter."
    ::= { adapterPropertiesEntry 2 }

reconstructionRate              OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Reconstruction rate on this Adapter."
    ::= { adapterPropertiesEntry 3 }

alarmState                      OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Alarm is enabled(1) or disabled(0) on this adapter."
    ::= { adapterPropertiesEntry 4 }

cacheFlushInteval                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Cache flush interval in seconds for this adapter."
    ::= { adapterPropertiesEntry 5 }
    
clusterState                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Cluster is enabled(1) or disabled(0) on this adapter."
    ::= { adapterPropertiesEntry 6 }

predFailPollInterval            OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of seconds between predictive fail polls on this adapter."
    ::= { adapterPropertiesEntry 7 }

intThrottleCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Interrupt throttle active count on this adapter."
    ::= { adapterPropertiesEntry 8 }

intThrottleTimeUs               OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Interrupt throttle completion hold time on this adapter."
    ::= { adapterPropertiesEntry 9 }

patrolReadRate                  OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Patrol Read Rate for this adapter."
    ::= { adapterPropertiesEntry 10 }

bgiRate                         OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Background initialization rate for this adapter."
    ::= { adapterPropertiesEntry 11 }
ccRate                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Consistency Check rate on this Adapter."
    ::= { adapterPropertiesEntry 12 }

spinupDelay                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of seconds to delay among spinup groups for this adapter."
    ::= { adapterPropertiesEntry 13 }

spinupDriveCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Maximum number of drives to spin up at one time for this adapter."
    ::= { adapterPropertiesEntry 14 }
    
coercionMode                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Drive capacity coercion mode. 0->None; 1->128MB; 2->1GB"
    ::= { adapterPropertiesEntry 15 }

disableAutoRebuild                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "auto-rebuild and hot-spare commissioning status. 1->Disable , 0->Enable"
    ::= { adapterPropertiesEntry 16 }

disableBatteryWarning                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "disable/enable warnings for missing battery or missing HW status. 1->Disable , 0->Enable"
    ::= { adapterPropertiesEntry 17 }

--------------start adp info-------------------------------------
adapterInfoTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF AdapterInfoEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of adapter Entries containing Information/Properties about the adapters."
    
    ::= { adapterDetails 3 }

    adapterInfoEntry                OBJECT-TYPE
    SYNTAX                      AdapterInfoEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the adapterInfo table."
    INDEX                       { adapterID }
    ::= { adapterInfoTable 1 }

    AdapterInfoEntry ::=
        SEQUENCE {
	infAdpID           INTEGER,
	vendorId         INTEGER,
	devId         INTEGER,
	subVendorID         INTEGER,
	subDevID         INTEGER,
	hostInterface    INTEGER,
	hostInterfacePortCnt         INTEGER,
	hostInterfacePortAddr         DisplayString,
	devInterface    DisplayString,
	devInterfacePortCnt         INTEGER,
	devInterfacePortAddr         DisplayString,
	productName         DisplayString,
	serialNo         DisplayString,
	firmwareVersion         DisplayString,
	driverVersion         DisplayString,
	nvramSize            INTEGER,
	memorySize            INTEGER,
	flashSize            INTEGER,
	vdPresentCount       INTEGER,
	vdDegradedCount       INTEGER,
	vdOfflineCount       INTEGER,
	pdPresentCount       INTEGER,
	pdDiskPresentCount       INTEGER,
	pdDiskPredFailureCount       INTEGER,
	pdDiskFailedCount       INTEGER,
	clusterStatus         INTEGER
        }

-- defines for each attribute in AdapterEntry

infAdpID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "AdapterID for this Adapter.(Unique)"
    ::= { adapterInfoEntry 1 }

vendorId                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "PCI Vendor ID for this Adapter."
    ::= { adapterInfoEntry 2 }

devId                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "PCI Device ID for this Adapter."
    ::= { adapterInfoEntry 3 }

subVendorID                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "PCI Sub-Vendor ID for this adapter."
    ::= { adapterInfoEntry 4 }
subDevID                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "PCI Sub-Device ID for this adapter."
    ::= { adapterInfoEntry 5 }
hostInterface                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Host interface information for this adapter.
	                             Values are as follows:
								 N/A(0), PCIX(1), PCIE(2), iSCSI(3), SAS_3G(4)"
    ::= { adapterInfoEntry 6 }
hostInterfacePortCnt                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Port Count on this adapter."
    ::= { adapterInfoEntry 7 }
hostInterfacePortAddr                 OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Port address comma delimited"
    ::= { adapterInfoEntry 8 }
devInterface                 OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Device (backend) interface supported on this adapter.SPI(1),SAS_3G(2),SATA_1_5G(3),SATA_3G(4). For multiple support comma delimited values will appear."
    ::= { adapterInfoEntry 9 }
devInterfacePortCnt           OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Device Port Count on this adapter."
    ::= { adapterInfoEntry 10 }
devInterfacePortAddr                 OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Device Port address comma delimited"
    ::= { adapterInfoEntry 11 }
productName                 OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Product name e.g. MegaRAID SAS-8E, MegaRAID SAS-4X, etc."
    ::= { adapterInfoEntry 12 }
serialNo                 OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Controller serial number"
    ::= { adapterInfoEntry 13 }

firmwareVersion                 OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Firmware version Format->(Firmware Package Version:Version:Date:Time)"
    ::= { adapterInfoEntry 14 }
    
driverVersion                 OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Driver version Format->(Driver Name:Version)"
    ::= { adapterInfoEntry 15 }

nvramSize                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "NVRAM size in KB for this adapter."
    ::= { adapterInfoEntry 16 }

memorySize                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Memory size in MB for this adapter."
    ::= { adapterInfoEntry 17 }

flashSize                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Flash size in MB for this adapter."
    ::= { adapterInfoEntry 18 }
vdPresentCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Virtual  devices present in this adapter."
    ::= { adapterInfoEntry 19 }
vdDegradedCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of virtual  devices in this adapter those are critical"
    ::= { adapterInfoEntry 20 }
vdOfflineCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of virtual  devices in this adapter those are offline"
    ::= { adapterInfoEntry 21 }
pdPresentCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Physical devices present in this adapter."
    ::= { adapterInfoEntry 22 }
pdDiskPresentCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Physical disk devices present in this adapter."
    ::= { adapterInfoEntry 23 }
pdDiskPredFailureCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of disk devices in this adapter those are critical"
    ::= { adapterInfoEntry 24 }
pdDiskFailedCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of disk devices in this adapter those are failed"
    ::= { adapterInfoEntry 25 }
clusterStatus                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Cluster state on this adapter. Values: ACTIVE(1), INACTIVE(0)"
    ::= { adapterInfoEntry 26 }

--------------end adp info          
--------------start adp support info
adapterSupportInfoTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF AdapterSupportInfoEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of  Entries containing Properties supported by the Controller."
    ::= { adapterDetails 4 }

    adapterSupportInfoEntry                OBJECT-TYPE
    SYNTAX                      AdapterSupportInfoEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the adapter table."
    INDEX                       { adapterID }
    ::= { adapterSupportInfoTable 1 }

    AdapterSupportInfoEntry ::=
        SEQUENCE {
            suAdpID           INTEGER,
            supportMaxArms         INTEGER,
            supportMaxSpans         INTEGER,
            supportMaxArrays         INTEGER,
            supportMaxLDs         INTEGER,
            supportHardwarePresent    DisplayString,
			supportMaxConcurrentCmds         INTEGER,
			supportMaxSGECount         INTEGER,
			supportMaxRequestSize         INTEGER,
			supportClusterPermitted         INTEGER,
			supportMinStripeSize  INTEGER,
			supportMaxStripeSize  INTEGER,
			supportSupportsSAS              INTEGER,
			supportSupportsSATA       INTEGER,
			supportAllowMixInEnclosure            INTEGER,
			supportAllowMixInVD       INTEGER,
			supportAllowSataInCluster  INTEGER

        }

-- defines for each attribute in AdapterEntry

suAdpID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "AdapterID for this Adapter.(Unique)"
    ::= { adapterSupportInfoEntry 1 }

supportMaxArms                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Maximum arms per Logical Drive supported for this Adapter."
    ::= { adapterSupportInfoEntry 2 }

supportMaxSpans                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Maximum spans per Logical Drive supported for this Adapter."
    ::= { adapterSupportInfoEntry 3 }

supportMaxArrays                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Maximum number arrays supported this Adapter."
    ::= { adapterSupportInfoEntry 4 }
supportMaxLDs                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Maximum number of Logical Drive's supported for this Adapter."
    ::= { adapterSupportInfoEntry 5 }     
supportHardwarePresent                 OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Supported Hardware on this adapter. bbu(1),alarm(2),nvram(3),uart(4). For multiple hardware support a comma delimited list will appear."
    ::= { adapterSupportInfoEntry 6 }     
supportMaxConcurrentCmds                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The maximum parallel commands supported on this Adapter."
    ::= { adapterSupportInfoEntry 7 }
supportMaxSGECount                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The maximum Scatter Gather Element count allowed on this Adapter."
    ::= { adapterSupportInfoEntry 8 }
supportMaxRequestSize                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The maximum data transfer size in sectors, on this Adapter."
    ::= { adapterSupportInfoEntry 9 }
supportClusterPermitted                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Clustering support on this Adapter. Values: FALSE(0), TRUE(1)"
    ::= { adapterSupportInfoEntry 10 }
supportMinStripeSize                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Minimum stripe size supported. 0(512),1(1K),2(2K),3(4K),4(8K),5(16K),6(32),7(64K),8(128K) ... 11(1MB) etc"
    ::= { adapterSupportInfoEntry 11 }

supportMaxStripeSize                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Maximum stripe size supported. 0(512),1(1K),2(2K),3(4K),4(8K),5(16K),6(32),7(64K),8(128K) ... 11(1MB) etc"
    ::= { adapterSupportInfoEntry 12 }
supportSupportsSAS              OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "SAS physical drive support.Values: notSupported(0), supported(1)"
    ::= { adapterSupportInfoEntry 13 }
supportSupportsSATA              OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "SATA physical drive support.Values: notSupported(0), supported(1)"
    ::= { adapterSupportInfoEntry 14 }
supportAllowMixInEnclosure              OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Mix InEnclosure support.Values: notSupported(0), supported(1)"
    ::= { adapterSupportInfoEntry 15 }
supportAllowMixInVD              OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "MixInVD support.Values: notSupported(0), supported(1)"
    ::= { adapterSupportInfoEntry 16 }
supportAllowSataInCluster              OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "SataInCluster support. Values: notSupported(0), supported(1)"
    ::= { adapterSupportInfoEntry 17 }


--------------end adp info
--------------start adp operations support info
adpOperationsSupportInfoTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF AdpOperationsSupportInfoEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of  Entries containing operations supported by the Controller."
    ::= { adapterDetails 5 }

    adpOperationsSupportInfoEntry                OBJECT-TYPE
    SYNTAX                      AdpOperationsSupportInfoEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the adapter table."
    INDEX                       { opAdpID }
    ::= { adpOperationsSupportInfoTable 1 }

    AdpOperationsSupportInfoEntry ::=
        SEQUENCE {
            opAdpID           INTEGER,
            rbldRate         INTEGER,
            suCCRate         INTEGER,
            suBgiRate         INTEGER,
            reconRate         INTEGER,
            patrolRate    INTEGER,
			alarmControl         INTEGER,
			clusterSupported         INTEGER,
            bbu    INTEGER,
			spanningAllowed         INTEGER,
			dedicatedHotSpares         INTEGER,
			revertibleHotSpares         INTEGER,
			foreignConfigImport         INTEGER,
			selfDiagnostic         INTEGER,
			allowMixedRedundancyOnArray         INTEGER,
			globalHotSpares INTEGER
        }

-- defines for each attribute in AdapterEntry

opAdpID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "AdapterID for this Adapter.(Unique)"
    ::= { adpOperationsSupportInfoEntry 1 }

rbldRate                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Rebuilding rate change support for this Adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 2 }

suCCRate                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Consistency Check rate change support for this Adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 3 }

suBgiRate                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Background initialization rate change support for this adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 4 }
reconRate                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Reconstruction rate change support for this adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 5 }
patrolRate                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Patrol read rate change support for this adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 6 }
alarmControl                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Alarm control support for this adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 7 }
clusterSupported                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Cluster support for this adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 8 }
bbu                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "BBU support for this adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 9 }
spanningAllowed                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Spanning support for this adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 10 }
dedicatedHotSpares                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Dedicated HotSpares for this adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 11 }
revertibleHotSpares                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Revertible HotSpares support for this adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 12 }
foreignConfigImport                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Support foreign config import on this adapter. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 13 }
selfDiagnostic                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Controller supports self diagnostic. Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 14 }
allowMixedRedundancyOnArray                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Allow different Virtual Disk on the same array to have different redundancy levels
	                             Values: False(0), True(1)"
    ::= { adpOperationsSupportInfoEntry 15 }
globalHotSpares                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Global hot spares are supported. Values: False(0), True(1) "
    ::= { adpOperationsSupportInfoEntry 16 }

--------------end adp info
driveOperationSupportTable               OBJECT-TYPE
    SYNTAX                      SEQUENCE OF DriveOperationSupportEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of operations supported by Physical Drive."
    ::= { adapterDetails 6 }

    driveOperationSupportEntry          OBJECT-TYPE
    SYNTAX                      DriveOperationSupportEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the driveOperationSupport table."
    INDEX                       { drvAdpID }
    ::= { driveOperationSupportTable 1 }

    DriveOperationSupportEntry ::=
        SEQUENCE {
        drvAdpID               INTEGER,
        forceOnline               INTEGER,
        forceOffline             INTEGER,
        forceRebuild      INTEGER
    }

-----------
drvAdpID                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Unique adapter ID"
    ::= { driveOperationSupportEntry 1 }

forceOnline                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Physical Drive force Online operation support
	                             Values: notSupported(0), supported(1)"
    ::= { driveOperationSupportEntry 2 }

forceOffline                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Physical Drive force Offline operation support
	                             Values: notSupported(0), supported(1)"
    ::= { driveOperationSupportEntry 3 }

forceRebuild              OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Physical Drive force Rebuild operation support
	                             Values: notSupported(0), supported(1)"
    ::= { driveOperationSupportEntry 4 }

-- vd operation support info

vdOperationSupportTable               OBJECT-TYPE
    SYNTAX                      SEQUENCE OF VdOperationSupportEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List operations supported by Virtual Drive"
    ::= { adapterDetails 7 }

    vdOperationSupportEntry          OBJECT-TYPE
    SYNTAX                      VdOperationSupportEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the vdOperationSupport Table."
    INDEX                       { adapterID }
    ::= { vdOperationSupportTable 1 }

    VdOperationSupportEntry ::=
        SEQUENCE {
        vdOpAdpID               INTEGER,
        readPolicy               INTEGER,
        writePolicy             INTEGER,
        ioPolicy      INTEGER,
        accessPolicy              INTEGER,
        diskCachePolicy       INTEGER

    }

vdOpAdpID                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Unique adapter ID"
    ::= { vdOperationSupportEntry 1 }
    
readPolicy                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Read policy support. Values: False(0), True(1)"
    ::= { vdOperationSupportEntry 2 }

writePolicy                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Write policy support. Values: False(0), True(1)"
    ::= { vdOperationSupportEntry 3 }

ioPolicy              OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "IO policy support. Values: False(0), True(1)"
    ::= { vdOperationSupportEntry 4 }
accessPolicy              OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Access policy support. Values: False(0), True(1)"
    ::= { vdOperationSupportEntry 5 }

diskCachePolicy                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "Disk Cache Policy support. Values: False(0), True(1)"
    ::= { vdOperationSupportEntry 6 }

--------------------------------------------------------------------------------
-- BBU Information.
--------------------------------------------------------------------------------
bbuInfo                      OBJECT IDENTIFIER ::= {adapter 2}

bbuNumber                       OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the bbuTable."
    ::= { bbuInfo 1 }
bbuTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF BBUEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of bbu Entries containing Information/Properties about the BBU."
    ::= { bbuInfo 2 }


    bbuEntry                OBJECT-TYPE
    SYNTAX                      BBUEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the BBU table."
    INDEX                       { bbuID }
    ::= { bbuTable 1 }

    BBUEntry ::=
        SEQUENCE {
            bbuID           INTEGER,
            batteryType    INTEGER,
            nextLearnTime         INTEGER,
            absStateOfCharge     INTEGER,
            fullChargeCapacity         INTEGER,
            averageEmptyTime         INTEGER,
            cycleCount         INTEGER,
            firmwareStatus         DisplayString,
            voltage         INTEGER,
            autoLearnPeriod         INTEGER,
            relStateOfCharge         INTEGER,
            capacityRemain         INTEGER,
            runTimeToEmpty         INTEGER,
            avgTimeToFull         INTEGER,
            errorMargin         INTEGER,
            temperature         INTEGER,
            mfgName             DisplayString,
            deviceName             DisplayString,
            serialNumber             DisplayString,
            chargerStatus        INTEGER,
            adpID        INTEGER,
            remainingCapAlarm        INTEGER,
            remainingTimeAlarm        INTEGER,
            bbu-current        INTEGER,
            gasGaugeStatus     INTEGER
    }


-- defines for each attribute in BBUEntry

bbuID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "BBUID for this BBU.(Unique)"
    ::= { bbuEntry 1 }

batteryType                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "BBU Type: Values: n/a(0), ibbu(1), bbu(2)"
    ::= { bbuEntry 2 }
nextLearnTime                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Time of next scheduled lean cycle (seconds path 1/1/2000)"
    ::= { bbuEntry 3 }
absStateOfCharge                OBJECT-TYPE
    SYNTAX                      INTEGER(0..100)
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Predicted remaining capacity expressed as % of DesignCapacity() (0-100)"
    ::= { bbuEntry 4 }
fullChargeCapacity                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Predicted pack capacity when it is fully charged in mAh"
    ::= { bbuEntry 5 }
averageEmptyTime                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "One-minute rolling average of the predicted remaining battery life"
    ::= { bbuEntry 6 }
cycleCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of charge cycles the battery has experienced"
    ::= { bbuEntry 7 }
firmwareStatus                OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "condition of battary in following order:
                                 packMissing(0/1)           
                                 voltageLow(0/1)            
                                 temperatureHigh(0/1)       
                                 chargeActive(0/1)          
                                 dischargeActive(0/1)       
                                 learnCycleRequested(0/1)   
                                 learnCycleActive(0/1)      
                                 learnCycleFailed(0/1)      
                                 learnCycleTimeout(0/1)     
                                 i2cErrorsDetected(0/1)
                                 Only enabled(1) values will be shown"     
    
    ::= { bbuEntry 8 }
voltage                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Accurate battery terminal voltage in mV, resolution of 1mV"
    ::= { bbuEntry 9 }
autoLearnPeriod                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Time (in seconds) between learn cycles (0 to disable auto learn)"
    ::= { bbuEntry 10 }
relStateOfCharge                OBJECT-TYPE
    SYNTAX                      INTEGER(0..100)
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Predicted remaining capacity expressed as % of FullChargeCapacity() (0-100)"
    ::= { bbuEntry 11 }
capacityRemain                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Predicted charge or energy remaining in the battery in mAh"
    ::= { bbuEntry 12 }
runTimeToEmpty                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "(in minutes)Relative gain or loss in remaining life in response to change in power policy"
    ::= { bbuEntry 13 }
avgTimeToFull                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "One-minute rolling average of predicted remaining time to full charge"
    ::= { bbuEntry 14 }
errorMargin                OBJECT-TYPE
    SYNTAX                      INTEGER(2..100)
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Expected margin of error (%) in charge calculation (2-100)"
    ::= { bbuEntry 15 }
temperature                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Battery temperature in degree Centigrade"
    ::= { bbuEntry 16 }
mfgName                OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Battery manufacturer's name"
    ::= { bbuEntry 17 }
deviceName                OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Battery name"
    ::= { bbuEntry 18 }
serialNumber                OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Battery serialNumber"
    ::= { bbuEntry 19 }
chargerStatus                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Battery charger status. Values: N/A(-1), off(0), complete(1), progress(2)"
    ::= { bbuEntry 20 }
adpID                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The adapter id where BBU is attached"
    ::= { bbuEntry 21 }
remainingCapAlarm                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Remaining capacity to alarm"
    ::= { bbuEntry 22 }
remainingTimeAlarm                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Remaining time to alarm"
    ::= { bbuEntry 23 }
bbu-current                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Current(In mA) being supplied (or accepted) through the terminals of the battery"
    ::= { bbuEntry 24 }
gasGaugeStatus                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Gas guage status"
    ::= { bbuEntry 25 }
--------------------------------------
device                          OBJECT IDENTIFIER ::= {megaRAID-SAS-IR 2}

physicalDriveInfo                      OBJECT IDENTIFIER ::= {device 1}
--------------------------------------------------------------------------------
-- PD Information group.
--------------------------------------------------------------------------------

pdNumber                        OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the physicalDrive table."
    ::= { physicalDriveInfo 1 }

pdTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF PdEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of physicalDrive Entries containing Information/Properties about the drives"
    ::= { physicalDriveInfo 2 }

pdEntry                     OBJECT-TYPE
        SYNTAX                  PdEntry
        ACCESS                  not-accessible
        STATUS                  optional
        DESCRIPTION             "An Entry in the Device Table."
        INDEX                   { physDevID  }
    ::= { pdTable 1 }

    PdEntry ::=
        SEQUENCE {
		    pdIndex           INTEGER,
            physDevID           INTEGER,
            oemSupported       INTEGER,
            scsiDevType            INTEGER,
            connectedAdapterPort                 INTEGER,
            deviceSpeed                 INTEGER,
            mediaErrCount                 INTEGER,
            otherErrCount                 INTEGER,
            predFailCount                 INTEGER,
            pdState                 INTEGER,
            disabledForRemoval                 INTEGER,
            linkSpeed                 INTEGER,
            pdSupportFlags                 DisplayString,
            sasAddr                 DisplayString,
            rawSize                 INTEGER,
            nonCoercedSize                 INTEGER,
            coercedSize                 INTEGER,
            enclDeviceId                 INTEGER,
            enclIndex                 INTEGER,
            slotNumber                 INTEGER,
            pdOperationProgress            DisplayString,
            pdAdpID                      INTEGER,
            operationSupport                DisplayString,
            vendorID                DisplayString,
            productID                DisplayString,
            diskType             INTEGER
            
        }
-- defines for each attribute in PhysicaldriveEntry
pdIndex                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The unique ID"
    ::= { pdEntry 1 }

physDevID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The Device ID"
    ::= { pdEntry 2 }

oemSupported                   OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Drive support by the OEM (OEM-specific checks)
Values: notSupported(1), supported(0)"
    ::= { pdEntry 3 }

scsiDevType                        OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Type of this Device. Values:
disk(0), tape(1), printer(2), processor(3), cdrom(5), scanner(6),
optical(7), enclosure(13), dvd(10), unknown(31)	"
    ::= { pdEntry 4 }

connectedAdapterPort                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Adapter port to which the device is connected."
    ::= { pdEntry 5 }

deviceSpeed                     OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Maximum supported speed. Values:
speed_unknown(0), speed_1p5G(1), speed_3G(2)"
    ::= { pdEntry 6 }
mediaErrCount                   OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Error count of the device"
    ::= { pdEntry 7 }
otherErrCount                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "other error count of the device"
    ::= { pdEntry 8 }
predFailCount                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Predictive fail count of the device"
    ::= { pdEntry 9 }
pdState                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Firmware's interpretation of drive state. Values:
unconfigured_good(0), unconfigured_bad(1), hot_spare(2), offline(16), failed(17), rebuild(20), online(24)"
    ::= { pdEntry 10 }
disabledForRemoval                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "If true, drive is ready for removal. Values: false(0), true(1)"
    ::= { pdEntry 11 }
linkSpeed                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Negotiated link speed. Values: speed_unknown(0), speed_1p5G(1), speed_3G(2)"
    ::= { pdEntry 12 }
pdSupportFlags                   OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "1st Byte:forcedPDGUID(0/1),2nd Byte:inVD(0/1),3rd Byte:isGlobalSpare(0/1),4th Byte:isSpare(0/1),5th Byte:isForeign(0/1),6th Byte:intf(0-Unknown, 1-parallel SCSI, 2-SAS, 3-SATA, 4-FC).A comma delimited list will appear."
    ::= { pdEntry 13 }
sasAddr                             OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Device SAS addresses. Comma separeted for multiple address"
    ::= { pdEntry 14 }
rawSize                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Size(MB) before COD and coercion"
    ::= { pdEntry 15 }
nonCoercedSize                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Size(MB) after COD is reserved but before coercion"
    ::= { pdEntry 16 }
coercedSize                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Size(MB) after COD is reserved and after coercion"
    ::= { pdEntry 17 }
enclDeviceId                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Enclosure's device Id (in decimal); if device is not within enclosure value is -1"
    ::= { pdEntry 18 }
enclIndex                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Firmware internal enclosure index"
    ::= { pdEntry 19 }
slotNumber                             OBJECT-TYPE
    SYNTAX                      INTEGER(0..255)
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Slot number of this drive, if this Physical Drive is an enclosure then -1"
    ::= { pdEntry 20 }
pdOperationProgress                             OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "% Progress is %. e.g. Rebuild progress is 10%"
    ::= { pdEntry 21 }
pdAdpID                             OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Controller id where this Physical Drive is attached"
    ::= { pdEntry 22 }
operationSupport                             OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Online,Offline,Failed,Bad,Uncofigured"--,Spare,Spare,replaceMissing,markMissing,startRebuild,stopRebuild"
    ::= { pdEntry 23 }
vendorID                             OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Vendor ID"
    ::= { pdEntry 24 }
productID                             OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Product ID"
    ::= { pdEntry 25 }

diskType                        OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Type of the disk : 0-Unknown, 1-parallel SCSI, 2-SAS, 3-SATA, 4-FC"
    ::= { pdEntry 26 }

--Virtual Devices
virtualDevice                      OBJECT IDENTIFIER ::= {megaRAID-SAS-IR 3}

vdInfo                     OBJECT IDENTIFIER ::= {virtualDevice 1}

vdNumber                        OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the virtualDrive table."
    ::= { vdInfo 1 }

vdTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF VdEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of Virtual Drive Entries containing Information/Properties about the virtualDrive."
    ::= { vdInfo 2 }

vdEntry                     OBJECT-TYPE
        SYNTAX                  VdEntry
        ACCESS                  not-accessible
        STATUS                  optional
        DESCRIPTION             "An Entry in the virtualDrive Table."
        INDEX                   { virtualDevID  }
    ::= { vdTable 1 }

    VdEntry ::=
        SEQUENCE {
            virtualDevID           INTEGER,
            size       INTEGER,
            clusterOwnerDeviceId       INTEGER,
            targetId       INTEGER,
            state       INTEGER,
            name       DisplayString,
            defaultCachePolicy       INTEGER,
            vdAccessPolicy       INTEGER,
            vdDiskCachePolicy       INTEGER,
            bgiState       INTEGER,
            prl       INTEGER,
            rLQ       INTEGER,
            sRL       INTEGER,
            stripeSize       INTEGER,
            numDrives       INTEGER,
            spanDepth       INTEGER,
            initState       INTEGER,
            currentCachePolicy     INTEGER,  
            operationProgress      DisplayString,
			vdAdpID         INTEGER
        }
-- defines for each attribute in PhysicaldriveEntry

virtualDevID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The unique Virtual Drive ID"
    ::= { vdEntry 1 }
size                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Total size in MB of the drive"
    ::= { vdEntry 2 }
clusterOwnerDeviceId                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Virtual Drive owner's device Id"
    ::= { vdEntry 3 }
targetId                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Virtual Drive target id (i.e. 0 to 63)"
    ::= { vdEntry 4 }
state                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Virtual Drive state. Values: offline(0), partially_degraded(1), degraded(2), optimal(3)"
    ::= { vdEntry 5 }
name                       OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Virtual Drive name"
    ::= { vdEntry 6 }
defaultCachePolicy         OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Default cache policy settings. Values: direct_io(0), cached_io(1)"
    ::= { vdEntry 7 }
vdAccessPolicy                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Access policy settings. Values: access_rw(0), access_read_only(2), access_blocked(3)"
    ::= { vdEntry 8 }
vdDiskCachePolicy                       OBJECT-TYPE
    SYNTAX                      INTEGER  (0..2)
    ACCESS                      read-write
    STATUS                      optional
    DESCRIPTION                 "Physical disk cache policy. Values: unchanged(0), enable(1), disable(2)"
    ::= { vdEntry 9 }
bgiState                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "BGI state on this VD. Values disable(1), enable(0) "
    ::= { vdEntry 10 }
prl                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Primay raid level"
    ::= { vdEntry 11 }
rLQ                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Raid level qaulifier"
    ::= { vdEntry 12 }
sRL                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Secondary raid level"
    ::= { vdEntry 13 }
stripeSize                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Stripe Size in KB"
    ::= { vdEntry 14 }
numDrives                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of drivers per span"
    ::= { vdEntry 15 }
spanDepth                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of spans. If only one array then it is considered as 1 span"
    ::= { vdEntry 16 }
initState                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "0=no init, 1=quick init, 2=full init"
    ::= { vdEntry 17 }
currentCachePolicy                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Default cache policy settings. Values: direct_io(0), cached_io(1)"
    ::= { vdEntry 18 }
operationProgress                       OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Progress % for operation x/ No operation in progress"
    ::= { vdEntry 19 }
vdAdpID                         OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Controller id where this vd is present"
    ::= { vdEntry 20 }

--VD Span
vdSpanInfo                     OBJECT IDENTIFIER ::= {virtualDevice 2}

vdSpanNumber                        OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the virtualDrive table."
    ::= { vdSpanInfo 1 }

vdSpanTable                   OBJECT-TYPE
    SYNTAX                      SEQUENCE OF VdSpanEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of span Entries containing Information/Properties vd span."
    ::= { vdSpanInfo 2 }

vdSpanEntry                     OBJECT-TYPE
        SYNTAX                  VdSpanEntry
        ACCESS                  not-accessible
        STATUS                  optional
        DESCRIPTION             "An Entry in the vdSpan Table."
        INDEX                   { spanID  }
    ::= { vdSpanTable 1 }

    VdSpanEntry ::=
        SEQUENCE {
            spanID              INTEGER,
            vDevID           INTEGER,
            startBlock           INTEGER,
            numBlocks           DisplayString,
            vdsArrayRef           INTEGER,
            spAdpId           INTEGER
        }
        
spanID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The unique Span ID"
    ::= { vdSpanEntry 1 }

vDevID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The Virtual Device ID"
    ::= { vdSpanEntry 2 }
startBlock                       OBJECT-TYPE
    SYNTAX                     INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Span physical disk starting block"
    ::= { vdSpanEntry 3 }
numBlocks                       OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Span physical disk block count"
    ::= { vdSpanEntry 4 }
vdsArrayRef                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Array reference (index)"
    ::= { vdSpanEntry 5 }
spAdpId                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Adapter where the span will be found"
    ::= { vdSpanEntry 6 }

---------------
arrayInfo                     OBJECT IDENTIFIER ::= {virtualDevice 3}

arrayNumber                        OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the array table."
    ::= { arrayInfo 1 }

arrayTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF ArrayEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of array Entries containing Information/Properties about the arrays."
    ::= { arrayInfo 2 }

arrayEntry                     OBJECT-TYPE
        SYNTAX                  ArrayEntry
        ACCESS                  not-accessible
        STATUS                  optional
        DESCRIPTION             "An Entry in the array Table."
        INDEX                   { arrayID  }
    ::= { arrayTable 1 }

    ArrayEntry ::=
        SEQUENCE {
            arrayID           INTEGER,
            arrSize           INTEGER,
            arrNumDrives           INTEGER,
            arrayRef           INTEGER,
            pdList         DisplayString,
	    arrAdpId           INTEGER
        }

arrayID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The unique array ID"
    ::= { arrayEntry 1 }
arrSize                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Size(MB) of smallest PD in array"
    ::= { arrayEntry 2 }
arrNumDrives                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of drives for this array"
    ::= { arrayEntry 3 }
arrayRef                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Tag for the array"
    ::= { arrayEntry 4 }
pdList                       OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Space separated pd identification. e.g. {devID devID devID} etc "
    ::= { arrayEntry 5 }
arrAdpId                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Adapter where the array will be found"
    ::= { arrayEntry 6 }

---------------
spareInfo                     OBJECT IDENTIFIER ::= {virtualDevice 4}

spareDevNumber                        OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the sparepool table."
    ::= { spareInfo 1 }

spareTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF SpareEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of sparepool Entries containing Information/Properties about the spare drive"
    ::= { spareInfo 2 }

spareEntry                     OBJECT-TYPE
        SYNTAX                  SpareEntry
        ACCESS                  not-accessible
        STATUS                  optional
        DESCRIPTION             "An Entry in the sparepool Table."
        INDEX                   { spareID  }
    ::= { spareTable 1 }

    SpareEntry ::=
        SEQUENCE {
            spareID           INTEGER,
            deviceIdentification           INTEGER,
            spareType           DisplayString,
            arrayCount           INTEGER,
            arrRef         DisplayString,
            sprAdpId           INTEGER
       }
-- defines for each attribute in PhysicaldriveEntry

spareID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The unique Index"
    ::= { spareEntry 1 }
deviceIdentification                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The Device ID"
    ::= { spareEntry 2 }
spareType                       OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Spare type. isDedicated(0/1)isRevertible(0/1)isEnclAffinity(0/1). 1 implies particular feature is enable and 0 represent feature is disable."
    ::= { spareEntry 3 }
arrayCount                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The number of arrays to which the PD can be dedicated"
    ::= { spareEntry 4 }
arrRef                       OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Comma separated array ids. e.g. 2,4,5 etc "
    ::= { spareEntry 5 }

sprAdpId                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Adapter where the spare will be found"
    ::= { spareEntry 6 }

--------------------------------------------------------------------------------
-- Enclosure Information.
--------------------------------------------------------------------------------
enclosure                      OBJECT IDENTIFIER ::= {megaRAID-SAS-IR 4}
enclosureInfo                      OBJECT IDENTIFIER ::= {enclosure 1}

enclosureNumber                       OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the enclosure table."
    ::= { enclosureInfo 1 }
enclosureTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF EnclosureEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of enclosure Entries containing Information/Properties about the enclosures in the system."
    ::= { enclosureInfo 2 }


    enclosureEntry                OBJECT-TYPE
    SYNTAX                      EnclosureEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the enclosure table."
    INDEX                       { enclosureID }
    ::= { enclosureTable 1 }

    EnclosureEntry ::=
        SEQUENCE {
            enclosureID           INTEGER,
            deviceId    INTEGER,
            enclosureIndex         INTEGER,
            slotCount     INTEGER,
            psCount         INTEGER,
            fanCount         INTEGER,
            tempSensorCount         INTEGER,
            alarmCount         INTEGER,
            simCount         INTEGER,
            isFault         INTEGER,
            pdCount         INTEGER,
            pdIds         DisplayString,
			encAdpID         INTEGER
    }

-- defines for each attribute in EncloserEntry

enclosureID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "EnclosureID for this enclosure.(Unique)"
    ::= { enclosureEntry 1 }

deviceId                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Enclosure device Id."
    ::= { enclosureEntry 2 }
enclosureIndex                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Firmware internal enclosure index"
    ::= { enclosureEntry 3 }
slotCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of slots"
    ::= { enclosureEntry 4 }
psCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of power supplies"
    ::= { enclosureEntry 5 }
fanCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of fans"
    ::= { enclosureEntry 6 }
tempSensorCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of temperature sensors"
    ::= { enclosureEntry 7 }
alarmCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of alarms"
    ::= { enclosureEntry 8 }
simCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of SIM modules"
    ::= { enclosureEntry 9 }
isFault                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Enclosure has entered a FAULT state or not. Values: false(0), true(1)"
    ::= { enclosureEntry 10 }
pdCount                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of physical drives present"
    ::= { enclosureEntry 11 }
pdIds                OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Physical drive deviceId's comma separated."
    ::= { enclosureEntry 12 }
encAdpID                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Adapter ID where this enclosure is connected"
    ::= { enclosureEntry 13 }

----------------------
enclosureFanInfo                      OBJECT IDENTIFIER ::= {enclosure 2}

enclosureFanNumber                       OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the enclosure fan table."
    ::= { enclosureFanInfo 1 }

enclosureFanTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF EnclosureFanEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of fan Entries containing Information/Properties about the enclosureFan."
    ::= { enclosureFanInfo 2 }


    enclosureFanEntry                OBJECT-TYPE
    SYNTAX                      EnclosureFanEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the enclosureFan table."
    INDEX                       { fanID }
    ::= { enclosureFanTable 1 }

    EnclosureFanEntry ::=
        SEQUENCE {
            fanID           INTEGER,
            enclosureId    INTEGER,
            fanStatus         INTEGER
    }

-- defines for each attribute in EncloserEntry

fanID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "ID for this enclosureFan.(Unique)"
    ::= { enclosureFanEntry 1 }

enclosureId                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Enclosure ID where the fan is attached"
    ::= { enclosureFanEntry 2 }
fanStatus                OBJECT-TYPE
    SYNTAX                      INTEGER{
                                status-ok(1),
                                status-critical(2),
                                status-nonCritical(3),
                                status-unrecoverable(4),
                                status-not-installed(5),
                                status-unknown(6),
                                status-not-available(7)
                                }
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "status of the device"
    ::= { enclosureFanEntry 3 }

----------------------
enclosureSlotInfo                      OBJECT IDENTIFIER ::= {enclosure 3}

enclosureSlotNum                       OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the enclosure slot table."
    ::= { enclosureSlotInfo 1 }

enclosureSlotTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF EnclosureSlotEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of slot Entries containing Information/Properties about the enclosure slots."
    ::= { enclosureSlotInfo 2 }


    enclosureSlotEntry                OBJECT-TYPE
    SYNTAX                      EnclosureSlotEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the enclosureSlot table."
    INDEX                       { slotID }
    ::= { enclosureSlotTable 1 }

    EnclosureSlotEntry ::=
        SEQUENCE {
            slotID           INTEGER,
            sltEncId    INTEGER,
            slotStatus         INTEGER
    }

-- defines for each attribute in EncloserEntry

slotID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "ID for this slot.(Unique)"
    ::= { enclosureSlotEntry 1 }

sltEncId                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Enclosure ID where the slot"
    ::= { enclosureSlotEntry 2 }
slotStatus                OBJECT-TYPE
    SYNTAX                      INTEGER{
                                status-ok(1),
                                status-critical(2),
                                status-nonCritical(3),
                                status-unrecoverable(4),
                                status-not-installed(5),
                                status-unknown(6),
                                status-not-available(7)
                                }
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "status of the device"
    ::= { enclosureSlotEntry 3 }
----------------------
enclosurePSInfo                      OBJECT IDENTIFIER ::= {enclosure 4}

enclosurePSNumber                       OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the enclosure fan table."
    ::= { enclosurePSInfo 1 }
enclosurePSTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF EnclosurePSEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of powerSupply Entries containing Information/Properties about the enclosure powerSupply"
    ::= { enclosurePSInfo 2 }

enclosurePSEntry                OBJECT-TYPE
SYNTAX                      EnclosurePSEntry
ACCESS                      not-accessible
STATUS                      mandatory
DESCRIPTION                 "An Entry in the powerSupply table."
INDEX                       { powerSupplyID }
::= { enclosurePSTable 1 }

EnclosurePSEntry ::=
    SEQUENCE {
        powerSupplyID           INTEGER,
        psEnclosureId    INTEGER,
        powerSupplyStatus         INTEGER
}

-- defines for each attribute in EncloserEntry

powerSupplyID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "ID for this powerSupply.(Unique)"
    ::= { enclosurePSEntry 1 }

psEnclosureId                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Enclosure id for the powerSupply"
    ::= { enclosurePSEntry 2 }
powerSupplyStatus                OBJECT-TYPE
    SYNTAX                      INTEGER{
                                status-ok(1),
                                status-critical(2),
                                status-nonCritical(3),
                                status-unrecoverable(4),
                                status-not-installed(5),
                                status-unknown(6),
                                status-not-available(7)
                                }
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "status of the power Supply"
    ::= { enclosurePSEntry 3 }
----------------------
enclosureTSInfo                      OBJECT IDENTIFIER ::= {enclosure 5}

enclosureTSNumber                       OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the enclosure fan table."
    ::= { enclosureTSInfo 1 }
enclosureTSTable              OBJECT-TYPE
    SYNTAX                      SEQUENCE OF EnclosureTSEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of TempSensor Entries containing Information/Properties about the enclosure TempSensor"
    ::= { enclosureTSInfo 2 }


    enclosureTSEntry     OBJECT-TYPE
    SYNTAX                      EnclosureTSEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the adapter table."
    INDEX                       { tempSensorID }
    ::= { enclosureTSTable 1 }

    EnclosureTSEntry ::=
        SEQUENCE {
            tempSensorID           INTEGER,
            encId    INTEGER,
            tempSensorStatus         INTEGER,
            tsTemperature         INTEGER
    }

-- defines for each attribute in EncloserEntry

tempSensorID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "ID for this TempSensor.(Unique)"
    ::= { enclosureTSEntry 1 }

encId                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "enclosure id for this TempSensor"
    ::= { enclosureTSEntry 2 }
tempSensorStatus                OBJECT-TYPE
    SYNTAX                      INTEGER{
                                status-ok(1),
                                status-critical(2),
                                status-nonCritical(3),
                                status-unrecoverable(4),
                                status-not-installed(5),
                                status-unknown(6),
                                status-not-available(7)
                                }
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "status of this tempSensor"
    ::= { enclosureTSEntry 3 }
tsTemperature                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Current temperature in degree Centigrade"
    ::= { enclosureTSEntry 4 }
    
----------------------
enclosureAlarmInfo                      OBJECT IDENTIFIER ::= {enclosure 6}

enclosureAlarmNumber                       OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the enclosure fan table."
    ::= { enclosureAlarmInfo 1 }
enclosureAlarmTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF EnclosureAlarmEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of Alarm Entries containing Information/Properties about enclosure Alarms"
    ::= { enclosureAlarmInfo 2 }


    enclosureAlarmEntry                OBJECT-TYPE
    SYNTAX                      EnclosureAlarmEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the enclosureAlarm table."
    INDEX                       { alarmID }
    ::= { enclosureAlarmTable 1 }

    EnclosureAlarmEntry ::=
        SEQUENCE {
            alarmID           INTEGER,
            almEnclosureId    INTEGER,
            alarmStatus         INTEGER
    }

-- defines for each attribute in EncloserAlarmEntry

alarmID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "ID for this Alarm.(Unique)"
    ::= { enclosureAlarmEntry 1 }

almEnclosureId                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Enclosure id where the Alarm is attached"
    ::= { enclosureAlarmEntry 2 }
alarmStatus                OBJECT-TYPE
    SYNTAX                      INTEGER{
                                status-ok(1),
                                status-critical(2),
                                status-nonCritical(3),
                                status-unrecoverable(4),
                                status-not-installed(5),
                                status-unknown(6),
                                status-not-available(7)
                                }
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Status of the alarm"
    ::= { enclosureAlarmEntry 3 }
----------------------
enclosureSIMInfo                      OBJECT IDENTIFIER ::= {enclosure 7}

enclosureSIMNumber                       OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the enclosure fan table."
    ::= { enclosureSIMInfo 1 }
enclosureSIMTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF EnclosureSIMEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of SIM Entries containing Information/Properties about enclosure SIMs"
    ::= { enclosureSIMInfo 2 }


    enclosureSIMEntry                OBJECT-TYPE
    SYNTAX                      EnclosureSIMEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the enclosureSIM table."
    INDEX                       { simID }
    ::= { enclosureSIMTable 1 }

    EnclosureSIMEntry ::=
        SEQUENCE {
            simID           INTEGER,
            simEnclosureId    INTEGER,
            simStatus         INTEGER
    }

-- defines for each attribute in EncloserEntry

simID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "ID for this SIM.(Unique)"
    ::= { enclosureSIMEntry 1 }

simEnclosureId                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Enclosure id where the SIM is attached"
    ::= { enclosureSIMEntry 2 }
simStatus                OBJECT-TYPE
    SYNTAX                      INTEGER{
                                status-ok(1),
                                status-critical(2),
                                status-nonCritical(3),
                                status-unrecoverable(4),
                                status-not-installed(5),
                                status-unknown(6),
                                status-not-available(7)
                                }
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Number of Logical Drives Configured on this Adapter."
    ::= { enclosureSIMEntry 3 }
    
--------------------------------------------------------------------------------
-- Topology Information.
--------------------------------------------------------------------------------
topology                      OBJECT IDENTIFIER ::= {megaRAID-SAS-IR 5}

phyInfo                      OBJECT IDENTIFIER ::= {topology 1}

phyNumber                   OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the Phy table."
    ::= { phyInfo 1 }

phyTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF PhyEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of phy Entries containing Information/Properties about the sas topology in the system."
    ::= { phyInfo 2 }


    phyEntry                OBJECT-TYPE
    SYNTAX                      PhyEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the Phy table."
    INDEX                       { phyIndex }
    ::= { phyTable 1 }

    PhyEntry ::=
        SEQUENCE {
            phyIndex           INTEGER,
            deviceIndex    INTEGER,
            deviceType    INTEGER,
            phyID    INTEGER,
            deviceOffset       INTEGER,
            phyPos   INTEGER
   }

-- defines for each attribute in PhyEntry
phyIndex                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Index for this phy.(Unique)"
    ::= { phyEntry 1 }

deviceIndex                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Index of the device in tDeviceTable where the phy is attached"
    ::= { phyEntry 2 }

deviceType                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Type of device attached to this phy NO_DEVICE = 0, IOC(1), EDGE_EXPANDER(2), FANOUT_EXPANDER(3),END_DEVICE(4)"
    ::= { phyEntry 3 }  
    
phyID                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The phy ID of the attached device"
    ::= { phyEntry 4 }

deviceOffset                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "The memory offset where the node of the device that is attached to this phy starts."
    ::= { phyEntry 5 }

phyPos                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Position of the Phy in device attached."
    ::= { phyEntry 6 }

-------------------------------------------------------------------------------
devicesInTopology                      OBJECT IDENTIFIER ::= {topology 2}

tDeviceNumber                   OBJECT-TYPE
    SYNTAX                      Gauge
    ACCESS                      read-only
    STATUS                      mandatory
    DESCRIPTION                 "The present number of rows in the topology Device table."
    ::= { devicesInTopology 1 }

tDeviceTable                    OBJECT-TYPE
    SYNTAX                      SEQUENCE OF TDeviceEntry
    ACCESS                      not-accessible
    STATUS                      optional
    DESCRIPTION                 "A List of device Entries containing Information/Properties about the sas topology in the system."
    ::= { devicesInTopology 2 }


    tDeviceEntry                OBJECT-TYPE
    SYNTAX                      TDeviceEntry
    ACCESS                      not-accessible
    STATUS                      mandatory
    DESCRIPTION                 "An Entry in the tDevice table."
    INDEX                       { tDeviceIndex }
    ::= { tDeviceTable 1 }

    TDeviceEntry ::=
        SEQUENCE {
            tDeviceIndex           INTEGER,
            contID      INTEGER,
            tDeviceId    INTEGER,
            tDeviceType    INTEGER,
            tParentIndex    INTEGER,
            tNumPhy       INTEGER,
            tSASAddr         DisplayString,
            tDevDescription         DisplayString
   }

-- defines for each attribute in TDeviceEntry

tDeviceIndex                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Index for this device.(Unique)"
    ::= { tDeviceEntry 1 }

contID                       OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Adapter ID where this device is attached"
    ::= { tDeviceEntry 2 }

tDeviceId                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Device ID."
    ::= { tDeviceEntry 3 }  
    
tDeviceType                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "NO_DEVICE = 0, IOC(1), EDGE_EXPANDER(2), FANOUT_EXPANDER(3),END_DEVICE(4)"
    ::= { tDeviceEntry 4 }

tParentIndex                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Index of the parent device in the table where this device is connected. -1 if it root device."
    ::= { tDeviceEntry 5 }

tNumPhy                OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Total no of Phy present in this device"
    ::= { tDeviceEntry 6 }
    
tSASAddr                             OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Device SAS addresses. Comma separeted for multiple address"
    ::= { tDeviceEntry 7 }

tDevDescription                             OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Detailed description of the Device."
    ::= { tDeviceEntry 8 }
    
------------------------------Traps------------------------------
lsi-SAS-Traps                      OBJECT IDENTIFIER ::= {megaRAID-SAS-IR 6}

-- Following are the Objects defined for Traps

atAdpNumber                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Adapter ID for which Trap is generated."
    ::= { lsi-SAS-Traps 1001 }

atAlarmState            OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Alarm disabled(0)/enabled(1)"
    ::= { lsi-SAS-Traps 1002 }

atRate            OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "BGI/Check Consistency/Rebuild/Patrol Read/Reconstruction Rate"
    ::= { lsi-SAS-Traps 1003 }

atFlashImageName            OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Flash Image Name"
    ::= { lsi-SAS-Traps 1004 }

	
	
	
	-- Following are the VD trap vars

vdNum                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Virtual Drive Target ID for which Trap is generated."
    ::= { lsi-SAS-Traps 1101 }
vdSeq                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Virtual Drive Sequence no for which Trap is generated."
    ::= { lsi-SAS-Traps 1102 }
vdProg                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "progress %"
    ::= { lsi-SAS-Traps 1103 }

vdCachePolicyChangeReason            OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Virtual Drive cache policy."
    ::= { lsi-SAS-Traps 1104 }
vdNewState            OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Virtual Drive state"
    ::= { lsi-SAS-Traps 1105 }
vdOldState            OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Virtual Drive state"
    ::= { lsi-SAS-Traps 1106 }



	

-- Following are the PD trap vars

pdID                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Device ID for which Trap is generated."
    ::= { lsi-SAS-Traps 1201 }
pdEncIndex                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Enclosure index(0 means not within an enclosure) for which Trap is generated."
    ::= { lsi-SAS-Traps 1202 }
pdSlotNo                 OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Slot no for the enclosure"
    ::= { lsi-SAS-Traps 1203 }
pdNewState            OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Physical Drive state"
    ::= { lsi-SAS-Traps 1204 }
pdOldState            OBJECT-TYPE
    SYNTAX                      INTEGER
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Physical Drive state"
    ::= { lsi-SAS-Traps 1205 }
pdCDBData  			  OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "CDB Data."
    ::= { lsi-SAS-Traps 1206 }
pdSenseData  			  OBJECT-TYPE
    SYNTAX                      DisplayString
    ACCESS                      read-only
    STATUS                      optional
    DESCRIPTION                 "Sence Data."
    ::= { lsi-SAS-Traps 1207 }
      

	  
	  
	  
-- Following are the trap definitions

irAdpAlarmStateEnabled TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
        DESCRIPTION "Alarm has been enabled by user for Adapter $1"
	--#TYPE "LSI SAS-IR Trap: Alarm Enabled"
	--#SUMMARY "Alarm has been enabled by user for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
    --#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL    
    ::= 7001

irAdpBGIRateChanged TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atRate,
        atAdpNumber
        }
    DESCRIPTION "Background initialization rate changed to $1 for Adapter $2" 
    --#TYPE "LSI SAS-IR Trap: Background Initialization Rate Changed"
	--#SUMMARY "Background Initialization Rate changed to %d for Adapter %d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL 
    ::= 7002
irAdpCacheDiscarded TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Controller $1 cache discarded due to memory/battery problems"
    --#TYPE "LSI SAS-IR Trap: Controller Cache Discarded"
	--#SUMMARY "Controller %d cache discarded due to memory/battery problems"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7003
irAdpCacheRebootCantRecover TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Unable to recover cache data due to configuration mismatch for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Unable to Recover Cache data"
	--#SUMMARY "Unable to recover Cache Data due to configuration mismatch for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL 
    ::= 7004
irAdpCacheRebootRecover TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Cache data recovered successfully for Adapter $1" 
    --#TYPE "LSI SAS-IR Trap:Cache Recovered"
	--#SUMMARY "Cache Data Recovered for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7005
irAdpCacheVersionMismatch TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Controller cache discarded due to firmware version incompatibility for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Controller Cache Discarded"
	--#SUMMARY "Controller Cache Discarded due to Firmware version incompatibility for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7006

irAdpCCRateChanged TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atRate,
        atAdpNumber
        }
    DESCRIPTION "Consistency Check rate changed to $1 for Adapter $2" 
    --#TYPE "LSI SAS-IR Trap: Consistency Check Rate changed"
	--#SUMMARY "Consistency Check Rate changed to %d for Adapter %d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL 
    ::= 7007
irAdpFlashBadImage TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Flash downloaded image corrupted for Adapter $1" 
    --#TYPE "LSI SAS-IR Trap: Flash Download Image corrupted"
	--#SUMMARY "Flash download image corrupted for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7008
irAdpFlashEraseError TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Flash erase error for Adapter $1" 
    --#TYPE "LSI SAS-IR Trap: Flash Erase Error"
	--#SUMMARY "Flash erase error for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7009
irAdpFlashEraseTimeout TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Flash timeout during erase for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Flash Timeout during Erase"
	--#SUMMARY "Flash Timeout during Erase for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7010
irAdpFlashGeneralError TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Flash error for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Flash Error"
	--#SUMMARY "General Flash Error occurred for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7011
irAdpFlashImage TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atFlashImageName,
        atAdpNumber
        }
    DESCRIPTION "Flashing image: $1 for Adapter $2"
    --#TYPE "LSI SAS-IR Trap: Flashing Image"
	--#SUMMARY "Flashing Image %s for Adapter %d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL 
    ::= 7012
irAdpFlashOK TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Flash of new firmware image(s)complete for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Flash of Firmware Image Complete"
	--#SUMMARY "Flash of Firmware Image complete for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7013
irAdpFlashProgramError TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Flash programming error for Adapter $1" 
    --#TYPE "LSI SAS-IR Trap: Flash programming Error"
	--#SUMMARY "Flash programming error for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL 
    ::= 7014
irAdpFlashProgramTimeout TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Flash timeout during programming for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Flash timeout"
	--#SUMMARY "Flash timeout during programming for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7015
    
irAdpLogCleared TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Event log cleared for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Event Log cleared"
	--#SUMMARY "Event log cleared for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7016
irAdpLogWrapped TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Event log wrapped for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Event log wrapped"
	--#SUMMARY "Event log wrapped for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7017
    
irAdpPatrolReadComplete TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Patrol Read complete for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Patrol Read complete"
	--#SUMMARY "Patrol Read complete for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7018
irAdpPatrolReadPaused TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Patrol Read paused for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Patrol Read paused"
	--#SUMMARY "Patrol Read paused for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7019
irAdpPatrolReadResumed TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Patrol Read resumed for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Patrol Read resumed"
	--#SUMMARY "Patrol Read resumed for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7020
irAdpPatrolReadStarted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Patrol Read started for Adapter $1" 
    --#TYPE "LSI SAS-IR Trap: Patrol Read Started"
	--#SUMMARY "Patrol Read started for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7021
irAdpShutdown TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Shutdown command received for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Shutdown command received"
	--#SUMMARY "Shutdown command received for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL 
    ::= 7022
irAdpHibernate TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Hibernate command received for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Hibernate command received"
	--#SUMMARY "Hibernate command received for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7023
irAdpCrash TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atAdpNumber
        }
    DESCRIPTION "Fatal error received for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Fatal Error received"
	--#SUMMARY "Fatal error received for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7024

irAdpRRChanged TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atRate,
        atAdpNumber
        }
    DESCRIPTION "Rebuild rate changed to $1 for Adapter $2"
    --#TYPE "LSI SAS-IR Trap: Rebuild Rate changed"
	--#SUMMARY "Rebuild Rate changed to %d for Adapter %d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL"
    ::= 7025
irAdpPRRateChanged TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atRate,
        atAdpNumber
        }
    DESCRIPTION "Patrol Read rate changed to $1 for Adapter $2"
    --#TYPE "LSI SAS-IR Trap: Patrol Read Rate changed"
	--#SUMMARY "Patrol Read Rate changed to %d for Adapter %d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7026
irAdpAlarmStateDisabled TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Alarm has been disabled by user for Adapter $1" 
    --#TYPE "LSI SAS-IR Trap: Alarm disabled"
	--#SUMMARY "Alarm disabled by user for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7027
irAdpConfigCleared TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Configuration cleared for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Configuration cleared"
	--#SUMMARY "Configuration cleared for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7028
irAdpReconRateChanged TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {
        atRate,
        atAdpNumber
        }
    DESCRIPTION "Reconstruction rate changed to $1 for Adapter $2"
    --#TYPE "LSI SAS-IR Trap: Reconstruction Rate changed"
	--#SUMMARY "Reconstruction Rate changed to %d for Adapter %d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL 
    ::= 7029
irAdpDefault TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Factory defaults restored for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Factory defaults restored"
	--#SUMMARY "Factory defaults restored for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7030   
   

   

---------------vd trap----------

irVdtBGIAborted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES { atAdpNumber,vdNum}
    DESCRIPTION "BGI aborted on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: BGI aborted"
	--#SUMMARY "BGI aborted on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7101
irVdtBGICompleted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES { atAdpNumber,vdNum}
    DESCRIPTION "BGI completed on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: BGI completed"
	--#SUMMARY "BGI completed on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7102
irVdtBGIDoneWR TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES { atAdpNumber,vdNum}
    DESCRIPTION "BGI completed with uncorrectable errors on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: BGI completed with uncorrectble errors"
	--#SUMMARY "BGI completed with uncorrectable errors on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7103
irVdtBGIFailed TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES { atAdpNumber,vdNum}
    DESCRIPTION "BGI failed on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: BGI failed"
	--#SUMMARY "BGI failedon Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7104
irVdtBGIStarted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES { atAdpNumber,vdNum}
    DESCRIPTION "BGI started on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: BGI started"
	--#SUMMARY "BGI started on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7105

irVdtCCStarted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "CC started on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: CC started"
	--#SUMMARY "CC started on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7107
irVdtCCCompleted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "CC completed on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: CC completed"
	--#SUMMARY "CC completed on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7108
irVdtCCFailed TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "CC failed on Adapter -$1 VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: CC failed"
	--#SUMMARY "CC failed on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7109
irVdtCCAborted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "CC aborted on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: CC aborted"
	--#SUMMARY "CC aborted on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7110
irVdtCCCompCor TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "CC completed with correction on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: CC completed with correction"
	--#SUMMARY "CC completed with correction on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7111
irVdtInitAborted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "Initialization aborted on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: Initialization aborted"
	--#SUMMARY "Initialization aborted on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7112
irVdtInitFailed TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "Initialization failed on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: Initialization failed"
	--#SUMMARY "Initialization failed on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7113
irVdtInitCompleted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "Initialization completed on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: Initialization completed"
	--#SUMMARY "Initialization completed on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7114
irVdtInitFastStarted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "Fast Initialization started on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: Fast Initialization started"
	--#SUMMARY "Fast Initialization started on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7115
irVdtInitFullStarted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "Full Initialization started on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: Full Initialization started"
	--#SUMMARY "Full Initialization started on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7116
irVdtReconStarted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "Reconstructoin started on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: Reconstruction started"
	--#SUMMARY "Reconstruction started on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7117
irVdtReconCompleted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "Reconstruction completed on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: Reconstruction completed"
	--#SUMMARY "Reconstruction completed on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7118
irVdtReconResumed TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "Reconstruction resumed on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: Reconstruction resumed"
	--#SUMMARY "Reconstruction resumed on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7119
irVdtReconStopped TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "Reconstruction stopped on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: Reconstruction stopped"
	--#SUMMARY "Reconstruction stopped on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7120
irVdtStateChange TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum, vdOldState, vdNewState}
    DESCRIPTION "VD state changed on Adapter -$1  VD Target -$2  from $3 to $4"
    --#TYPE "LSI SAS-IR Trap: VD state changed"
	--#SUMMARY "VD state changed on Adapter -%d  VD Target -%d from %d to %d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7121
irVdtCreated TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "A new VD created on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: New VD created"
	--#SUMMARY "A new VD created on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7122
irVdtDeleted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,vdNum}
    DESCRIPTION "A VD deleted on Adapter -$1  VD Target -$2"
    --#TYPE "LSI SAS-IR Trap: VD deleted"
	--#SUMMARY "A VD deleted on Adapter -%d  VD Target -%d"
	--#ARGUMENTS {0,1}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7123


---------------pd trap----------
irPdtClearAborted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES { atAdpNumber,pdID,pdEncIndex,pdSlotNo }
    DESCRIPTION "PD Clear aborted on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Physical Drive Clear aborted"
	--#SUMMARY "Physical Drive Clear aborted on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7201
irPdtClearFailed TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES { atAdpNumber,pdID,pdEncIndex,pdSlotNo }
    DESCRIPTION "PD Clear failed on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Physical Drive Clear failed"
	--#SUMMARY "Physical Drive Clear failed on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7202
irPdtClearStarted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES { atAdpNumber,pdID,pdEncIndex,pdSlotNo }
    DESCRIPTION "PD Clear started on Adapter -$1 Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Physical Drive Clear started"
	--#SUMMARY "Physical Drive Clear started on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7203
irPdtClearCompleted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES { atAdpNumber,pdID,pdEncIndex,pdSlotNo }
    DESCRIPTION "PD Clear completed on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Physical Drive Clear completed"
	--#SUMMARY "Physical Drive Clear completed on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7204
irPdtError TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "Error occurred on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Error occurred"
	--#SUMMARY "Error occurred on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7205
irPdtFormatStart TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "PD format started on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Physical Drive Format started"
	--#SUMMARY "Physical Drive Format started on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7206
irPdtFormatCompleted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "PD format completed on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Physical Drive Format completed"
	--#SUMMARY "Physical Drive Format completed on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7207
irPdtInserted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "PD inserted on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Physical Drive Inserted"
	--#SUMMARY "Physical Drive inserted on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7208
irPdtRblAborted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "Rebuild aborted on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Rebuild aborted"
	--#SUMMARY "Rebuild aborted on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7209
irPdtRblCompleted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "Rebuild completed on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Rebuild completed"
	--#SUMMARY "Rebuild completed on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7210
irPdtRblFailedBS TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "Rebuild failed(bad source) on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Rebuild failed(bad source)"
	--#SUMMARY "Rebuild failed(bad source) on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7211
irPdtRblFailedBT TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "Rebuild failed(bad target) on Adapter -$1  Dev -$2  Enc -$3 Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Rebuild failed(bad target)"
	--#SUMMARY "Rebuild failed(bad target) on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7212
irPdtRblStart TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "Rebuild started on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Rebuild started"
	--#SUMMARY "Rebuild started on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7213
irPdtRblResumed TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "Rebuild resumed on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Rebuild resumed"
	--#SUMMARY "Rebuild resumed on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7214
irPdtRblStartA TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "Rebuild started(auto) on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Rebuild started(auto)"
	--#SUMMARY "Rebuild started(auto) on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7215
irPdtRemoved TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo}
    DESCRIPTION "PD removed on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Physical Drive removed"
	--#SUMMARY "Physical Drive removed on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7216
irPdtStateChange TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        {atAdpNumber,pdID,pdEncIndex,pdSlotNo, pdOldState, pdNewState}
    DESCRIPTION "PD state changed on Adapter -$1  Dev -$2  Enc -$3  Slot -$4  from $5 to $6"
    --#TYPE "LSI SAS-IR Trap: PD state changed"
	--#SUMMARY "PD state changed on Adapter -%d  Dev -%d  Enc -%d  Slot -%d  from %d to %d"
	--#ARGUMENTS {0,1,2,3,4,5}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7217
irPdtSENSEAlert TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES
        { atAdpNumber, pdID, pdEncIndex,pdSlotNo, pdCDBData,pdSenseData }
    DESCRIPTION "An unexpected Sense was detected on Adapter -$1  Dev -$2  Enc -$3  Slot -$4  CDBData -$5  SenseData -$6"
    --#TYPE "LSI SAS-IR Trap: PD SENSE Alert"
	--#SUMMARY "Unexpected Sense detected on Adapter -%d  Dev -%d  Enc -%d  Slot -%d  CDBData -%s  SenseData -%s"
	--#ARGUMENTS {0,1,2,3,4,5}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7218
irPdtPredictiveThresholdExceed TRAP-TYPE
	ENTERPRISE lsi-SAS-Traps
	VARIABLES
		{ atAdpNumber, pdID, pdEncIndex,pdSlotNo}
	DESCRIPTION "Predictive Threshold Exceeded on Adapter -$1  Dev -$2  Enc -$3  Slot -$4"
    --#TYPE "LSI SAS-IR Trap: Predictive Threshold Exceeded"
	--#SUMMARY "Predictive Threshold Exceeded on Adapter -%d  Dev -%d  Enc -%d  Slot -%d"
	--#ARGUMENTS {0,1,2,3}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7219		
---------------bbu trap----------
irBbuPresent TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery Present for Adapter %d"
	--#TYPE "LSI SAS-IR Trap: Battery present"
	--#SUMMARY "Battery Present for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7301   
irBbuNotPresent TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery Not Present for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery Not present"
	--#SUMMARY "Battery Not Present for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7302   
irBbuNewBattery TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "New Battery for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: New Battery "
	--#SUMMARY "New Battery for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7303   
irBbuReplaced TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }  
    DESCRIPTION "Battery replaced for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery replaced"
	--#SUMMARY "Battery has been replaced for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7304   
irBbuTempHigh TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }  
    DESCRIPTION "Battery temperature high for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery temperature high"
	--#SUMMARY "Battery Temperature is high for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7305   
irBbuVoltageLow TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    } 
    DESCRIPTION "Battery voltage low for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery voltage low"
	--#SUMMARY "Battery Voltage low for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7306   
irBbuCharging TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery started charging for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery started changing"
	--#SUMMARY "Battery started changing for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7307   
irBbuDisCharging TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery is discharging for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery discharging"
	--#SUMMARY "Battery is discharging for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7308   
irBbuTempNormal TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery temperature is normal for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery temperature normal"
	--#SUMMARY "Battery Temperature is normal for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7309   
irBbuReplace TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery needs replacement, SOH Bad for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery needs replacement"
	--#SUMMARY "Battery needs replacement for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7310   
irBbuRelearnStarted TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery relearn started for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery relearn started"
	--#SUMMARY "Battery Relearn started for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7311   
irBbuRelearnProgress TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery relearn in progress for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery relearn in progress"
	--#SUMMARY "Battery Relearn in progress for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7312   
irBbuRelearnComplete TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery relearn completed for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery relearn completed"
	--#SUMMARY "Battery Relearn completed for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7313   
irBbuRelearnTimeout TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery relearn timed out for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery relearn timed out"
	--#SUMMARY "Battery Relearn timed out for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7314   
irBbuRelearnPending TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery relearn pending: Battery is under charge for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery relearn pending"
	--#SUMMARY "Battery Relearn pending: Battery is under charge for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7315   
irBbuRelearnPostponed TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery relearn postponed for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery relearn postponed"
	--#SUMMARY "Battery Relearn postponed for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7316   
irBbuRemoved TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Battery removed for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Battery removed"
	--#SUMMARY "Battery removed for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7317   
irBbuCapacityLow TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Current capacity of the battery is below threshold for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Current capacity below threshold"
	--#SUMMARY "Current Capacity of the battery is below threshold for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
    ::= 7318   
irBbuCapacityAbove TRAP-TYPE
    ENTERPRISE lsi-SAS-Traps
    VARIABLES 
    { 
    atAdpNumber
    }
    DESCRIPTION "Current capacity of the battery is above threshold for Adapter $1"
    --#TYPE "LSI SAS-IR Trap: Current capacity above threshold"
	--#SUMMARY "Current Capacity of the battery is above threshold for Adapter %d"
	--#ARGUMENTS {0}
	--#SEVERITY INFORMATIONAL
	--#GENERIC 6
	--#CATEGORY "Error Events"
	--#STATE OPERATIONAL
	::= 7319

copyrightInfo                     OBJECT IDENTIFIER ::= {lsiRAIDServer 8}

copyright                     OBJECT-TYPE
   SYNTAX                     DisplayString (SIZE(0..63))
   ACCESS                     read-only
   STATUS                     mandatory
   DESCRIPTION                "LSI LOGIC "
    ::= { copyrightInfo 1 }
END
