--
-- LGC-SS-MSC-MIB_070824.my
-- MIB generated by MG-SOFT Visual MIB Builder Version 7.0  Build 209
-- Friday, August 24, 2007 at 09:51:33
--

	LGC-SS-MSC-MIB DEFINITIONS ::= BEGIN
 
		IMPORTS
			lgcSS, DisplayString16, TimeStamp, RowStatus, DisplayString8, 
			DisplayString32, DisplayString, AdminStateChoices			
				FROM LGC-MIB			
			IpAddress, Integer32, Counter32, OBJECT-TYPE, MODULE-IDENTITY			
				FROM SNMPv2-SMI;
	
	
		-- 1.3.6.1.4.1.1373.2.3.3.2
		msc MODULE-IDENTITY 
			LAST-UPDATED "200706291606Z"		-- June 29, 2007 at 16:06 GMT
			ORGANIZATION 
				"LGC Wireless"
			CONTACT-INFO 
				"lcrd
				lcrdsupport@lgcwireless.com"
			DESCRIPTION 
				"Description."
			REVISION "200706051219Z"		-- June 05, 2007 at 12:19 GMT
			DESCRIPTION 
				"This is the first release version of the MSC MIB"
			::= { application 2 }

		
	
--
-- Type definitions
--
	
		AvailStateChoices ::= INTEGER
			{
			inTest(0),
			failed(1),
			powerOff(2),
			offLine(3),
			onLine(4),
			dependency(5),
			degraded(6),
			notInstalled(7)
			}

--   shutdown
-- enabled
-- deleted
		OperStateChoices ::= INTEGER
			{
			online(1),
			offline(2)
			}

	
	
--
-- Node definitions
--
	
-- Node definitions
-- 
--  The MIB module for WXC2.
-- 1.3.6.1.4.1.1373.1.3
		-- 1.3.6.1.4.1.1373.2.3
		wxc2 OBJECT IDENTIFIER ::= { lgcSS 3 }

		
--  1.3.6.1.4.1.1373.1.3.3
		-- 1.3.6.1.4.1.1373.2.3.3
		application OBJECT IDENTIFIER ::= { wxc2 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.1
		heartbeat OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { msc 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2
		parameter OBJECT IDENTIFIER ::= { msc 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1
		routingZoneSet OBJECT IDENTIFIER ::= { parameter 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1
		rzsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF RzsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { routingZoneSet 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1
		rzsEntry OBJECT-TYPE
			SYNTAX RzsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { rzsIndex }
			::= { rzsTable 1 }

		
		RzsEntry ::=
			SEQUENCE { 
				rzsIndex
					INTEGER,
				rzsTitle
					DisplayString16,
				rzsCreateTimeStamp
					TimeStamp,
				rzsDialingPrefixSetID
					INTEGER,
				rzsAnnouncementSetID
					INTEGER,
				rzsMSRNRangeStart
					DisplayString16,
				rzsMSRNRangeEnd
					DisplayString16,
				cdrOption
					OCTET STRING,
				rzsNITZ
					Counter32,
				rzsMaxCallDurationOfMO
					INTEGER,
				rzsMaxCallDurationOfMT
					INTEGER,
				rzsCallDisconnectionMidCallWarning
					INTEGER,
				rzsSRFNumber0
					Integer32,
				rzsSRFNumber1
					Integer32,
				rzsCreateEntryRoutingSelection
					INTEGER,
				rzsRoutingSelectionEntries
					INTEGER,
				rzsRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.1
		rzsIndex OBJECT-TYPE
			SYNTAX INTEGER (1..32)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { rzsEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.2
		rzsTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ASCII Title of the Routing Zone (max 16 characters)"
			DEFVAL { "RZS#" }
			::= { rzsEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.3
		rzsCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Routing Zone Set"
			::= { rzsEntry 3 }

		
--  Dialing Prefix Set ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.4
		rzsDialingPrefixSetID OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Select the Dialing Prefix Set for this Routing Zone"
			DEFVAL { 0 }
			::= { rzsEntry 4 }

		
--  Announcement(CUA) Set ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.5
		rzsAnnouncementSetID OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Select the Call Unattainable Announcement Set for this Routing Zone"
			::= { rzsEntry 5 }

		
--  MSRN Range Start
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.6
		rzsMSRNRangeStart OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:The start of the MSRN range for this Routing Zone"
			::= { rzsEntry 6 }

		
--  MSRN Range End
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.7
		rzsMSRNRangeEnd OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:The end of the MSRN range for this Routing Zone"
			::= { rzsEntry 7 }

		
--  1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.8
		cdrOption OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (11))
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { rzsEntry 8 }

		
--  NITZ
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.9
		rzsNITZ OBJECT-TYPE
			SYNTAX Counter32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Network Identity and Time Zone"
			::= { rzsEntry 9 }

		
--  Max Call Duration Of MO
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.10
		rzsMaxCallDurationOfMO OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Define the permitted maximum call duration for MO call. Any ongoing call reaching this threshold will be compulsively cut off. 
				Set 0 to disable this function.
				"
			DEFVAL { 0 }
			::= { rzsEntry 10 }

		
--  Max Call Duration Of MT
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.11
		rzsMaxCallDurationOfMT OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Define the permitted maximum call duration for MT call. Any incoming call reaching this threshold will be compulsively cut off. 
				Set 0 to disable this function."
			DEFVAL { 0 }
			::= { rzsEntry 11 }

		
--  Call Disconnection Mid-call Warning
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.12
		rzsCallDisconnectionMidCallWarning OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Specify the time based trigger to play indicating tone for an ongoing prepaid call before the account balance is used up. Unit is second.
				Set 0 to disable this function.
				"
			DEFVAL { 0 }
			::= { rzsEntry 12 }

		
--  SRF Number0
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.13
		rzsSRFNumber0 OBJECT-TYPE
			SYNTAX Integer32 (0..65535)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The E.164 node address of the SRF connecting to MSS platform 0."
			::= { rzsEntry 13 }

		
--  SRF Number1
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.14
		rzsSRFNumber1 OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The E.164 node address of the SRF connecting to MSS platform 1."
			::= { rzsEntry 14 }

		
--  Route Selection
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.15
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.15
		rzsCreateEntryRoutingSelection OBJECT-TYPE
			SYNTAX INTEGER (0..32)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { rzsEntry 15 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.16
		rzsRoutingSelectionEntries OBJECT-TYPE
			SYNTAX INTEGER (0..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { rzsEntry 16 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.16
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.17
		rzsRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { rzsEntry 17 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2
		rsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF RsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { routingZoneSet 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.1.4.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1
		rsEntry OBJECT-TYPE
			SYNTAX RsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { rsRzsIndex, rsIndex }
			::= { rsTable 1 }

		
		RsEntry ::=
			SEQUENCE { 
				rsRzsIndex
					INTEGER,
				rsIndex
					INTEGER,
				rsTitle
					DisplayString16,
				rsCreateTimeStamp
					TimeStamp,
				rsTrunkGroup
					INTEGER,
				rsAlternativeTrunkGroupOption
					INTEGER,
				rsAlternativeTrunkGroup
					INTEGER,
				rsNAIForOutgoingCall
					INTEGER,
				rsNumberOfDigitDeletion
					INTEGER,
				rsInsertionNumber
					DisplayString16,
				rsRowStatus
					RowStatus
			 }

--  Route Selection RZS Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1.1
		rsRzsIndex OBJECT-TYPE
			SYNTAX INTEGER (1..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { rsEntry 1 }

		
--  Route Selection Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1.2
		rsIndex OBJECT-TYPE
			SYNTAX INTEGER (1..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Select the routing plan according to the RSC getting from the dialing prefix"
			::= { rsEntry 2 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1.3
		rsTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ASCII Title of the Routing Selection (max 16 characters)"
			DEFVAL { "RS#" }
			::= { rsEntry 3 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1.4
		rsCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Routing Selection"
			::= { rsEntry 4 }

		
--  Trunk Group
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1.5
		rsTrunkGroup OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			DEFVAL { 0 }
			::= { rsEntry 5 }

		
--  Alternative Trunk Group Option
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1.6
		rsAlternativeTrunkGroupOption OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			DEFVAL { disable }
			::= { rsEntry 6 }

		
--  Alternative Trunk Group
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1.7
		rsAlternativeTrunkGroup OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			DEFVAL { 0 }
			::= { rsEntry 7 }

		
--  NAI For Outgoing Call
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1.8
		rsNAIForOutgoingCall OBJECT-TYPE
			SYNTAX INTEGER
				{
				sub(1),
				unknown(2),
				ndd(3),
				idd(4)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Specify the Nature of Address Indicator (NAI) of an outgoing call for the terminating node to route this call with proper dialed number digit manipulation"
			::= { rsEntry 8 }

		
--  Number Of Digit Deletion
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1.9
		rsNumberOfDigitDeletion OBJECT-TYPE
			SYNTAX INTEGER (0..16)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:number of deleted prefix digit (0-16)"
			DEFVAL { 0 }
			::= { rsEntry 9 }

		
--  Insertion Number
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1.10
		rsInsertionNumber OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:inserted digits (0-9999999999999999)"
			DEFVAL { "FFFFFFFFFFFFFFFF" }
			::= { rsEntry 10 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2.1.11
		rsRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { rsEntry 11 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2
		dialingPrefixSet OBJECT IDENTIFIER ::= { parameter 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.2.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1
		dpsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF DpsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { dialingPrefixSet 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.2.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1
		dpsEntry OBJECT-TYPE
			SYNTAX DpsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { dpsIndex }
			::= { dpsTable 1 }

		
		DpsEntry ::=
			SEQUENCE { 
				dpsIndex
					INTEGER,
				dpsTitle
					DisplayString16,
				dpsCreateTimeStamp
					TimeStamp,
				dpsCC
					INTEGER,
				dpsNDC
					Counter32,
				dpsInternationalPrefix
					DisplayString8,
				dpsNationalPrefix
					DisplayString8,
				dpsHPLMNCC0
					DisplayString16,
				dpsHPLMNCC1
					DisplayString16,
				dpsHPLMNCC2
					DisplayString16,
				dpsHPLMNCC3
					DisplayString16,
				dpsHPLMNCC4
					DisplayString16,
				dpsHPLMNCC5
					DisplayString16,
				dpsHPLMNCC6
					DisplayString16,
				dpsHPLMNCC7
					DisplayString16,
				dpsCreateEntrydDalingPrefix
					INTEGER,
				dpsDalingPrefixEntries
					INTEGER,
				dpsRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.1
		dpsIndex OBJECT-TYPE
			SYNTAX INTEGER (1..16)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { dpsEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.2
		dpsTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ASCII Title of the Dialing Prefix Set (max 16 characters)"
			DEFVAL { "DPS#" }
			::= { dpsEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.3
		dpsCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Dialing Prefix Set"
			::= { dpsEntry 3 }

		
--  Country Code
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.4
		dpsCC OBJECT-TYPE
			SYNTAX INTEGER (0..65535)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Country Code (Read only)"
			::= { dpsEntry 4 }

		
--  National Destination Code
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.5
		dpsNDC OBJECT-TYPE
			SYNTAX Counter32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:National Destination Code"
			::= { dpsEntry 5 }

		
--  International Prefix
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.6
		dpsInternationalPrefix OBJECT-TYPE
			SYNTAX DisplayString8
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:A digit or combination of digits used by a subscriber when making an international call. 
				The international prefix is used to indicate that the following digits represent an international number and should be routed to an international gateway.
				"
			DEFVAL { "00" }
			::= { dpsEntry 6 }

		
--  National Prefix
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.7
		dpsNationalPrefix OBJECT-TYPE
			SYNTAX DisplayString8
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:A digit or combination of digits used by a subscriber when calling a national destination (within the country) other than that of the local area network.
				"
			DEFVAL { "0" }
			::= { dpsEntry 7 }

		
--  HPLMN CC0
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.8
		dpsHPLMNCC0 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:HPLMN Country Code Table: define multiple CC as one country"
			::= { dpsEntry 8 }

		
--  HPLMN CC1
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.9
		dpsHPLMNCC1 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:HPLMN Country Code Table: define multiple CC as one country"
			::= { dpsEntry 9 }

		
--  HPLMN CC2
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.10
		dpsHPLMNCC2 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:HPLMN Country Code Table: define multiple CC as one country"
			::= { dpsEntry 10 }

		
--  HPLMN CC3
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.11
		dpsHPLMNCC3 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:HPLMN Country Code Table: define multiple CC as one country"
			::= { dpsEntry 11 }

		
--  HPLMN CC4
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.12
		dpsHPLMNCC4 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:HPLMN Country Code Table: define multiple CC as one country"
			::= { dpsEntry 12 }

		
--  HPLMN CC5
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.13
		dpsHPLMNCC5 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:HPLMN Country Code Table: define multiple CC as one country"
			::= { dpsEntry 13 }

		
--  HPLMN CC6
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.14
		dpsHPLMNCC6 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:HPLMN Country Code Table: define multiple CC as one country"
			::= { dpsEntry 14 }

		
--  HPLMN CC7
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.15
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.15
		dpsHPLMNCC7 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:HPLMN Country Code Table: define multiple CC as one country"
			::= { dpsEntry 15 }

		
--  Dialing Prefix
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.16
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.16
		dpsCreateEntrydDalingPrefix OBJECT-TYPE
			SYNTAX INTEGER { create(1) }
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { dpsEntry 16 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.17
		dpsDalingPrefixEntries OBJECT-TYPE
			SYNTAX INTEGER (0..1024)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { dpsEntry 17 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.17
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.18
		dpsRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { dpsEntry 18 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.2.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2
		dpTable OBJECT-TYPE
			SYNTAX SEQUENCE OF DpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { dialingPrefixSet 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.2.3.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1
		dpEntry OBJECT-TYPE
			SYNTAX DpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { dpdpsIndex, dpIndex }
			::= { dpTable 1 }

		
		DpEntry ::=
			SEQUENCE { 
				dpdpsIndex
					INTEGER,
				dpIndex
					INTEGER,
				dpCallNumberPrefix
					DisplayString16,
				dpCallNumberAttribute
					INTEGER,
				dpAdministrationState
					AdminStateChoices,
				dpCallNumberLength
					INTEGER,
				dpServiceType
					INTEGER,
				dpEmergencyType
					INTEGER,
				dpNumberType
					INTEGER,
				dpCLIType
					INTEGER,
				dpRSC
					INTEGER,
				dpCDRFlag
					INTEGER,
				dpMNPFlag
					INTEGER,
				dpPremiumCall
					INTEGER,
				dpCallAllowFlag
					INTEGER,
				dpCallBarFlag
					INTEGER,
				dpNAIForOutgoingCall
					INTEGER,
				dpPSTNNumberOfDigitDeletion
					INTEGER,
				dpPSTNInsertionNumber
					DisplayString16,
				dpE164NumberOfDigitDeletion
					INTEGER,
				dpE164InsertionNumber
					DisplayString16,
				dpRowStatus
					RowStatus
			 }

--  DP DPS Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.1
		dpdpsIndex OBJECT-TYPE
			SYNTAX INTEGER (1..16)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { dpEntry 1 }

		
--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.2
		dpIndex OBJECT-TYPE
			SYNTAX INTEGER (1..1024)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { dpEntry 2 }

		
--  Call Number Prefix
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.3
		dpCallNumberPrefix OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:A combination digits that dial to  originate a call.
				"
			::= { dpEntry 3 }

		
--  Call Number Attribute
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.4
		dpCallNumberAttribute OBJECT-TYPE
			SYNTAX INTEGER
				{
				sub(1),
				unknown(2),
				ndd(3),
				idd(4)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { dpEntry 4 }

		
--  Administration State
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.5
		dpAdministrationState OBJECT-TYPE
			SYNTAX AdminStateChoices
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { dpEntry 5 }

		
--  Call Number Length
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.6
		dpCallNumberLength OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Set the called number length; =0 means do not care"
			DEFVAL { 0 }
			::= { dpEntry 6 }

		
--  Service Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.7
		dpServiceType OBJECT-TYPE
			SYNTAX INTEGER
				{
				normalCall(0),
				emergencyType(1),
				intelligentCall(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Service Type#:0-7=Emergency Numberl [Type A-H];  8=Normal call; 9=Intelligent call"
			DEFVAL { normalCall }
			::= { dpEntry 7 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.8
		dpEmergencyType OBJECT-TYPE
			SYNTAX INTEGER
				{
				zero(0),
				one(1),
				two(2),
				three(3),
				four(4),
				five(5),
				six(6),
				seven(7)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			DEFVAL { zero }
			::= { dpEntry 8 }

		
--  Number Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.9
		dpNumberType OBJECT-TYPE
			SYNTAX INTEGER
				{
				msisdn(0),
				msrn(1),
				pstn(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Indicatior: 0=MSISDN; MSRN; PSTN, Emergency (0-7)"
			DEFVAL { msisdn }
			::= { dpEntry 9 }

		
--  CLI Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.10
		dpCLIType OBJECT-TYPE
			SYNTAX INTEGER
				{
				sub(0),
				ndd(1),
				idd(2),
				unknownSub(3),
				unknownNdd(4),
				unknownIdd(5)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Calling number CLI number type"
			DEFVAL { ndd }
			::= { dpEntry 10 }

		
--  Routing Selection Code
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.11
		dpRSC OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark: set the routing selection plan [RSC] "
			DEFVAL { 0 }
			::= { dpEntry 11 }

		
--  CDR Flag
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.12
		dpCDRFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Generate CDR"
			DEFVAL { enable }
			::= { dpEntry 12 }

		
--  MNP Flag
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.13
		dpMNPFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			DEFVAL { disable }
			::= { dpEntry 13 }

		
--  Premium Call
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.14
		dpPremiumCall OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			DEFVAL { disable }
			::= { dpEntry 14 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.15
		dpCallAllowFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			DEFVAL { enable }
			::= { dpEntry 15 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.16
		dpCallBarFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disbale(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			DEFVAL { enable }
			::= { dpEntry 16 }

		
--  NAI For Outgoing Call
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.17
		dpNAIForOutgoingCall OBJECT-TYPE
			SYNTAX INTEGER
				{
				sub(1),
				unknown(2),
				ndd(3),
				idd(4)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Specify the Nature of Address Indicator (NAI) of an outgoing call for the terminating node to route this call with proper dialed number digit manipulation"
			::= { dpEntry 17 }

		
--  PSTN Number Of Digit Deletion
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.15
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.18
		dpPSTNNumberOfDigitDeletion OBJECT-TYPE
			SYNTAX INTEGER (0..16)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:number of prefix digit to delete (0-16)"
			DEFVAL { 0 }
			::= { dpEntry 18 }

		
--  PSTN Insertion Number
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.16
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.19
		dpPSTNInsertionNumber OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:digits to insert (0-9999999999999999)"
			DEFVAL { 'FFFFFFFFFFFFFFFF'h }
			::= { dpEntry 19 }

		
--  E164 Number Of Digit Deletion
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.17
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.20
		dpE164NumberOfDigitDeletion OBJECT-TYPE
			SYNTAX INTEGER (0..16)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:number of prefix digit to delete (0-16)"
			::= { dpEntry 20 }

		
--  E164 Insertion Number
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.18
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.21
		dpE164InsertionNumber OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:digits to insert (0-9999999999999999)"
			DEFVAL { 'FFFFFFFFFFFFFFFF'h }
			::= { dpEntry 21 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.19
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.22
		dpRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { dpEntry 22 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3
		trunkGroup OBJECT IDENTIFIER ::= { parameter 3 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1
		tgTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TgEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkGroup 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1
		tgEntry OBJECT-TYPE
			SYNTAX TgEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { tgIndex }
			::= { tgTable 1 }

		
		TgEntry ::=
			SEQUENCE { 
				tgIndex
					INTEGER,
				tgTitle
					DisplayString16,
				tgCreateTimeStamp
					TimeStamp,
				tgAdministrationState
					AdminStateChoices,
				tgOperabilityStatus
					OperStateChoices,
				tgAvailabilityStatus
					AvailStateChoices,
				tgOpc
					INTEGER,
				tgDpc
					INTEGER,
				tgNetworkIndication
					INTEGER,
				tgProtocolType
					INTEGER,
				tgProtocolVariant
					INTEGER,
				tgCircuitSelectionMode
					INTEGER,
				tgBackoffFlag
					INTEGER,
				tgTandemRestriction
					INTEGER,
				tgCDRFlag
					INTEGER,
				tgTrunkGroupType
					INTEGER,
				tgRoutingZoneID
					INTEGER,
				tgAlternativeRoutingTrigger
					INTEGER,
				tgCreateEntryTrunk
					INTEGER,
				tgTrunkEntries
					INTEGER,
				tgRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.1
		tgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tgEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.2
		tgTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ASCII Title of the Trunk Group(max length = 16 characters)"
			DEFVAL { "TG#" }
			::= { tgEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.3
		tgCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the TG"
			::= { tgEntry 3 }

		
--  Administration State
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.4
		tgAdministrationState OBJECT-TYPE
			SYNTAX AdminStateChoices
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tgEntry 4 }

		
--  Operability Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.5
		tgOperabilityStatus OBJECT-TYPE
			SYNTAX OperStateChoices
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tgEntry 5 }

		
--  Availability Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.6
		tgAvailabilityStatus OBJECT-TYPE
			SYNTAX AvailStateChoices
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tgEntry 6 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.7
		tgOpc OBJECT-TYPE
			SYNTAX INTEGER (0..16777215)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgEntry 7 }

		
--  DPC
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.8
		tgDpc OBJECT-TYPE
			SYNTAX INTEGER (0..16777215)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tgEntry 8 }

		
--  Network Indication
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.9
		tgNetworkIndication OBJECT-TYPE
			SYNTAX INTEGER
				{
				int(0),
				intSpare(1),
				nat(2),
				natSpare(3)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			DEFVAL { int }
			::= { tgEntry 9 }

		
--  Protocol Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.10
		tgProtocolType OBJECT-TYPE
			SYNTAX INTEGER
				{
				aif(0),
				isup(1),
				bicc(2),
				isdn(3),
				tup(4)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { tgEntry 10 }

		
--  Protocol Variant
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.11
		tgProtocolVariant OBJECT-TYPE
			SYNTAX INTEGER
				{
				itu(0),
				etsi(1),
				ansi(2),
				china(3)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			DEFVAL { itu }
			::= { tgEntry 11 }

		
--  Circuit Selection Mode
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.12
		tgCircuitSelectionMode OBJECT-TYPE
			SYNTAX INTEGER
				{
				clockwise(0),
				antiClockwise(1),
				odd(2),
				even(3)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			DEFVAL { clockwise }
			::= { tgEntry 12 }

		
--  Backoff Flag
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.13
		tgBackoffFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Backoff when dual-seizure happen"
			DEFVAL { enable }
			::= { tgEntry 13 }

		
--  Tandem Restriction
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.14
		tgTandemRestriction OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Inhibit PSTN-PSTN transit call via this trunk group"
			DEFVAL { enable }
			::= { tgEntry 14 }

		
--  CDR Flag
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.15
		tgCDRFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			DEFVAL { enable }
			::= { tgEntry 15 }

		
--  Trunk Group Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.15
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.16
		tgTrunkGroupType OBJECT-TYPE
			SYNTAX INTEGER
				{
				interconnection(0),
				normal(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			DEFVAL { normal }
			::= { tgEntry 16 }

		
--  Routing Zone ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.16
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.17
		tgRoutingZoneID OBJECT-TYPE
			SYNTAX INTEGER (0..31)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Set the Routing Zone of the Trunk Group"
			DEFVAL { 0 }
			::= { tgEntry 17 }

		
--  Alternative Routing Trigger
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.17
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.18
		tgAlternativeRoutingTrigger OBJECT-TYPE
			SYNTAX INTEGER (0..15)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Alternative Routing Trigger [ART ID]"
			DEFVAL { 0 }
			::= { tgEntry 18 }

		
--  Trunk
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.18
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.19
		tgCreateEntryTrunk OBJECT-TYPE
			SYNTAX INTEGER { create(1) }
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { tgEntry 19 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.20
		tgTrunkEntries OBJECT-TYPE
			SYNTAX INTEGER (0..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tgEntry 20 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.19
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.21
		tgRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tgEntry 21 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2
		trunkTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkGroup 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.2.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1
		trunkEntry OBJECT-TYPE
			SYNTAX TrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { trunkIndex, trunkTgIndex }
			::= { trunkTable 1 }

		
		TrunkEntry ::=
			SEQUENCE { 
				trunkTgIndex
					INTEGER,
				trunkIndex
					INTEGER,
				trunkTitle
					DisplayString16,
				trunkCreateTimeStamp
					TimeStamp,
				trunkAdministrationState
					AdminStateChoices,
				trunkOperabilityStatus
					OperStateChoices,
				trunkAvailabilityStatus
					AvailStateChoices,
				trunkMgID
					INTEGER,
				trunkPortID
					INTEGER,
				trunkPortType
					INTEGER,
				trunkGroupID
					INTEGER,
				trunkTypicalCICAssignmentPlan
					INTEGER,
				trunkTypicalCICValueAssignment
					Integer32,
				trunkChannelInUse
					INTEGER,
				trunkCICEntries
					INTEGER,
				trunkRowStatus
					RowStatus
			 }

--  Trunk TG Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.1
		trunkTgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { trunkEntry 1 }

		
--  Trunk Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.2
		trunkIndex OBJECT-TYPE
			SYNTAX INTEGER (1..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { trunkEntry 2 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.3
		trunkTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ASCII Title of the Trunk(max length = 16 characters)"
			DEFVAL { "TK#" }
			::= { trunkEntry 3 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.4
		trunkCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Trunk"
			::= { trunkEntry 4 }

		
--  Administration State
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.5
		trunkAdministrationState OBJECT-TYPE
			SYNTAX AdminStateChoices
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { trunkEntry 5 }

		
--  Operability Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.6
		trunkOperabilityStatus OBJECT-TYPE
			SYNTAX OperStateChoices
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { trunkEntry 6 }

		
--  Availability Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.7
		trunkAvailabilityStatus OBJECT-TYPE
			SYNTAX AvailStateChoices
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { trunkEntry 7 }

		
--  MG ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.8
		trunkMgID OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Which MG; Not applicable to virtual MG"
			DEFVAL { 0 }
			::= { trunkEntry 8 }

		
--  Port ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.9
		trunkPortID OBJECT-TYPE
			SYNTAX INTEGER (0..31)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Which port of the MG; not applicable to virtual MG"
			::= { trunkEntry 9 }

		
--  Port Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.10
		trunkPortType OBJECT-TYPE
			SYNTAX INTEGER
				{
				e1(0),
				t1(1),
				analogue(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			DEFVAL { enable }
			::= { trunkEntry 10 }

		
--  Group ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.11
		trunkGroupID OBJECT-TYPE
			SYNTAX INTEGER
				{
				group0(0),
				group1(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:For redundancy backup"
			DEFVAL { group0 }
			::= { trunkEntry 11 }

		
--  Typical CIC Assignment Plan
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.12
		trunkTypicalCICAssignmentPlan OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			DEFVAL { enable }
			::= { trunkEntry 12 }

		
--  Typical CIC Value Assignment
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.13
		trunkTypicalCICValueAssignment OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Typical CIC value assignment: E1=0, 31, 64бн T1=0, 24, 48бн"
			::= { trunkEntry 13 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.14
		trunkChannelInUse OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkEntry 14 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.15
		trunkCICEntries OBJECT-TYPE
			SYNTAX INTEGER (0..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { trunkEntry 15 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.16
		trunkRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { trunkEntry 16 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3
		cicTable OBJECT-TYPE
			SYNTAX SEQUENCE OF CicEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkGroup 3 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.3.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1
		cicEntry OBJECT-TYPE
			SYNTAX CicEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { cicIndex, cicTrunkIndex, cicTrunkTgIndex }
			::= { cicTable 1 }

		
		CicEntry ::=
			SEQUENCE { 
				cicTrunkTgIndex
					INTEGER,
				cicTrunkIndex
					INTEGER,
				cicIndex
					INTEGER,
				cicType
					INTEGER,
				cicChannelCIC
					Counter32,
				cicCallStatus
					INTEGER,
				cicLocalBlock
					INTEGER,
				cicRemoteBlock
					INTEGER
			 }

--  CIC Trunk TG Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.1
		cicTrunkTgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { cicEntry 1 }

		
--  CIC Trunk Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.2
		cicTrunkIndex OBJECT-TYPE
			SYNTAX INTEGER (1..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { cicEntry 2 }

		
--  CIC Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.3
		cicIndex OBJECT-TYPE
			SYNTAX INTEGER (1..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { cicEntry 3 }

		
--  CIC Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.4
		cicType OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				incoming(1),
				outgoing(2),
				bidirectional(3),
				leaseLine(4),
				dChannel(5),
				xChannel(6)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			DEFVAL { bidirectiona }
			::= { cicEntry 4 }

		
--  Channel CIC
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.5
		cicChannelCIC OBJECT-TYPE
			SYNTAX Counter32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:CIC assigned to the channel"
			::= { cicEntry 5 }

		
--  Call Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.6
		cicCallStatus OBJECT-TYPE
			SYNTAX INTEGER
				{
				idle(0),
				incomingCallOccupied(1),
				outgoingCallOccupied(2)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { cicEntry 6 }

		
--  Local Block
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.7
		cicLocalBlock OBJECT-TYPE
			SYNTAX INTEGER
				{
				unblocked(0),
				localBlocked(1)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { cicEntry 7 }

		
--  Remote Block
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.8
		cicRemoteBlock OBJECT-TYPE
			SYNTAX INTEGER
				{
				unblocked(0),
				remoteBlocked(1)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { cicEntry 8 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4
		locationArea OBJECT IDENTIFIER ::= { parameter 4 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.4.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1
		laTable OBJECT-TYPE
			SYNTAX SEQUENCE OF LaEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { locationArea 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.4.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1
		laEntry OBJECT-TYPE
			SYNTAX LaEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { laIndex }
			::= { laTable 1 }

		
		LaEntry ::=
			SEQUENCE { 
				laIndex
					INTEGER,
				laTitle
					DisplayString16,
				laCreateTimeStamp
					TimeStamp,
				laLAC
					Integer32,
				laTrunkGroup
					INTEGER,
				laPageType
					INTEGER,
				laNumberOfRepeatPaging
					INTEGER,
				laLocalEmergencyNumber0
					DisplayString32,
				laLocalEmergencyNumber1
					DisplayString32,
				laLocalEmergencyNumber2
					DisplayString32,
				laLocalEmergencyNumber3
					DisplayString32,
				laLocalEmergencyNumber4
					DisplayString32,
				laLocalEmergencyNumber5
					DisplayString32,
				laLocalEmergencyNumber6
					DisplayString32,
				laLocalEmergencyNumber7
					DisplayString32,
				laCreateEntryCell
					INTEGER,
				laCellEntries
					INTEGER,
				laRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.1
		laIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { laEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.2
		laTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ASCII Title of the Location Area(max length = 16 characters)"
			DEFVAL { "LA#" }
			::= { laEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.3
		laCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Location Area"
			::= { laEntry 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.4
		laLAC OBJECT-TYPE
			SYNTAX Integer32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { laEntry 4 }

		
--  Trunk Group
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.5
		laTrunkGroup OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Trunk Group of the BSC"
			::= { laEntry 5 }

		
--  Page Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.6
		laPageType OBJECT-TYPE
			SYNTAX INTEGER
				{
				byLAC(0),
				byAllCell(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			DEFVAL { byLAC }
			::= { laEntry 6 }

		
--  Number Of Repeat Paging
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.7
		laNumberOfRepeatPaging OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Number of repeat paging for a MT call before give up."
			DEFVAL { 2 }
			::= { laEntry 7 }

		
--  Local Emergency Number0
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.8
		laLocalEmergencyNumber0 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { laEntry 8 }

		
--  Local Emergency Number1
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.9
		laLocalEmergencyNumber1 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { laEntry 9 }

		
--  Local Emergency Number2
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.10
		laLocalEmergencyNumber2 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { laEntry 10 }

		
--  Local Emergency Number3
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.11
		laLocalEmergencyNumber3 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { laEntry 11 }

		
--  Local Emergency Number4
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.12
		laLocalEmergencyNumber4 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { laEntry 12 }

		
--  Local Emergency Number5
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.13
		laLocalEmergencyNumber5 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { laEntry 13 }

		
--  Local Emergency Number6
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.14
		laLocalEmergencyNumber6 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { laEntry 14 }

		
--  Local Emergency Number7
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.15
		laLocalEmergencyNumber7 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { laEntry 15 }

		
--  Cell
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.15
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.16
		laCreateEntryCell OBJECT-TYPE
			SYNTAX INTEGER { create(1) }
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { laEntry 16 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.17
		laCellEntries OBJECT-TYPE
			SYNTAX INTEGER (0..16)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { laEntry 17 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.16
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.18
		laRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { laEntry 18 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.4.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2
		cellTable OBJECT-TYPE
			SYNTAX SEQUENCE OF CellEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { locationArea 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.4.3.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1
		cellEntry OBJECT-TYPE
			SYNTAX CellEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { cellLaIndex, cellIndex }
			::= { cellTable 1 }

		
		CellEntry ::=
			SEQUENCE { 
				cellLaIndex
					INTEGER,
				cellIndex
					INTEGER,
				cellTitle
					DisplayString16,
				cellCreateTimeStamp
					TimeStamp,
				cellRoutingZoneID
					INTEGER,
				cellRegionalSubscriptionZoneCode
					INTEGER,
				cellID
					INTEGER,
				cellLocalEmergencyNumber0
					DisplayString32,
				cellLocalEmergencyNumber1
					DisplayString32,
				cellLocalEmergencyNumber2
					DisplayString32,
				cellLocalEmergencyNumber3
					DisplayString32,
				cellLocalEmergencyNumber4
					DisplayString32,
				cellLocalEmergencyNumber5
					DisplayString32,
				cellLocalEmergencyNumber6
					DisplayString32,
				cellLocalEmergencyNumber7
					DisplayString32,
				cellRowStatus
					RowStatus
			 }

--  Cell Location Area Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.1
		cellLaIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { cellEntry 1 }

		
--  Cell Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.2
		cellIndex OBJECT-TYPE
			SYNTAX INTEGER (1..16)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { cellEntry 2 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.3
		cellTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ASCII Title of the Location Area(max length = 16 characters)"
			DEFVAL { "CELL#" }
			::= { cellEntry 3 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.4
		cellCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Cell"
			::= { cellEntry 4 }

		
--  Rounting Zone ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.5
		cellRoutingZoneID OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Select the routing zone of the cell"
			DEFVAL { 0 }
			::= { cellEntry 5 }

		
--  Regional Subscription Zone Code
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.6
		cellRegionalSubscriptionZoneCode OBJECT-TYPE
			SYNTAX INTEGER (0..65535)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:A 2 byte Regional Subscription Zone Code. Defines the regional subscription zone that this cell belong to. FFFF=no RSZC"
			DEFVAL { 'FF'h }
			::= { cellEntry 6 }

		
--  Cell ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.7
		cellID OBJECT-TYPE
			SYNTAX INTEGER (0..65535)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { cellEntry 7 }

		
--  Cell Local Emergency Number0
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.8
		cellLocalEmergencyNumber0 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { cellEntry 8 }

		
--  Cell Local Emergency Number1
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.9
		cellLocalEmergencyNumber1 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { cellEntry 9 }

		
--  Cell Local Emergency Number2
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.10
		cellLocalEmergencyNumber2 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { cellEntry 10 }

		
--  Cell Local Emergency Number3
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.11
		cellLocalEmergencyNumber3 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { cellEntry 11 }

		
--  Cell Local Emergency Number4
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.12
		cellLocalEmergencyNumber4 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { cellEntry 12 }

		
--  Cell Local Emergency Number5
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.13
		cellLocalEmergencyNumber5 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { cellEntry 13 }

		
--  Cell Local Emergency Number6
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.14
		cellLocalEmergencyNumber6 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { cellEntry 14 }

		
--  Cell Local Emergency Number7
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.15
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.15
		cellLocalEmergencyNumber7 OBJECT-TYPE
			SYNTAX DisplayString32
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { cellEntry 15 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.16
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.16
		cellRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { cellEntry 16 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5
		mediaGateway OBJECT IDENTIFIER ::= { parameter 5 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.5.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1
		mgTable OBJECT-TYPE
			SYNTAX SEQUENCE OF MgEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { mediaGateway 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.5.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1
		mgEntry OBJECT-TYPE
			SYNTAX MgEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { mgIndex }
			::= { mgTable 1 }

		
		MgEntry ::=
			SEQUENCE { 
				mgIndex
					INTEGER,
				mgTitle
					DisplayString16,
				mgCreateTimeStamp
					TimeStamp,
				mgAdministrationState
					AdminStateChoices,
				mgIp
					IpAddress,
				mgDomainName
					DisplayString16,
				mgSwitchingMode
					INTEGER,
				mgEndPoint
					INTEGER,
				mgToneGenCapability
					INTEGER,
				mgType
					INTEGER,
				mgMaxPhysicalPorts
					INTEGER,
				mgMaxChannels
					INTEGER,
				mgPacketizationPeriod
					INTEGER,
				mgPriorityLevel
					INTEGER,
				mgCodecType
					OCTET STRING,
				mgPhysicalPortEntries
					INTEGER,
				mgRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.1
		mgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { mgEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.2
		mgTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ASCII Title of the MG (max length = 16 characters)"
			DEFVAL { "MG#" }
			::= { mgEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.3
		mgCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the MG table"
			::= { mgEntry 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.4
		mgAdministrationState OBJECT-TYPE
			SYNTAX AdminStateChoices
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { mgEntry 4 }

		
--  IP
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.5
		mgIp OBJECT-TYPE
			SYNTAX IpAddress
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:IP address of the MG or 8KE1 Card"
			::= { mgEntry 5 }

		
--  Domain Name
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.6
		mgDomainName OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Domain Name of the MG"
			::= { mgEntry 6 }

		
--  Switching Mode
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.7
		mgSwitchingMode OBJECT-TYPE
			SYNTAX INTEGER
				{
				mgcp(0),
				eightECP(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Circuit Switch (8KE1) or Soft Switch (MG)"
			DEFVAL { mgcp }
			::= { mgEntry 7 }

		
--  End Point Description
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.8
		mgEndPoint OBJECT-TYPE
			SYNTAX INTEGER
				{
				structured(1),
				unStructured(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:MGCP Endpoint description method: structured or unstructured"
			DEFVAL { structured }
			::= { mgEntry 8 }

		
--  Tone Gen Capability
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.9
		mgToneGenCapability OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:If MG has tone gen cap then will use its tone gen"
			DEFVAL { enable }
			::= { mgEntry 9 }

		
--  MG Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.10
		mgType OBJECT-TYPE
			SYNTAX INTEGER
				{
				audioCodes(1),
				lgcMG(2),
				lgcCS(3),
				analogLine(11),
				announcementServer(21),
				interactiveVoiceResponse(31),
				conferenceBridge(41),
				packetRelay(51),
				wiretap(61),
				atm(71)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			DEFVAL { digitalChannel }
			::= { mgEntry 10 }

		
--  Max Physical Ports
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.11
		mgMaxPhysicalPorts OBJECT-TYPE
			SYNTAX INTEGER (0..32)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Max Physical Port number of the MG. Max=32 ports; Not applicable to virtual MG
								"
			::= { mgEntry 11 }

		
--  Max Channels
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.12
		mgMaxChannels OBJECT-TYPE
			SYNTAX INTEGER (0..1024)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Maximum channels of the virtual MG.Max=1024channels; Applicable to virtual MG only
								"
			::= { mgEntry 12 }

		
--  Packetization Period
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.13
		mgPacketizationPeriod OBJECT-TYPE
			SYNTAX INTEGER
				{
				x20ms(20),
				x40ms(40),
				x60ms(60),
				x80ms(80)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			DEFVAL { x20ms }
			::= { mgEntry 13 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.14
		mgPriorityLevel OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Set the priority level of the MG codec table; 255=highest priority level; 0=least priority level. In the MGCP codec negotiation, codec type always follow the MG [Codec Table] with the higher priority level. If two MGs are in the same priority level then follows the MG with higher MG ID#"
			::= { mgEntry 14 }

		
--  Codec Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.15
		mgCodecType OBJECT-TYPE
			SYNTAX OCTET STRING (SIZE (16))
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:0=ALaw, 1=uLaw, 2=FR, 3-EFR, 4=AMR, G729b, ff=nil;
				Entry 0-15, entry 0 is the highest priority, entry 15 is the least"
			::= { mgEntry 15 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.16
		mgPhysicalPortEntries OBJECT-TYPE
			SYNTAX INTEGER (0..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { mgEntry 16 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.17
		mgRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { mgEntry 17 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2
		ppTable OBJECT-TYPE
			SYNTAX SEQUENCE OF PpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { mediaGateway 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1
		ppEntry OBJECT-TYPE
			SYNTAX PpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { ppMgIndex, ppIndex }
			::= { ppTable 1 }

		
		PpEntry ::=
			SEQUENCE { 
				ppMgIndex
					INTEGER,
				ppIndex
					INTEGER,
				ppUsedFlag
					INTEGER,
				ppStatus
					INTEGER
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.1
		ppMgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { ppEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.2
		ppIndex OBJECT-TYPE
			SYNTAX INTEGER (1..32)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { ppEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.3
		ppUsedFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				idle(0),
				inUse(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { ppEntry 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.4
		ppStatus OBJECT-TYPE
			SYNTAX INTEGER
				{
				l1NotReady(0),
				l1Ready(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { ppEntry 4 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6
		alternativeRoutingTrigger OBJECT IDENTIFIER ::= { parameter 6 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.6.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1
		artTable OBJECT-TYPE
			SYNTAX SEQUENCE OF ArtEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { alternativeRoutingTrigger 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.6.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1
		artEntry OBJECT-TYPE
			SYNTAX ArtEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { artIndex }
			::= { artTable 1 }

		
		ArtEntry ::=
			SEQUENCE { 
				artIndex
					INTEGER,
				artTitle
					DisplayString16,
				artCreateTimeStamp
					TimeStamp,
				artCreateEntryTriggerCause
					INTEGER,
				artTriggerCauseEntries
					INTEGER,
				artRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.1
		artIndex OBJECT-TYPE
			SYNTAX INTEGER (1..16)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { artEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.2
		artTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ASCII Title of the Alternative Routing Trigger Table(max length = 16 characters)"
			DEFVAL { "ART#" }
			::= { artEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.3
		artCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Creation date and time of the Alternative Routing Trigger Table"
			::= { artEntry 3 }

		
--  Trigger Cause
-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.4
		artCreateEntryTriggerCause OBJECT-TYPE
			SYNTAX INTEGER { create(1) }
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { artEntry 4 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.5
		artTriggerCauseEntries OBJECT-TYPE
			SYNTAX INTEGER (0..128)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { artEntry 5 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.6
		artRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { artEntry 6 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.6.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2
		tcTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TcEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { alternativeRoutingTrigger 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.6.2.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1
		tcEntry OBJECT-TYPE
			SYNTAX TcEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { tcArtIndex, tcIndex }
			::= { tcTable 1 }

		
		TcEntry ::=
			SEQUENCE { 
				tcArtIndex
					INTEGER,
				tcIndex
					INTEGER,
				tcCauseValue
					INTEGER,
				tcRowStatus
					RowStatus
			 }

--  Trigger Cause Art Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.1
		tcArtIndex OBJECT-TYPE
			SYNTAX INTEGER (1..16)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { tcEntry 1 }

		
--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.2
		tcIndex OBJECT-TYPE
			SYNTAX INTEGER (1..128)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tcEntry 2 }

		
--  Cause Value
-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.3
		tcCauseValue OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ISUP cause values in this table will trigger the alternative routing"
			::= { tcEntry 3 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.4
		tcRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tcEntry 4 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7
		callUnattainableAnnouncements OBJECT IDENTIFIER ::= { parameter 7 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.7.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1
		cuaTable OBJECT-TYPE
			SYNTAX SEQUENCE OF CuaEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { callUnattainableAnnouncements 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.7.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1
		cuaEntry OBJECT-TYPE
			SYNTAX CuaEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { cuaIndex }
			::= { cuaTable 1 }

		
		CuaEntry ::=
			SEQUENCE { 
				cuaIndex
					INTEGER,
				cuaTitle
					DisplayString16,
				cuaCreateTimeStamp
					TimeStamp,
				cuaAASPrefix
					DisplayString16,
				cuaCreateEntryAnnouncementCUA
					INTEGER,
				cuaAnnouncementCUAEntries
					INTEGER,
				cuaRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.1
		cuaIndex OBJECT-TYPE
			SYNTAX INTEGER (1..16)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { cuaEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.2
		cuaTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ASCII Title of the Call Unattainable Announcement Set (max length = 16 characters)"
			DEFVAL { "CUA#" }
			::= { cuaEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.3
		cuaCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Call Unattainable Announcement Table"
			::= { cuaEntry 3 }

		
--  AAS Prefix
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.4
		cuaAASPrefix OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Dailing Prefix of the AAS."
			DEFVAL { "***8" }
			::= { cuaEntry 4 }

		
--  Announcement
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.5
		cuaCreateEntryAnnouncementCUA OBJECT-TYPE
			SYNTAX INTEGER { create(1) }
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { cuaEntry 5 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.6
		cuaAnnouncementCUAEntries OBJECT-TYPE
			SYNTAX INTEGER (0..128)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { cuaEntry 6 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.1.1.7
		cuaRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { cuaEntry 7 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.7.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2
		acTable OBJECT-TYPE
			SYNTAX SEQUENCE OF AcEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { callUnattainableAnnouncements 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.7.2.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1
		acEntry OBJECT-TYPE
			SYNTAX AcEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { acCuaIndex, acIndex }
			::= { acTable 1 }

		
		AcEntry ::=
			SEQUENCE { 
				acCuaIndex
					INTEGER,
				acIndex
					INTEGER,
				acCauseValue
					INTEGER,
				acAnnouncementType
					INTEGER,
				acAnnouncementCode
					INTEGER,
				acRowStatus
					RowStatus
			 }

--  Announcement CUA Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.1
		acCuaIndex OBJECT-TYPE
			SYNTAX INTEGER (1..16)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { acEntry 1 }

		
--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.2
		acIndex OBJECT-TYPE
			SYNTAX INTEGER (1..128)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { acEntry 2 }

		
--  Cause Value
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.3
		acCauseValue OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ISUP cause value"
			::= { acEntry 3 }

		
--  Announcement Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.4
		acAnnouncementType OBJECT-TYPE
			SYNTAX INTEGER
				{
				playAnnouncement(0),
				playTone(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			DEFVAL { playAnnouncement }
			::= { acEntry 4 }

		
--  Announcement Code
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.5
		acAnnouncementCode OBJECT-TYPE
			SYNTAX INTEGER (0..999)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Announcement Number = AAS Prefix + Announcement code. Announcement code is concatenated with AAS prefix to form the announcement number"
			::= { acEntry 5 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.7.2.1.6
		acRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { acEntry 6 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8
		leaseCircuitStatisticConnection OBJECT IDENTIFIER ::= { parameter 8 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.8.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1
		sctTable OBJECT-TYPE
			SYNTAX SEQUENCE OF SctEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { leaseCircuitStatisticConnection 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.8.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1
		sctEntry OBJECT-TYPE
			SYNTAX SctEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { sctIndex }
			::= { sctTable 1 }

		
		SctEntry ::=
			SEQUENCE { 
				sctIndex
					INTEGER,
				sctTitle
					DisplayString16,
				sctCreateTimeStamp
					TimeStamp,
				sctOMG
					INTEGER,
				sctOTrunk
					INTEGER,
				sctOChannel
					INTEGER,
				sctDMG
					INTEGER,
				sctDTrunk
					INTEGER,
				sctDChannel
					INTEGER,
				sctRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.1
		sctIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { sctEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.2
		sctTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:ASCII Title of the Lease Circuit(max length = 16 characters)"
			DEFVAL { "LC#" }
			::= { sctEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.3
		sctCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Lease Circuit"
			::= { sctEntry 3 }

		
--  Origination MG
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.4
		sctOMG OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:MG# of the origination MG"
			::= { sctEntry 4 }

		
--  Origination Trunk
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.5
		sctOTrunk OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Trunk# of the origination MG"
			::= { sctEntry 5 }

		
--  Origination Channel
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.6
		sctOChannel OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Channelt# of the lease line of the origination Trunk"
			::= { sctEntry 6 }

		
--  Destination MG
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.7
		sctDMG OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:MG# of the destination MG"
			::= { sctEntry 7 }

		
--  Destination Trunk
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.8
		sctDTrunk OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Trunk# of the destination MG"
			::= { sctEntry 8 }

		
--  Destination Channel
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.9
		sctDChannel OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Channel# of the lease line of the destination Trunk"
			::= { sctEntry 9 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.10
		sctRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { sctEntry 10 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3
		csta OBJECT IDENTIFIER ::= { msc 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.3
		tgIncomingTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TgIncomingEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.3.1
		tgIncomingEntry OBJECT-TYPE
			SYNTAX TgIncomingEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { tgIncomingTgndex, tgIncomingIndex }
			::= { tgIncomingTable 1 }

		
		TgIncomingEntry ::=
			SEQUENCE { 
				tgIncomingTgndex
					INTEGER,
				tgIncomingIndex
					INTEGER,
				tgIncomingData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.3.1.1
		tgIncomingTgndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgIncomingEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.3.1.2
		tgIncomingIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgIncomingEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.3.1.3
		tgIncomingData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgIncomingEntry 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.4
		tgOutgoingTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TgOutgoingEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 4 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.4.1
		tgOutgoingEntry OBJECT-TYPE
			SYNTAX TgOutgoingEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { tgOutgoingTgIndex, tgOutgoingIndex }
			::= { tgOutgoingTable 1 }

		
		TgOutgoingEntry ::=
			SEQUENCE { 
				tgOutgoingTgIndex
					INTEGER,
				tgOutgoingIndex
					INTEGER,
				tgOutgoingData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.4.1.1
		tgOutgoingTgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgOutgoingEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.4.1.2
		tgOutgoingIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgOutgoingEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.4.1.3
		tgOutgoingData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgOutgoingEntry 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.5
		subsToSubsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF SubsToSubsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 5 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.5.1
		subsToSubsEntry OBJECT-TYPE
			SYNTAX SubsToSubsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { subsToSubsIndex }
			::= { subsToSubsTable 1 }

		
		SubsToSubsEntry ::=
			SEQUENCE { 
				subsToSubsIndex
					INTEGER,
				subsToSubsData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.5.1.1
		subsToSubsIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToSubsEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.5.1.2
		subsToSubsData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToSubsEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.6
		subsToTrunkTable OBJECT-TYPE
			SYNTAX SEQUENCE OF SubsToTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 6 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.6.1
		subsToTrunkEntry OBJECT-TYPE
			SYNTAX SubsToTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { subsToTrunkIndex }
			::= { subsToTrunkTable 1 }

		
		SubsToTrunkEntry ::=
			SEQUENCE { 
				subsToTrunkIndex
					INTEGER,
				subsToTrunkData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.6.1.1
		subsToTrunkIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToTrunkEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.6.1.2
		subsToTrunkData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToTrunkEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.7
		trunkToSubsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TrunkToSubsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 7 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.7.1
		trunkToSubsEntry OBJECT-TYPE
			SYNTAX TrunkToSubsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { trunkToSubsIndex }
			::= { trunkToSubsTable 1 }

		
		TrunkToSubsEntry ::=
			SEQUENCE { 
				trunkToSubsIndex
					INTEGER,
				trunkToSubsData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.7.1.1
		trunkToSubsIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToSubsEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.7.1.2
		trunkToSubsData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToSubsEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.8
		trunkToTrunkTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TrunkToTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 8 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.8.1
		trunkToTrunkEntry OBJECT-TYPE
			SYNTAX TrunkToTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { trunkToTrunkIndex }
			::= { trunkToTrunkTable 1 }

		
		TrunkToTrunkEntry ::=
			SEQUENCE { 
				trunkToTrunkIndex
					INTEGER,
				trunkToTrunkData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.8.1.1
		trunkToTrunkIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToTrunkEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.8.1.2
		trunkToTrunkData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToTrunkEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.9
		intraconnectionTable OBJECT-TYPE
			SYNTAX SEQUENCE OF IntraconnectionEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 9 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.9.1
		intraconnectionEntry OBJECT-TYPE
			SYNTAX IntraconnectionEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { intraconnectionIndex }
			::= { intraconnectionTable 1 }

		
		IntraconnectionEntry ::=
			SEQUENCE { 
				intraconnectionIndex
					INTEGER,
				intraconnectionData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.9.1.1
		intraconnectionIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { intraconnectionEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.9.1.2
		intraconnectionData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { intraconnectionEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.10
		subsToIpTable OBJECT-TYPE
			SYNTAX SEQUENCE OF SubsToIpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 10 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.10.1
		subsToIpEntry OBJECT-TYPE
			SYNTAX SubsToIpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { subsToIpIndex }
			::= { subsToIpTable 1 }

		
		SubsToIpEntry ::=
			SEQUENCE { 
				subsToIpIndex
					INTEGER,
				subsToIpData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.10.1.1
		subsToIpIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToIpEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.10.1.2
		subsToIpData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToIpEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.11
		trunkToIpTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TrunkToIpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 11 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.11.1
		trunkToIpEntry OBJECT-TYPE
			SYNTAX TrunkToIpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { trunkToIpIndex }
			::= { trunkToIpTable 1 }

		
		TrunkToIpEntry ::=
			SEQUENCE { 
				trunkToIpIndex
					INTEGER,
				trunkToIpData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.11.1.1
		trunkToIpIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToIpEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.11.1.2
		trunkToIpData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToIpEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.12
		mobileOriginatedTable OBJECT-TYPE
			SYNTAX SEQUENCE OF MobileOriginatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 12 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.12.1
		mobileOriginatedEntry OBJECT-TYPE
			SYNTAX MobileOriginatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { mobileOriginatedIndex }
			::= { mobileOriginatedTable 1 }

		
		MobileOriginatedEntry ::=
			SEQUENCE { 
				mobileOriginatedIndex
					INTEGER,
				mobileOriginatedData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.12.1.1
		mobileOriginatedIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { mobileOriginatedEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.12.1.2
		mobileOriginatedData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { mobileOriginatedEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.13
		mobileTerminatedTable OBJECT-TYPE
			SYNTAX SEQUENCE OF MobileTerminatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 13 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.13.1
		mobileTerminatedEntry OBJECT-TYPE
			SYNTAX MobileTerminatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { mobileTerminatedIndex }
			::= { mobileTerminatedTable 1 }

		
		MobileTerminatedEntry ::=
			SEQUENCE { 
				mobileTerminatedIndex
					INTEGER,
				mobileTermiginatedData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.13.1.1
		mobileTerminatedIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { mobileTerminatedEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.13.1.2
		mobileTermiginatedData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { mobileTerminatedEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.14
		inTrunkTable OBJECT-TYPE
			SYNTAX SEQUENCE OF InTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 14 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.14.1
		inTrunkEntry OBJECT-TYPE
			SYNTAX InTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { inTrunkIndex }
			::= { inTrunkTable 1 }

		
		InTrunkEntry ::=
			SEQUENCE { 
				inTrunkIndex
					INTEGER,
				inTrunkData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.14.1.1
		inTrunkIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { inTrunkEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.14.1.2
		inTrunkData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { inTrunkEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.15
		outTrunkTable OBJECT-TYPE
			SYNTAX SEQUENCE OF OutTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 15 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.15.1
		outTrunkEntry OBJECT-TYPE
			SYNTAX OutTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { outTrunkIndex }
			::= { outTrunkTable 1 }

		
		OutTrunkEntry ::=
			SEQUENCE { 
				outTrunkIndex
					INTEGER,
				outTrunkData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.15.1.1
		outTrunkIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { outTrunkEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.15.1.2
		outTrunkData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { outTrunkEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.16
		ipTerminatedTable OBJECT-TYPE
			SYNTAX SEQUENCE OF IpTerminatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 16 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.16.1
		ipTerminatedEntry OBJECT-TYPE
			SYNTAX IpTerminatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { ipTermiginatedIndex }
			::= { ipTerminatedTable 1 }

		
		IpTerminatedEntry ::=
			SEQUENCE { 
				ipTermiginatedIndex
					INTEGER,
				ipTermiginatedData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.16.1.1
		ipTermiginatedIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { ipTerminatedEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.16.1.2
		ipTermiginatedData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { ipTerminatedEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.4
		cdr OBJECT IDENTIFIER ::= { msc 4 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.4.1
		cdrHeadOid OBJECT-TYPE
			SYNTAX INTEGER
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { cdr 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.4.2
		cdrTailOid OBJECT-TYPE
			SYNTAX INTEGER
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { cdr 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.4.3
		cdrDataOid OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { cdr 3 }

		
	
	END

--
-- LGC-SS-MSC-MIB_070824.my
--
