--
-- LGC-SS-MSC-MIB-R91-official-080825.my
-- MIB generated by MG-SOFT Visual MIB Builder Version 7.0  Build 220
-- Monday, August 25, 2008 at 14:01:05
--

	LGC-SS-MSC-MIB DEFINITIONS ::= BEGIN
 
		IMPORTS
			lgcSS, DisplayString16, TimeStamp, RowStatus, DisplayString8, 
			DisplayString, AdminStateChoices, OperStateChoices			
				FROM LGC-MIB			
			IpAddress, Opaque, OBJECT-TYPE, MODULE-IDENTITY			
				FROM SNMPv2-SMI;
	
	
		-- 1.3.6.1.4.1.1373.2.3.3.2
		msc MODULE-IDENTITY 
			LAST-UPDATED "200706291606Z"		-- June 29, 2007 at 16:06 GMT
			ORGANIZATION 
				"LGC Wireless"
			CONTACT-INFO 
				"lcrd
				lcrdsupport@lgcwireless.com"
			DESCRIPTION 
				"Description."
			REVISION "200706051219Z"		-- June 05, 2007 at 12:19 GMT
			DESCRIPTION 
				"This is the first release version of the MSC MIB"
			::= { application 2 }

		
	
--
-- Type definitions
--
	
		AvailStateChoices ::= INTEGER
			{
			inTest(0),
			failed(1),
			powerOff(2),
			offLine(3),
			onLine(4),
			dependency(5),
			degraded(6),
			notInstalled(7)
			}

	
	
--
-- Node definitions
--
	
-- Node definitions
-- 
--  The MIB module for WXC2.
-- 1.3.6.1.4.1.1373.1.3
		-- 1.3.6.1.4.1.1373.2.3
		wxc2 OBJECT IDENTIFIER ::= { lgcSS 3 }

		
--  1.3.6.1.4.1.1373.1.3.3
		-- 1.3.6.1.4.1.1373.2.3.3
		application OBJECT IDENTIFIER ::= { wxc2 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.1
		heartbeat OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { msc 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2
		parameter OBJECT IDENTIFIER ::= { msc 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1
		system OBJECT IDENTIFIER ::= { parameter 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1
		cdrOption OBJECT-TYPE
			SYNTAX Opaque (SIZE (8))
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"OPAQUE DECODE RULE:
				[unit]MO Call[u]00.0-00.0[u]select
				[v]0[opt]Disable
				[v]1[opt]Enable
				[unit]MT Call[u]00.1-00.1[u]select
				[v]0[opt]Disable
				[v]1[opt]Enable
				[unit]Roaming[u]00.2-00.2[u]select
				[v]0[opt]Disable
				[v]1[opt]Enable
				[unit]In Gateway[u]00.3-00.3[u]select
				[v]0[opt]Disable
				[v]1[opt]Enable
				[unit]Out Gateway[u]00.4-00.4[u]select
				[v]0[opt]Disable
				[v]1[opt]Enable
				[unit]Transit Call[u]00.5-00.5[u]select
				[v]0[opt]Disable
				[v]1[opt]Enable
				[unit]SS Action[u]00.6-00.6[u]select
				[v]0[opt]Disable
				[v]1[opt]Enable
				[unit]MO SMS[u]00.7-00.7[u]select
				[v]0[opt]Disable
				[v]1[opt]Enable
				[unit]MT SMS[u]01.0-01.0[u]select
				[v]0[opt]Disable
				[v]1[opt]Enable
				[unit]Common Equipment[u]01.1-01.1[u]select
				[v]0[opt]Disable
				[v]1[opt]Enable
				[unit]Term CAMEL[u]01.2-01.2[u]select
				[v]0[opt]Disable
				[v]1[opt]Enable
				[unit]Reserved[u]01.3-01.7[u]select
				[unit]Reserved[u]02.0-03.7[u]select"
			::= { system 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.2
		maxCallDurationMO OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Define the permitted maximum call duration for MO call. Any ongoing call reaching this threshold will be compulsively cut off. Set 0 to disable this function."
			::= { system 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.3
		maxCallDurationMT OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Define the permitted maximum call duration for MT call. Any incoming call reaching this threshold will be compulsively cut off. Set 0 to disable this function."
			::= { system 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4
		locationNumber OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { system 4 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2
		routingZoneSet OBJECT IDENTIFIER ::= { parameter 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1
		rzsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF RzsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { routingZoneSet 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1
		rzsEntry OBJECT-TYPE
			SYNTAX RzsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { rzsIndex }
			::= { rzsTable 1 }

		
		RzsEntry ::=
			SEQUENCE { 
				rzsIndex
					INTEGER,
				rzsTitle
					DisplayString16,
				rzsCreateTimeStamp
					TimeStamp,
				rzsDialingPrefixSetID
					INTEGER,
				rzsAnnouncementSetID
					INTEGER,
				rzsMSRNRangeStart
					DisplayString16,
				rzsMSRNRangeEnd
					DisplayString16,
				rzsNITZ
					INTEGER,
				rzsSRFNumber0
					DisplayString16,
				rzsSRFNumber1
					DisplayString16,
				rzsCreateEntryRoutingSelection
					INTEGER,
				rzsRoutingSelectionEntries
					INTEGER,
				rzsRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.1
		rzsIndex OBJECT-TYPE
			SYNTAX INTEGER (1..31)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 32."
			::= { rzsEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.2
		rzsTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Title of the Routing Zone Set (max 16 characters)."
			DEFVAL { "RZS#" }
			::= { rzsEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.3
		rzsCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Routing Zone Set."
			::= { rzsEntry 3 }

		
--  Dialing Prefix Set ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.4
		rzsDialingPrefixSetID OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Specify the Dialing Prefix Set ID to this Routing Zone Set."
			DEFVAL { 0 }
			::= { rzsEntry 4 }

		
--  Announcement(CUA) Set ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.5
		rzsAnnouncementSetID OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Specify the Call Unattainable Announcement Set ID to this Routing Zone Set."
			::= { rzsEntry 5 }

		
--  MSRN Range Start
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.6
		rzsMSRNRangeStart OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:The start of the MSRN range for this Routing Zone."
			::= { rzsEntry 6 }

		
--  MSRN Range End
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.7
		rzsMSRNRangeEnd OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:The end of the MSRN range for this Routing Zone."
			::= { rzsEntry 7 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.8
		rzsNITZ OBJECT-TYPE
			SYNTAX INTEGER
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Specify the Network Identity and Time Zone."
			::= { rzsEntry 8 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.9
		rzsSRFNumber0 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The E.164 node address of the SRF connecting to MSS platform 0."
			::= { rzsEntry 9 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.10
		rzsSRFNumber1 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The E.164 node address of the SRF connecting to MSS platform 1."
			::= { rzsEntry 10 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.11
		rzsCreateEntryRoutingSelection OBJECT-TYPE
			SYNTAX INTEGER (1..31)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { rzsEntry 11 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.12
		rzsRoutingSelectionEntries OBJECT-TYPE
			SYNTAX INTEGER (0..31)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:The total number of configured Routing Selections in this Routing Zone Set."
			::= { rzsEntry 12 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.13
		rzsRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { rzsEntry 13 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2
		rsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF RsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { routingZoneSet 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.1.4.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1
		rsEntry OBJECT-TYPE
			SYNTAX RsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { rsRzsIndex, rsIndex }
			::= { rsTable 1 }

		
		RsEntry ::=
			SEQUENCE { 
				rsRzsIndex
					INTEGER,
				rsIndex
					INTEGER,
				rsTitle
					DisplayString16,
				rsCreateTimeStamp
					TimeStamp,
				rsTrunkGroup
					INTEGER,
				rsAlternativeTrunkGroupOption
					INTEGER,
				rsAlternativeTrunkGroup
					INTEGER,
				rsNAIForOutgoingCall
					INTEGER,
				rsNumberOfDigitDeletion
					INTEGER,
				rsInsertionNumber
					DisplayString16,
				rsRowStatus
					RowStatus
			 }

--  Route Selection RZS Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.1
		rsRzsIndex OBJECT-TYPE
			SYNTAX INTEGER (1..31)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { rsEntry 1 }

		
--  Route Selection Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.2
		rsIndex OBJECT-TYPE
			SYNTAX INTEGER (1..31)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 32."
			::= { rsEntry 2 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.3
		rsTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Title of the Routing Selection (max 16 characters)."
			DEFVAL { "RS#" }
			::= { rsEntry 3 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.4
		rsCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Routing Selection."
			::= { rsEntry 4 }

		
--  Trunk Group
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.5
		rsTrunkGroup OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Select the Trunk Group for the outgoing routing. "
			DEFVAL { 0 }
			::= { rsEntry 5 }

		
--  Alternative Trunk Group Option
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.6
		rsAlternativeTrunkGroupOption OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Enable or disable alternative Trunk Group when the primary Trunk Group is unavailable. "
			DEFVAL { disable }
			::= { rsEntry 6 }

		
--  Alternative Trunk Group
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.7
		rsAlternativeTrunkGroup OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Specify the alternative Trunk Group. It is available only when the previous Alternative TG Flag is enabled."
			DEFVAL { 0 }
			::= { rsEntry 7 }

		
--  NAI For Outgoing Call
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.8
		rsNAIForOutgoingCall OBJECT-TYPE
			SYNTAX INTEGER
				{
				sub(1),
				unknown(2),
				ndd(3),
				idd(4),
				UKSpecific(126)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Type Of Number for outgoing call."
			::= { rsEntry 8 }

		
--  Number Of Digit Deletion
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.9
		rsNumberOfDigitDeletion OBJECT-TYPE
			SYNTAX INTEGER (0..16)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Number of digits to be deleted from the beginning of the dialed number. "
			DEFVAL { 0 }
			::= { rsEntry 9 }

		
--  Insertion Number
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.10
		rsInsertionNumber OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The digits to be inserted to the front of the dialed number."
			DEFVAL { "FFFFFFFFFFFFFFFF" }
			::= { rsEntry 10 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.1.4.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.2.1.11
		rsRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { rsEntry 11 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3
		dialingPrefixSet OBJECT IDENTIFIER ::= { parameter 3 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.2.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1
		dpsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF DpsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { dialingPrefixSet 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.2.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1
		dpsEntry OBJECT-TYPE
			SYNTAX DpsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { dpsIndex }
			::= { dpsTable 1 }

		
		DpsEntry ::=
			SEQUENCE { 
				dpsIndex
					INTEGER,
				dpsTitle
					DisplayString16,
				dpsCreateTimeStamp
					TimeStamp,
				dpsCC
					DisplayString8,
				dpsNDC
					DisplayString8,
				dpsInternationalPrefix
					DisplayString8,
				dpsNationalPrefix
					DisplayString8,
				dpsHPLMNCC0
					DisplayString16,
				dpsHPLMNCC1
					DisplayString16,
				dpsHPLMNCC2
					DisplayString16,
				dpsHPLMNCC3
					DisplayString16,
				dpsHPLMNCC4
					DisplayString16,
				dpsHPLMNCC5
					DisplayString16,
				dpsHPLMNCC6
					DisplayString16,
				dpsHPLMNCC7
					DisplayString16,
				dpsCreateEntrydDalingPrefix
					INTEGER,
				dpsDialingPrefixEntries
					INTEGER,
				dpsRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.1
		dpsIndex OBJECT-TYPE
			SYNTAX INTEGER (1..15)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 16."
			::= { dpsEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.2
		dpsTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Title of the Dialing Prefix Set (max 16 characters)."
			DEFVAL { "DPS#" }
			::= { dpsEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.3
		dpsCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Dialing Prefix Set."
			::= { dpsEntry 3 }

		
--  Country Code
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.4
		dpsCC OBJECT-TYPE
			SYNTAX DisplayString8
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:(Read Only) Country Code: The code that identifies the network in the country."
			::= { dpsEntry 4 }

		
--  National Destination Code
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.5
		dpsNDC OBJECT-TYPE
			SYNTAX DisplayString8
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:National Destination Code: Defines the national calling area or national network to which the subscriber belongs."
			::= { dpsEntry 5 }

		
--  International Prefix
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.6
		dpsInternationalPrefix OBJECT-TYPE
			SYNTAX DisplayString8
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:A digit or combination of digits used by a subscriber when making an international call. The international prefix is used to indicate that the following digits represent an international number and should be routed to an international gateway."
			::= { dpsEntry 6 }

		
--  National Prefix
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.7
		dpsNationalPrefix OBJECT-TYPE
			SYNTAX DisplayString8
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:A digit or combination of digits used by a subscriber when calling a national destination (within the country) other than that of the local area network."
			DEFVAL { "0" }
			::= { dpsEntry 7 }

		
--  HPLMN CC0
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.8
		dpsHPLMNCC0 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Assign up to 8 Country Code to the home PLMN. "
			::= { dpsEntry 8 }

		
--  HPLMN CC1
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.9
		dpsHPLMNCC1 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Assign up to 8 Country Code to the home PLMN. "
			::= { dpsEntry 9 }

		
--  HPLMN CC2
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.10
		dpsHPLMNCC2 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Assign up to 8 Country Code to the home PLMN. "
			::= { dpsEntry 10 }

		
--  HPLMN CC3
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.11
		dpsHPLMNCC3 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Assign up to 8 Country Code to the home PLMN. "
			::= { dpsEntry 11 }

		
--  HPLMN CC4
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.12
		dpsHPLMNCC4 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Assign up to 8 Country Code to the home PLMN. "
			::= { dpsEntry 12 }

		
--  HPLMN CC5
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.13
		dpsHPLMNCC5 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Assign up to 8 Country Code to the home PLMN. "
			::= { dpsEntry 13 }

		
--  HPLMN CC6
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.14
		dpsHPLMNCC6 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Assign up to 8 Country Code to the home PLMN. "
			::= { dpsEntry 14 }

		
--  HPLMN CC7
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.15
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.15
		dpsHPLMNCC7 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Assign up to 8 Country Code to the home PLMN. "
			::= { dpsEntry 15 }

		
--  Dialing Prefix
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.16
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.16
		dpsCreateEntrydDalingPrefix OBJECT-TYPE
			SYNTAX INTEGER { create(1) }
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { dpsEntry 16 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.17
		dpsDialingPrefixEntries OBJECT-TYPE
			SYNTAX INTEGER (0..1024)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:The total number of the configured Dialing Prefixes in this Dialing Prefix Set."
			::= { dpsEntry 17 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.1.1.17
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.18
		dpsRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { dpsEntry 18 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.2.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2
		dpTable OBJECT-TYPE
			SYNTAX SEQUENCE OF DpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { dialingPrefixSet 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.2.3.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1
		dpEntry OBJECT-TYPE
			SYNTAX DpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { dpIndex, dpDPSIndex }
			::= { dpTable 1 }

		
		DpEntry ::=
			SEQUENCE { 
				dpDPSIndex
					INTEGER,
				dpIndex
					INTEGER,
				dpTitle
					DisplayString16,
				dpCallNumberPrefix
					DisplayString16,
				dpCallNumberAttribute
					INTEGER,
				dpAdministrationState
					AdminStateChoices,
				dpCallNumberLength
					INTEGER,
				dpServiceType
					INTEGER,
				dpEmergencyType
					INTEGER,
				dpServiceKey
					INTEGER,
				dpNumberType
					INTEGER,
				dpCLIType
					INTEGER,
				dpRSC
					INTEGER,
				dpCDRFlag
					INTEGER,
				dpMNPFlag
					INTEGER,
				dpPremiumCall
					INTEGER,
				dpOSB1Flag
					INTEGER,
				dpOSB2Flag
					INTEGER,
				dpNAIForOutgoingCall
					INTEGER,
				dpPSTNNumberOfDigitDeletion
					INTEGER,
				dpPSTNInsertionNumber
					DisplayString16,
				dpE164NumberOfDigitDeletion
					INTEGER,
				dpE164InsertionNumber
					DisplayString16,
				dpRowStatus
					RowStatus
			 }

--  DP DPS Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.1
		dpDPSIndex OBJECT-TYPE
			SYNTAX INTEGER (1..15)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { dpEntry 1 }

		
--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.2
		dpIndex OBJECT-TYPE
			SYNTAX INTEGER (1..1024)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 1024."
			::= { dpEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.3
		dpTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { dpEntry 3 }

		
--  Call Number Prefix
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.4
		dpCallNumberPrefix OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:A combination digits that dial to originate a call."
			::= { dpEntry 4 }

		
--  Call Number Attribute
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.5
		dpCallNumberAttribute OBJECT-TYPE
			SYNTAX INTEGER
				{
				sub(1),
				unknown(2),
				ndd(3),
				idd(4),
				UKSpecific(126)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:The original type of the incoming number. It is specified by originating node for terminating node to route this call with proper dialed number manipulation."
			::= { dpEntry 5 }

		
--  Administration State
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.6
		dpAdministrationState OBJECT-TYPE
			SYNTAX AdminStateChoices
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Enable or disable this prefix."
			::= { dpEntry 6 }

		
--  Call Number Length
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.7
		dpCallNumberLength OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The length of the dialed number. Set 0 for uncertain length. "
			DEFVAL { 0 }
			::= { dpEntry 7 }

		
--  Service Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.8
		dpServiceType OBJECT-TYPE
			SYNTAX INTEGER
				{
				normalCall(0),
				emergencyCall(1),
				intelligentCall(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Service type of the outgoing call."
			DEFVAL { normalCall }
			::= { dpEntry 8 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.9
		dpEmergencyType OBJECT-TYPE
			SYNTAX INTEGER
				{
				zero(0),
				one(1),
				two(2),
				three(3),
				four(4),
				five(5),
				six(6),
				seven(7)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			DEFVAL { zero }
			::= { dpEntry 9 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.10
		dpServiceKey OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { dpEntry 10 }

		
--  Number Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.11
		dpNumberType OBJECT-TYPE
			SYNTAX INTEGER
				{
				msisdn(0),
				msrn(1),
				pstn(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:It determines how the numbers are sent out."
			DEFVAL { msisdn }
			::= { dpEntry 11 }

		
--  CLI Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.12
		dpCLIType OBJECT-TYPE
			SYNTAX INTEGER
				{
				sub(0),
				ndd(1),
				idd(2),
				unknownSub(3),
				unknownNdd(4),
				unknownIdd(5)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:It determines the format of the Caller Line ID (CLI)."
			DEFVAL { ndd }
			::= { dpEntry 12 }

		
--  Routing Selection Code
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.13
		dpRSC OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Specify the Routing Selection ID to this Dialing Prefix."
			DEFVAL { 0 }
			::= { dpEntry 13 }

		
--  CDR Flag
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.14
		dpCDRFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Enable or disable the Call Detail Record generation of this prefix."
			DEFVAL { enable }
			::= { dpEntry 14 }

		
--  MNP Flag
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.15
		dpMNPFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				portableNumber(1),
				portedNumber(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Enable if this prefix relating to Mobile Number Portability service."
			DEFVAL { disable }
			::= { dpEntry 15 }

		
--  Premium Call
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.16
		dpPremiumCall OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				information(1),
				entertainment(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Enable if this prefix relating to Premium Call service."
			DEFVAL { disable }
			::= { dpEntry 16 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.17
		dpOSB1Flag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Subscribers with OSB type 1 can only make calls to this dialing prefix with Call Allow Flag enabled."
			DEFVAL { disable }
			::= { dpEntry 17 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.18
		dpOSB2Flag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Subscribers with OSB type 2 cannot make calls to this dialing prefix with Call Bar Flag enabled."
			DEFVAL { disable }
			::= { dpEntry 18 }

		
--  NAI For Outgoing Call
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.19
		dpNAIForOutgoingCall OBJECT-TYPE
			SYNTAX INTEGER
				{
				sub(1),
				unknown(2),
				ndd(3),
				idd(4),
				UKSpecific(126)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The transformed type of the incoming number, which will be routed to the associated trunk group. "
			::= { dpEntry 19 }

		
--  PSTN Number Of Digit Deletion
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.15
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.20
		dpPSTNNumberOfDigitDeletion OBJECT-TYPE
			SYNTAX INTEGER (0..16)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Number of digits to be deleted from the beginning of the dialed number."
			DEFVAL { 0 }
			::= { dpEntry 20 }

		
--  PSTN Insertion Number
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.16
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.21
		dpPSTNInsertionNumber OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Digits of the number to be added to the front of the dialed number. "
			DEFVAL { 'FFFFFFFFFFFFFFFF'h }
			::= { dpEntry 21 }

		
--  E164 Number Of Digit Deletion
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.17
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.22
		dpE164NumberOfDigitDeletion OBJECT-TYPE
			SYNTAX INTEGER (0..16)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Number of digits to be deleted from the beginning of the  incoming number."
			::= { dpEntry 22 }

		
--  E164 Insertion Number
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.18
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.23
		dpE164InsertionNumber OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Digits of the number to be added to the front of the incoming number to convert it to an international E.164 format."
			DEFVAL { 'FFFFFFFFFFFFFFFF'h }
			::= { dpEntry 23 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.2.3.1.19
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.24
		dpRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { dpEntry 24 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4
		trunkGroup OBJECT IDENTIFIER ::= { parameter 4 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1
		tgTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TgEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkGroup 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1
		tgEntry OBJECT-TYPE
			SYNTAX TgEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { tgIndex }
			::= { tgTable 1 }

		
		TgEntry ::=
			SEQUENCE { 
				tgIndex
					INTEGER,
				tgTitle
					DisplayString16,
				tgCreateTimeStamp
					TimeStamp,
				tgAdministrationState
					AdminStateChoices,
				tgOperabilityStatus
					OperStateChoices,
				tgAvailabilityStatus
					AvailStateChoices,
				tgOpc
					INTEGER,
				tgDpc
					INTEGER,
				tgNetworkIndicator
					INTEGER,
				tgProtocolType
					INTEGER,
				tgProtocolVariant
					INTEGER,
				tgCircuitSelectionMode
					INTEGER,
				tgBackoffFlag
					INTEGER,
				tgTandemRestriction
					INTEGER,
				tgCDRFlag
					INTEGER,
				tgTrunkGroupType
					INTEGER,
				tgRoutingZoneID
					INTEGER,
				tgAlternativeRoutingTrigger
					INTEGER,
				tgNFAS
					INTEGER,
				tgPrimaryLink
					INTEGER,
				tgBackupLink
					INTEGER,
				tgCreateEntryTrunk
					INTEGER,
				tgTrunkEntries
					INTEGER,
				tgRowStatus
					RowStatus,
				tgEventLog
					DisplayString
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.1
		tgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 256."
			::= { tgEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.2
		tgTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Title of the selected Trunk Group (max 16 characters)."
			DEFVAL { "TG#" }
			::= { tgEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.3
		tgCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Trunk Group."
			::= { tgEntry 3 }

		
--  Administration State
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.4
		tgAdministrationState OBJECT-TYPE
			SYNTAX AdminStateChoices
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Control the operation of the managed Trunk Group."
			::= { tgEntry 4 }

		
--  Operability Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.5
		tgOperabilityStatus OBJECT-TYPE
			SYNTAX OperStateChoices
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:(Read Only) Indicate the current Trunk Group operation is qualified by Availability Status."
			::= { tgEntry 5 }

		
--  Availability Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.6
		tgAvailabilityStatus OBJECT-TYPE
			SYNTAX AvailStateChoices
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:(Read Only) Qualify Operation State providing details about the current operational status."
			::= { tgEntry 6 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.7
		tgOpc OBJECT-TYPE
			SYNTAX INTEGER (0..16777215)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The Originating Point Code of the current TG."
			::= { tgEntry 7 }

		
--  DPC
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.8
		tgDpc OBJECT-TYPE
			SYNTAX INTEGER (0..16777215)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:The Destination Point Code of the current TG."
			::= { tgEntry 8 }

		
--  Network Indication
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.9
		tgNetworkIndicator OBJECT-TYPE
			SYNTAX INTEGER
				{
				int(0),
				intSpare(1),
				nat(2),
				natSpare(3)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Specify the Trunk Group to a network."
			DEFVAL { int }
			::= { tgEntry 9 }

		
--  Protocol Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.10
		tgProtocolType OBJECT-TYPE
			SYNTAX INTEGER
				{
				aif(0),
				isup(1),
				bicc(2),
				isdn(3)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Select the protocol type for this Trunk Group. "
			::= { tgEntry 10 }

		
--  Protocol Variant
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.11
		tgProtocolVariant OBJECT-TYPE
			SYNTAX INTEGER
				{
				itu(0),
				ansi(1),
				etsi(2),
				uk(3)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Select the protocol variant for this Trunk Group."
			DEFVAL { itu }
			::= { tgEntry 11 }

		
--  Circuit Selection Mode
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.12
		tgCircuitSelectionMode OBJECT-TYPE
			SYNTAX INTEGER
				{
				clockwise(0),
				antiClockwise(1),
				lowToHigh(128),
				highToLow(129)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Circuit selection mode of the traffic channel connections."
			DEFVAL { clockwise }
			::= { tgEntry 12 }

		
--  Backoff Flag
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.13
		tgBackoffFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Enable or disable Back Off when simultaneously select the same channel with the opposite side."
			DEFVAL { enable }
			::= { tgEntry 13 }

		
--  Tandem Restriction
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.14
		tgTandemRestriction OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Enable or disable Tandem to allow or prohibit transit calls from PSTN to PSTN via this trunk group."
			DEFVAL { enable }
			::= { tgEntry 14 }

		
--  CDR Flag
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.15
		tgCDRFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Enable or disable the Call Detail Record generation of this Trunk Group."
			DEFVAL { enable }
			::= { tgEntry 15 }

		
--  Trunk Group Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.15
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.16
		tgTrunkGroupType OBJECT-TYPE
			SYNTAX INTEGER
				{
				normal(0),
				interconnectionForMSS0(16),
				interconnectionForMSS1(17)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Application type of this Trunk Group."
			DEFVAL { normal }
			::= { tgEntry 16 }

		
--  Routing Zone ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.16
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.17
		tgRoutingZoneID OBJECT-TYPE
			SYNTAX INTEGER (0..31)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Specify the Trunk Group to a Routing Zone Set. Set 255 to apply this TG in all Routing Zone Sets."
			DEFVAL { 0 }
			::= { tgEntry 17 }

		
--  Alternative Routing Trigger
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.17
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.18
		tgAlternativeRoutingTrigger OBJECT-TYPE
			SYNTAX INTEGER (0..15)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Specify the ID of the Alternative Routing Trigger for backup purpose. "
			DEFVAL { 0 }
			::= { tgEntry 18 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.19
		tgNFAS OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgEntry 19 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.20
		tgPrimaryLink OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgEntry 20 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.21
		tgBackupLink OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgEntry 21 }

		
--  Trunk
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.18
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.22
		tgCreateEntryTrunk OBJECT-TYPE
			SYNTAX INTEGER { create(1) }
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { tgEntry 22 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.23
		tgTrunkEntries OBJECT-TYPE
			SYNTAX INTEGER (0..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:The total number of configured Trunks in this Trunk Group."
			::= { tgEntry 23 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.1.1.19
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.24
		tgRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tgEntry 24 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.25
		tgEventLog OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS accessible-for-notify
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgEntry 25 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2
		trunkTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkGroup 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.2.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1
		trunkEntry OBJECT-TYPE
			SYNTAX TrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { trunkIndex, trunkTgIndex }
			::= { trunkTable 1 }

		
		TrunkEntry ::=
			SEQUENCE { 
				trunkTgIndex
					INTEGER,
				trunkIndex
					INTEGER,
				trunkTitle
					DisplayString16,
				trunkCreateTimeStamp
					TimeStamp,
				trunkAdministrationState
					AdminStateChoices,
				trunkOperabilityStatus
					OperStateChoices,
				trunkAvailabilityStatus
					AvailStateChoices,
				trunkMgID
					INTEGER,
				trunkPortID
					INTEGER,
				trunkPortType
					INTEGER,
				trunkGroupID
					INTEGER,
				trunkSupervisionMethod
					INTEGER,
				trunkLinkID
					INTEGER,
				trunkUserNetworkInterface
					INTEGER,
				trunkCICValueAssignment
					INTEGER,
				trunkChannelInUse
					INTEGER,
				trunkTimeSlotEntries
					INTEGER,
				trunkRowStatus
					RowStatus
			 }

--  Trunk TG Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.1
		trunkTgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..255)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { trunkEntry 1 }

		
--  Trunk Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.2
		trunkIndex OBJECT-TYPE
			SYNTAX INTEGER (1..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 32."
			::= { trunkEntry 2 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.3
		trunkTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Title of the selected Trunk (max 16 characters)."
			DEFVAL { "TK#" }
			::= { trunkEntry 3 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.4
		trunkCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Trunk"
			::= { trunkEntry 4 }

		
--  Administration State
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.5
		trunkAdministrationState OBJECT-TYPE
			SYNTAX AdminStateChoices
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Control the operation of the managed Trunk."
			::= { trunkEntry 5 }

		
--  Operability Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.6
		trunkOperabilityStatus OBJECT-TYPE
			SYNTAX OperStateChoices
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:(Read Only) Indicate the current linkset operation is qualified by Availability Status."
			::= { trunkEntry 6 }

		
--  Availability Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.7
		trunkAvailabilityStatus OBJECT-TYPE
			SYNTAX AvailStateChoices
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:(Read Only) Qualify Operation State providing details about the current operational status."
			::= { trunkEntry 7 }

		
--  MG ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.8
		trunkMgID OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Specify the Trunk to a Media Gateway. Not applicable to virtual MG."
			DEFVAL { 0 }
			::= { trunkEntry 8 }

		
--  Port ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.9
		trunkPortID OBJECT-TYPE
			SYNTAX INTEGER (0..31)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Specify the Trunk to a physical port of the selected Media Gateway. Not applicable to virtual MG."
			::= { trunkEntry 9 }

		
--  Port Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.10
		trunkPortType OBJECT-TYPE
			SYNTAX INTEGER
				{
				e1(0),
				t1(1),
				analogue(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Specify the type of MG physical ports."
			DEFVAL { enable }
			::= { trunkEntry 10 }

		
--  Group ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.11
		trunkGroupID OBJECT-TYPE
			SYNTAX INTEGER
				{
				group0(0),
				group1(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Select the application group of the Trunk for redundancy backup."
			DEFVAL { group0 }
			::= { trunkEntry 11 }

		
--  Typical CIC Assignment Plan
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.12
		trunkSupervisionMethod OBJECT-TYPE
			SYNTAX INTEGER
				{
				circuitGroup(0),
				circuit(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Select a mode for the Circuit Identity Code assignment of this Trunk."
			DEFVAL { enable }
			::= { trunkEntry 12 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.13
		trunkLinkID OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkEntry 13 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.14
		trunkUserNetworkInterface OBJECT-TYPE
			SYNTAX INTEGER
				{
				networkSide(0),
				userSide(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkEntry 14 }

		
--  Typical CIC Value Assignment
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.15
		trunkCICValueAssignment OBJECT-TYPE
			SYNTAX INTEGER (0..65535)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Specify the start CIC to the Trunk for typical mode."
			::= { trunkEntry 15 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.16
		trunkChannelInUse OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkEntry 16 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.17
		trunkTimeSlotEntries OBJECT-TYPE
			SYNTAX INTEGER (0..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { trunkEntry 17 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.2.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.2.1.18
		trunkRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { trunkEntry 18 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3
		tsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkGroup 3 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.3.3.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1
		tsEntry OBJECT-TYPE
			SYNTAX TsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { tsTrunkTgIndex, tsTrunkIndex, tsIndex }
			::= { tsTable 1 }

		
		TsEntry ::=
			SEQUENCE { 
				tsTrunkTgIndex
					INTEGER,
				tsTrunkIndex
					INTEGER,
				tsIndex
					INTEGER,
				tsType
					INTEGER,
				tsChannelCIC
					INTEGER,
				tsChannelStatus
					INTEGER,
				tsLocalBlock
					INTEGER,
				tsRemoteBlock
					INTEGER
			 }

--  CIC Trunk TG Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.1
		tsTrunkTgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..255)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { tsEntry 1 }

		
--  CIC Trunk Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.2
		tsTrunkIndex OBJECT-TYPE
			SYNTAX INTEGER (1..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { tsEntry 2 }

		
--  CIC Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.3
		tsIndex OBJECT-TYPE
			SYNTAX INTEGER (1..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 32."
			::= { tsEntry 3 }

		
--  CIC Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.4
		tsType OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				incoming(1),
				outgoing(2),
				bidirectional(3),
				leaseLine(4),
				dChannel(5),
				xChannel(6)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Specify the type of the channel."
			DEFVAL { bidirectiona }
			::= { tsEntry 4 }

		
--  Channel CIC
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.5
		tsChannelCIC OBJECT-TYPE
			SYNTAX INTEGER (0..65535)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Assign a Circuit Identity Code to the channel."
			::= { tsEntry 5 }

		
--  Call Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.6
		tsChannelStatus OBJECT-TYPE
			SYNTAX INTEGER
				{
				outOfService(0),
				idle(1),
				busy(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tsEntry 6 }

		
--  Local Block
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.7
		tsLocalBlock OBJECT-TYPE
			SYNTAX INTEGER
				{
				unblocked(0),
				localBlocked(1)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tsEntry 7 }

		
--  Remote Block
-- 1.3.6.1.4.1.1373.2.3.3.2.2.3.3.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.8
		tsRemoteBlock OBJECT-TYPE
			SYNTAX INTEGER
				{
				unblocked(0),
				remoteBlocked(1)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { tsEntry 8 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5
		locationArea OBJECT IDENTIFIER ::= { parameter 5 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.4.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1
		laTable OBJECT-TYPE
			SYNTAX SEQUENCE OF LaEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { locationArea 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.4.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1
		laEntry OBJECT-TYPE
			SYNTAX LaEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { laIndex }
			::= { laTable 1 }

		
		LaEntry ::=
			SEQUENCE { 
				laIndex
					INTEGER,
				laTitle
					DisplayString16,
				laCreateTimeStamp
					TimeStamp,
				laLAC
					INTEGER,
				laTrunkGroup
					INTEGER,
				laPageType
					INTEGER,
				laNumberOfRepeatPaging
					INTEGER,
				laLocalEmergencyNumber0
					DisplayString16,
				laLocalEmergencyNumber1
					DisplayString16,
				laLocalEmergencyNumber2
					DisplayString16,
				laLocalEmergencyNumber3
					DisplayString16,
				laLocalEmergencyNumber4
					DisplayString16,
				laLocalEmergencyNumber5
					DisplayString16,
				laLocalEmergencyNumber6
					DisplayString16,
				laLocalEmergencyNumber7
					DisplayString16,
				laCreateEntryCell
					INTEGER,
				laCellEntries
					INTEGER,
				laRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.1
		laIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 256."
			::= { laEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.2
		laTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Title of the selected Location Area (max 16 characters)."
			DEFVAL { "LA#" }
			::= { laEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.3
		laCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Location Area."
			::= { laEntry 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.4
		laLAC OBJECT-TYPE
			SYNTAX INTEGER (0..65535)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { laEntry 4 }

		
--  Trunk Group
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.5
		laTrunkGroup OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Specify the Trunk Group to the BSC."
			::= { laEntry 5 }

		
--  Page Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.6
		laPageType OBJECT-TYPE
			SYNTAX INTEGER
				{
				byLAC(0),
				byAllCell(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Paging messages broadcast in the specified LAC or in the whole network."
			DEFVAL { byLAC }
			::= { laEntry 6 }

		
--  Number Of Repeat Paging
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.7
		laNumberOfRepeatPaging OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Specify the subsequent paging times if the initial paging fails."
			DEFVAL { 2 }
			::= { laEntry 7 }

		
--  Local Emergency Number0
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.8
		laLocalEmergencyNumber0 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Location Area, will be transformed to this number and route to the emergency center."
			::= { laEntry 8 }

		
--  Local Emergency Number1
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.9
		laLocalEmergencyNumber1 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Location Area, will be transformed to this number and route to the emergency center."
			::= { laEntry 9 }

		
--  Local Emergency Number2
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.10
		laLocalEmergencyNumber2 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Location Area, will be transformed to this number and route to the emergency center."
			::= { laEntry 10 }

		
--  Local Emergency Number3
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.11
		laLocalEmergencyNumber3 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Location Area, will be transformed to this number and route to the emergency center."
			::= { laEntry 11 }

		
--  Local Emergency Number4
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.12
		laLocalEmergencyNumber4 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Location Area, will be transformed to this number and route to the emergency center."
			::= { laEntry 12 }

		
--  Local Emergency Number5
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.13
		laLocalEmergencyNumber5 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Location Area, will be transformed to this number and route to the emergency center."
			::= { laEntry 13 }

		
--  Local Emergency Number6
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.14
		laLocalEmergencyNumber6 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Location Area, will be transformed to this number and route to the emergency center."
			::= { laEntry 14 }

		
--  Local Emergency Number7
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.15
		laLocalEmergencyNumber7 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Location Area, will be transformed to this number and route to the emergency center."
			::= { laEntry 15 }

		
--  Cell
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.15
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.16
		laCreateEntryCell OBJECT-TYPE
			SYNTAX INTEGER { create(1) }
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION			" "
			::= { laEntry 16 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.17
		laCellEntries OBJECT-TYPE
			SYNTAX INTEGER (0..16)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:The total number of configured Cells in this LAC."
			::= { laEntry 17 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.1.1.16
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.18
		laRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { laEntry 18 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.4.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2
		cellTable OBJECT-TYPE
			SYNTAX SEQUENCE OF CellEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { locationArea 2 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.4.3.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1
		cellEntry OBJECT-TYPE
			SYNTAX CellEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { cellLaIndex, cellIndex }
			::= { cellTable 1 }

		
		CellEntry ::=
			SEQUENCE { 
				cellLaIndex
					INTEGER,
				cellIndex
					INTEGER,
				cellTitle
					DisplayString16,
				cellCreateTimeStamp
					TimeStamp,
				cellRoutingZoneID
					INTEGER,
				cellRegionalSubscriptionZoneCode
					INTEGER,
				cellID
					INTEGER,
				cellLocalEmergencyNumber0
					DisplayString16,
				cellLocalEmergencyNumber1
					DisplayString16,
				cellLocalEmergencyNumber2
					DisplayString16,
				cellLocalEmergencyNumber3
					DisplayString16,
				cellLocalEmergencyNumber4
					DisplayString16,
				cellLocalEmergencyNumber5
					DisplayString16,
				cellLocalEmergencyNumber6
					DisplayString16,
				cellLocalEmergencyNumber7
					DisplayString16,
				cellRowStatus
					RowStatus
			 }

--  Cell Location Area Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.1
		cellLaIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION			" "
			::= { cellEntry 1 }

		
--  Cell Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.2
		cellIndex OBJECT-TYPE
			SYNTAX INTEGER (1..16)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 16."
			::= { cellEntry 2 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.3
		cellTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Title of the selected Cell (max 16 characters)."
			DEFVAL { "CELL#" }
			::= { cellEntry 3 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.4
		cellCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Cell."
			::= { cellEntry 4 }

		
--  Rounting Zone ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.5
		cellRoutingZoneID OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Specify the Routing Zone Set ID to this Cell."
			DEFVAL { 0 }
			::= { cellEntry 5 }

		
--  Regional Subscription Zone Code
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.6
		cellRegionalSubscriptionZoneCode OBJECT-TYPE
			SYNTAX INTEGER (0..65535)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Assign a regional subscription zone code to the LAC. Regional Subscription Code = CC+NDC+Zone Code."
			DEFVAL { 'FF'h }
			::= { cellEntry 6 }

		
--  Cell ID
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.7
		cellID OBJECT-TYPE
			SYNTAX INTEGER (0..65535)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Global Cell Identity defined in GSM 03.03."
			::= { cellEntry 7 }

		
--  Cell Local Emergency Number0
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.8
		cellLocalEmergencyNumber0 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Cell, will be transformed to this number and route to the emergency center."
			::= { cellEntry 8 }

		
--  Cell Local Emergency Number1
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.9
		cellLocalEmergencyNumber1 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Cell, will be transformed to this number and route to the emergency center."
			::= { cellEntry 9 }

		
--  Cell Local Emergency Number2
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.10
		cellLocalEmergencyNumber2 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Cell, will be transformed to this number and route to the emergency center."
			::= { cellEntry 10 }

		
--  Cell Local Emergency Number3
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.11
		cellLocalEmergencyNumber3 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Cell, will be transformed to this number and route to the emergency center."
			::= { cellEntry 11 }

		
--  Cell Local Emergency Number4
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.12
		cellLocalEmergencyNumber4 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Cell, will be transformed to this number and route to the emergency center."
			::= { cellEntry 12 }

		
--  Cell Local Emergency Number5
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.13
		cellLocalEmergencyNumber5 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Cell, will be transformed to this number and route to the emergency center."
			::= { cellEntry 13 }

		
--  Cell Local Emergency Number6
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.14
		cellLocalEmergencyNumber6 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Cell, will be transformed to this number and route to the emergency center."
			::= { cellEntry 14 }

		
--  Cell Local Emergency Number7
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.15
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.15
		cellLocalEmergencyNumber7 OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The emergency number, which subscriber dialed in the specific Cell, will be transformed to this number and route to the emergency center."
			::= { cellEntry 15 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.4.3.1.16
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.2.1.16
		cellRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { cellEntry 16 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6
		mediaGateway OBJECT IDENTIFIER ::= { parameter 6 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.5.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1
		mgTable OBJECT-TYPE
			SYNTAX SEQUENCE OF MgEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { mediaGateway 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.5.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1
		mgEntry OBJECT-TYPE
			SYNTAX MgEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { mgIndex }
			::= { mgTable 1 }

		
		MgEntry ::=
			SEQUENCE { 
				mgIndex
					INTEGER,
				mgTitle
					DisplayString16,
				mgCreateTimeStamp
					TimeStamp,
				mgAdministrationState
					AdminStateChoices,
				mgIp
					IpAddress,
				mgDomainName
					DisplayString16,
				mgSwitchingMode
					INTEGER,
				mgEndPoint
					INTEGER,
				mgToneGenCapability
					INTEGER,
				mgType
					INTEGER,
				mgMaxPhysicalPorts
					INTEGER,
				mgMaxChannels
					INTEGER,
				mgPacketizationPeriod
					INTEGER,
				mgPriorityLevel
					INTEGER,
				mgCodecType
					Opaque,
				mgAuditTimer
					INTEGER,
				mgPhysicalPortEntries
					INTEGER,
				mgRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.1
		mgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 256."
			::= { mgEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.2
		mgTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Title of the selected Media Gateway (max 16 characters)."
			DEFVAL { "MG#" }
			::= { mgEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.3
		mgCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the MG entry."
			::= { mgEntry 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.4
		mgAdministrationState OBJECT-TYPE
			SYNTAX AdminStateChoices
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Control the operation of the managed Media Gateway."
			::= { mgEntry 4 }

		
--  IP
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.5
		mgIp OBJECT-TYPE
			SYNTAX IpAddress
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:IP address of the Media Gateway or 8KE1 Card."
			::= { mgEntry 5 }

		
--  Domain Name
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.6
		mgDomainName OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Specify a domain name to the Media Gateway."
			::= { mgEntry 6 }

		
--  Switching Mode
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.7
		mgSwitchingMode OBJECT-TYPE
			SYNTAX INTEGER
				{
				mgcp(0),
				eightECP(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Select the switching mode of the specified MG."
			DEFVAL { mgcp }
			::= { mgEntry 7 }

		
--  End Point Description
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.8
		mgEndPoint OBJECT-TYPE
			SYNTAX INTEGER
				{
				structured(1),
				unStructured(2)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Specify the method of MGCP endpoint description."
			DEFVAL { structured }
			::= { mgEntry 8 }

		
--  Tone Gen Capability
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.9
		mgToneGenCapability OBJECT-TYPE
			SYNTAX INTEGER
				{
				disable(0),
				enable(1)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Enable if the Media Gateway has tone generation capability."
			DEFVAL { enable }
			::= { mgEntry 9 }

		
--  MG Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.10
		mgType OBJECT-TYPE
			SYNTAX INTEGER
				{
				audioCodes(1),
				lgcMG(2),
				lgcCS(3),
				ipBSS(4),
				analogLine(11),
				announcementServer(21),
				interactiveVoiceResponse(31),
				conferenceBridge(41),
				packetRelay(51),
				wiretap(61),
				atm(71)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Select the type of MG endpoint."
			DEFVAL { digitalChannel }
			::= { mgEntry 10 }

		
--  Max Physical Ports
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.11
		mgMaxPhysicalPorts OBJECT-TYPE
			SYNTAX INTEGER (0..32)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The total physical port number of the MG. Not applicable to virtual MG."
			::= { mgEntry 11 }

		
--  Max Channels
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.11
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.12
		mgMaxChannels OBJECT-TYPE
			SYNTAX INTEGER (0..1024)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The total channel number of the virtual MG. Applicable to virtual MG only."
			::= { mgEntry 12 }

		
--  Packetization Period
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.12
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.13
		mgPacketizationPeriod OBJECT-TYPE
			SYNTAX INTEGER
				{
				x20ms(20),
				x40ms(40),
				x60ms(60),
				x80ms(80)
				}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:The period over which encoded voice bits are collected for encapsulation in."
			DEFVAL { x20ms }
			::= { mgEntry 13 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.14
		mgPriorityLevel OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:Set the priority level of the MG codec table. Specify priority level as an integer between from 0 and 255. Use 0 to indicate the lowest priority and 255 to indicate the highest priority."
			::= { mgEntry 14 }

		
--  Codec Type
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.13
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.15
		mgCodecType OBJECT-TYPE
			SYNTAX Opaque (SIZE (16))
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"OPAQUE DECODE RULE:
				[unit]Codec 0[u]00.0-00.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 1[u]01.0-01.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 2[u]02.0-02.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 3[u]03.0-03.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 4[u]04.0-04.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 5[u]05.0-05.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 6[u]06.0-06.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 7[u]07.0-07.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 8[u]08.0-08.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 9[u]09.0-09.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 10[u]10.0-10.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 11[u]11.0-11.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 12[u]12.0-12.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 13[u]13.0-13.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 14[u]14.0-14.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL
				[unit]Codec 15[u]15.0-15.7[u]select
				[v]0[opt]aLaw
				[v]1[opt]uLaw
				[v]2[opt]FR
				[v]3[opt]EFR
				[v]5[opt]G729b
				[v]255[opt]NULL"
			::= { mgEntry 15 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.16
		mgAuditTimer OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { mgEntry 16 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.17
		mgPhysicalPortEntries OBJECT-TYPE
			SYNTAX INTEGER (0..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:The total number of the configured Physical Ports in this Media Gateway."
			::= { mgEntry 17 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.5.1.1.14
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.1.1.18
		mgRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { mgEntry 18 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2
		ppTable OBJECT-TYPE
			SYNTAX SEQUENCE OF PpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { mediaGateway 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1
		ppEntry OBJECT-TYPE
			SYNTAX PpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { ppMgIndex, ppIndex }
			::= { ppTable 1 }

		
		PpEntry ::=
			SEQUENCE { 
				ppMgIndex
					INTEGER,
				ppIndex
					INTEGER,
				ppUsedFlag
					INTEGER,
				ppStatus
					INTEGER
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.1
		ppMgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..255)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { ppEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.2
		ppIndex OBJECT-TYPE
			SYNTAX INTEGER (1..32)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 32."
			::= { ppEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.3
		ppUsedFlag OBJECT-TYPE
			SYNTAX INTEGER
				{
				idle(0),
				inUse(1)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { ppEntry 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.6.2.1.4
		ppStatus OBJECT-TYPE
			SYNTAX INTEGER
				{
				notReady(0),
				ready(1)
				}
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { ppEntry 4 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8
		leaseCircuitStaticConnection OBJECT IDENTIFIER ::= { parameter 8 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.8.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1
		lcscTable OBJECT-TYPE
			SYNTAX SEQUENCE OF LcscEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { leaseCircuitStaticConnection 1 }

		
--  1.3.6.1.4.1.1373.1.3.3.2.2.8.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1
		lcscEntry OBJECT-TYPE
			SYNTAX LcscEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { lcscIndex }
			::= { lcscTable 1 }

		
		LcscEntry ::=
			SEQUENCE { 
				lcscIndex
					INTEGER,
				lcscTitle
					DisplayString16,
				lcscCreateTimeStamp
					TimeStamp,
				lcscOMG
					INTEGER,
				lcscOTrunk
					INTEGER,
				lcscOChannel
					INTEGER,
				lcscDMG
					INTEGER,
				lcscDTrunk
					INTEGER,
				lcscDChannel
					INTEGER,
				lcscRowStatus
					RowStatus
			 }

--  Index
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.1
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.1
		lcscIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Index number range from 1 to 256."
			::= { lcscEntry 1 }

		
--  Title
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.2
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.2
		lcscTitle OBJECT-TYPE
			SYNTAX DisplayString16
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Title of the selected Lease Circuit (max 16 characters)."
			DEFVAL { "LC#" }
			::= { lcscEntry 2 }

		
--  Creation Time Stamp
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.3
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.3
		lcscCreateTimeStamp OBJECT-TYPE
			SYNTAX TimeStamp
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Remark:Creation date and time of the Lease Circuit."
			::= { lcscEntry 3 }

		
--  Origination MG
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.4
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.4
		lcscOMG OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:ID of the originating Media Gateway."
			::= { lcscEntry 4 }

		
--  Origination Trunk
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.5
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.5
		lcscOTrunk OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Trunk ID of the originating Media Gateway."
			::= { lcscEntry 5 }

		
--  Origination Channel
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.6
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.6
		lcscOChannel OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Channel ID of the originating Trunk."
			::= { lcscEntry 6 }

		
--  Destination MG
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.7
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.7
		lcscDMG OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Remark:ID of the destination Media Gateway."
			::= { lcscEntry 7 }

		
--  Destination Trunk
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.8
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.8
		lcscDTrunk OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Trunk ID of the destination Media Gateway."
			::= { lcscEntry 8 }

		
--  Destination Channel
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.9
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.9
		lcscDChannel OBJECT-TYPE
			SYNTAX INTEGER (0..255)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes
				Remark:Channel ID of the destination Trunk."
			::= { lcscEntry 9 }

		
--  Row Status
-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.10
		-- 1.3.6.1.4.1.1373.2.3.3.2.2.8.1.1.10
		lcscRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Key Parameter:Yes"
			::= { lcscEntry 10 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3
		csta OBJECT IDENTIFIER ::= { msc 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.3
		tgIncomingTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TgIncomingEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.3.1
		tgIncomingEntry OBJECT-TYPE
			SYNTAX TgIncomingEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { tgIncomingTgndex, tgIncomingIndex }
			::= { tgIncomingTable 1 }

		
		TgIncomingEntry ::=
			SEQUENCE { 
				tgIncomingTgndex
					INTEGER,
				tgIncomingIndex
					INTEGER,
				tgIncomingData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.3.1.1
		tgIncomingTgndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgIncomingEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.3.1.2
		tgIncomingIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgIncomingEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.3.1.3
		tgIncomingData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgIncomingEntry 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.4
		tgOutgoingTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TgOutgoingEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 4 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.4.1
		tgOutgoingEntry OBJECT-TYPE
			SYNTAX TgOutgoingEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { tgOutgoingTgIndex, tgOutgoingIndex }
			::= { tgOutgoingTable 1 }

		
		TgOutgoingEntry ::=
			SEQUENCE { 
				tgOutgoingTgIndex
					INTEGER,
				tgOutgoingIndex
					INTEGER,
				tgOutgoingData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.4.1.1
		tgOutgoingTgIndex OBJECT-TYPE
			SYNTAX INTEGER (1..256)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgOutgoingEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.4.1.2
		tgOutgoingIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgOutgoingEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.4.1.3
		tgOutgoingData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { tgOutgoingEntry 3 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.5
		subsToSubsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF SubsToSubsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 5 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.5.1
		subsToSubsEntry OBJECT-TYPE
			SYNTAX SubsToSubsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { subsToSubsIndex }
			::= { subsToSubsTable 1 }

		
		SubsToSubsEntry ::=
			SEQUENCE { 
				subsToSubsIndex
					INTEGER,
				subsToSubsData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.5.1.1
		subsToSubsIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToSubsEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.5.1.2
		subsToSubsData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToSubsEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.6
		subsToTrunkTable OBJECT-TYPE
			SYNTAX SEQUENCE OF SubsToTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 6 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.6.1
		subsToTrunkEntry OBJECT-TYPE
			SYNTAX SubsToTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { subsToTrunkIndex }
			::= { subsToTrunkTable 1 }

		
		SubsToTrunkEntry ::=
			SEQUENCE { 
				subsToTrunkIndex
					INTEGER,
				subsToTrunkData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.6.1.1
		subsToTrunkIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToTrunkEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.6.1.2
		subsToTrunkData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToTrunkEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.7
		trunkToSubsTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TrunkToSubsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 7 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.7.1
		trunkToSubsEntry OBJECT-TYPE
			SYNTAX TrunkToSubsEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { trunkToSubsIndex }
			::= { trunkToSubsTable 1 }

		
		TrunkToSubsEntry ::=
			SEQUENCE { 
				trunkToSubsIndex
					INTEGER,
				trunkToSubsData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.7.1.1
		trunkToSubsIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToSubsEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.7.1.2
		trunkToSubsData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToSubsEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.8
		trunkToTrunkTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TrunkToTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 8 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.8.1
		trunkToTrunkEntry OBJECT-TYPE
			SYNTAX TrunkToTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { trunkToTrunkIndex }
			::= { trunkToTrunkTable 1 }

		
		TrunkToTrunkEntry ::=
			SEQUENCE { 
				trunkToTrunkIndex
					INTEGER,
				trunkToTrunkData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.8.1.1
		trunkToTrunkIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToTrunkEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.8.1.2
		trunkToTrunkData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToTrunkEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.9
		intraconnectionTable OBJECT-TYPE
			SYNTAX SEQUENCE OF IntraconnectionEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 9 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.9.1
		intraconnectionEntry OBJECT-TYPE
			SYNTAX IntraconnectionEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { intraconnectionIndex }
			::= { intraconnectionTable 1 }

		
		IntraconnectionEntry ::=
			SEQUENCE { 
				intraconnectionIndex
					INTEGER,
				intraconnectionData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.9.1.1
		intraconnectionIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { intraconnectionEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.9.1.2
		intraconnectionData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { intraconnectionEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.10
		subsToIpTable OBJECT-TYPE
			SYNTAX SEQUENCE OF SubsToIpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 10 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.10.1
		subsToIpEntry OBJECT-TYPE
			SYNTAX SubsToIpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { subsToIpIndex }
			::= { subsToIpTable 1 }

		
		SubsToIpEntry ::=
			SEQUENCE { 
				subsToIpIndex
					INTEGER,
				subsToIpData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.10.1.1
		subsToIpIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToIpEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.10.1.2
		subsToIpData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { subsToIpEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.11
		trunkToIpTable OBJECT-TYPE
			SYNTAX SEQUENCE OF TrunkToIpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 11 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.11.1
		trunkToIpEntry OBJECT-TYPE
			SYNTAX TrunkToIpEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { trunkToIpIndex }
			::= { trunkToIpTable 1 }

		
		TrunkToIpEntry ::=
			SEQUENCE { 
				trunkToIpIndex
					INTEGER,
				trunkToIpData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.11.1.1
		trunkToIpIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToIpEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.11.1.2
		trunkToIpData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { trunkToIpEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.12
		mobileOriginatedTable OBJECT-TYPE
			SYNTAX SEQUENCE OF MobileOriginatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 12 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.12.1
		mobileOriginatedEntry OBJECT-TYPE
			SYNTAX MobileOriginatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { mobileOriginatedIndex }
			::= { mobileOriginatedTable 1 }

		
		MobileOriginatedEntry ::=
			SEQUENCE { 
				mobileOriginatedIndex
					INTEGER,
				mobileOriginatedData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.12.1.1
		mobileOriginatedIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { mobileOriginatedEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.12.1.2
		mobileOriginatedData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { mobileOriginatedEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.13
		mobileTerminatedTable OBJECT-TYPE
			SYNTAX SEQUENCE OF MobileTerminatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 13 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.13.1
		mobileTerminatedEntry OBJECT-TYPE
			SYNTAX MobileTerminatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { mobileTerminatedIndex }
			::= { mobileTerminatedTable 1 }

		
		MobileTerminatedEntry ::=
			SEQUENCE { 
				mobileTerminatedIndex
					INTEGER,
				mobileTermiginatedData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.13.1.1
		mobileTerminatedIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { mobileTerminatedEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.13.1.2
		mobileTermiginatedData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { mobileTerminatedEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.14
		inTrunkTable OBJECT-TYPE
			SYNTAX SEQUENCE OF InTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 14 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.14.1
		inTrunkEntry OBJECT-TYPE
			SYNTAX InTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { inTrunkIndex }
			::= { inTrunkTable 1 }

		
		InTrunkEntry ::=
			SEQUENCE { 
				inTrunkIndex
					INTEGER,
				inTrunkData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.14.1.1
		inTrunkIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { inTrunkEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.14.1.2
		inTrunkData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { inTrunkEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.15
		outTrunkTable OBJECT-TYPE
			SYNTAX SEQUENCE OF OutTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 15 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.15.1
		outTrunkEntry OBJECT-TYPE
			SYNTAX OutTrunkEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { outTrunkIndex }
			::= { outTrunkTable 1 }

		
		OutTrunkEntry ::=
			SEQUENCE { 
				outTrunkIndex
					INTEGER,
				outTrunkData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.15.1.1
		outTrunkIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { outTrunkEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.15.1.2
		outTrunkData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { outTrunkEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.16
		ipTerminatedTable OBJECT-TYPE
			SYNTAX SEQUENCE OF IpTerminatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			::= { csta 16 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.16.1
		ipTerminatedEntry OBJECT-TYPE
			SYNTAX IpTerminatedEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
				"Description."
			INDEX { ipTermiginatedIndex }
			::= { ipTerminatedTable 1 }

		
		IpTerminatedEntry ::=
			SEQUENCE { 
				ipTermiginatedIndex
					INTEGER,
				ipTermiginatedData
					DisplayString
			 }

		-- 1.3.6.1.4.1.1373.2.3.3.2.3.16.1.1
		ipTermiginatedIndex OBJECT-TYPE
			SYNTAX INTEGER (0..95)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { ipTerminatedEntry 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.3.16.1.2
		ipTermiginatedData OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Description."
			::= { ipTerminatedEntry 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.4
		cdr OBJECT IDENTIFIER ::= { msc 4 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.4.1
		cdrHeadOid OBJECT-TYPE
			SYNTAX INTEGER
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { cdr 1 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.4.2
		cdrTailOid OBJECT-TYPE
			SYNTAX INTEGER
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { cdr 2 }

		
		-- 1.3.6.1.4.1.1373.2.3.3.2.4.3
		cdrDataOid OBJECT-TYPE
			SYNTAX DisplayString
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
				"Description."
			::= { cdr 3 }

		
	
	END

--
-- LGC-SS-MSC-MIB-R91-official-080825.my
--
