[para]0[Name]IMEI
[sqlName]imei[t]input[unit]IMEI[u]00.0-07.7[u]
[v]keepHex-high-0
[remark]
International mobile station equipment identity and software version Number (IMEISV), as defined in TS GSM 03.03, is a 16-digit decimal number composed of four distinct elements:
- 6-digit Type Approval Code (TAC)
- 2-digit Final Assembly Code (FAC)
- 6-digit Serial Number (SNR)
- 2-digit Software Version Number (SVN)

[para]1[Name]Service status
[sqlName]status[t]radio[unit]Service status[u]00.0-00.7[u]
[v]1[opt]BlackListed
[v]2[opt]GreyListed
[remark]
The ME has the following three states:
White list: It is composed of all number series of equipment identities that are permitted for use
Black list: It contains all equipment identities that belong to equipment that need to be barred
Grey list: Equipments on the grey list are not barred (unless on the black list or not on the white list), but are tracked by the network for evaluation or other purposes
The EIR only store the MEs that has the Blacklisted or Greylisted state, the Whitelisted MEs are defined by the system parameter. 1=BlackListed, 2=GreyListed.