[para]0[Name]IMSI
[sqlName]imsi[t]input[unit]IMSI[u]00.0-07.7[u]
[v]keepAsc-low-E
[remark]
IMSI=MCC+MNC+MSIN
MCC=mobile country code, MNC=mobile network code, MSIN=mobile subscriber identity number.

[para]1[Name]IMSI flag
[sqlName]used_flag[t]radio[unit]IMSI flag[u]00.0-00.7[u]
[v]0[opt]Disable
[v]1[opt]Enable
[remark]
Enable or disable IMSI.Disable means all services turned off.

[para]2[Name]Network access mode
[sqlName]nam[t]select[unit]Network access mode[u]00.0-00.7[u]
[v]0[opt]Both
[v]1[opt]Non-GPRS only
[v]2[opt]GPRS Only
[remark]
Define what kind of network supported.

[para]3[Name]MSISDN
[sqlName]inter_msisdn[t]input[unit]MSISDN[u]00.0-08.7[u]code
[v]keepHex-low-E
[remark]
Mobile station international ISDN number, MSISDN=CC+NDC+SN.CC=country code, NDC=national domestic code, SN=subscriber phone number.

[para]4[Name]Fax number
[sqlName]fax_num[t]input[unit]Fax number[u]00.0-08.7[u]code
[v]keepHex-low-E
[remark]
ISDN number plan + ISDN number.ISDN=CC+NDC+SN=subscriber phone number.CC=country code, NDC=national domestic code.

[para]5[Name]Data number
[sqlName]data_num[t]input[unit]Data number[u]00.0-08.7[u]code
[v]keepHex-low-E
[remark]
ISDN number plan + ISDN number.ISDN=CC+NDC+SN=subscriber phone number.CC=country code, NDC=national domestic code.

[para]6[Name]Calling Category attributes
[sqlName]category[t]select[unit]Category[u]00.0-00.7[u]
[v]0[opt]Unknown
[v]1[opt]French language
[v]2[opt]English language
[v]3[opt]German language
[v]4[opt]Russian language
[v]5[opt]Spanish language
[v]10[opt]Ordinary
[v]11[opt]subscriber with priory
[remark]
Calling party defined in ISUP. Default is Ordinary.

[para]7[Name]ODB status
[sqlName]sub_status[t]select[unit]ODB status[u]00.0-00.7[u]
[v]0[opt]Service granted
[v]1[opt]Operator determined barring
[remark]A flag indicating whether a subscriber is subject to operator determined barring.Default is service granted.

[para]8[Name]ODB general data
[sqlName]odb_general[t]checkbox[unit]BAOC[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BOIC[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BOIC-HPLMN[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BPRIC[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BPREC[u]00.4-00.4[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BASS[u]00.5-00.5[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BAIC[u]02.0-02.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BAIC-ROAM[u]02.1-02.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Roaming[u]02.3-02.3[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Roaming CT[u]02.4-02.4[u]
[v]0[opt]not support
[v]1[opt]support
[remark]
BAOC (Barring of all outgoing calls).
BOIC (Barring of all outgoing international calls).
BOIC-HPLMN (ODB BOIC except those directed to home PLMN).
BPRIC (Bar of premium rate (information) call).
BPREC (Bar of premium rate (entertainment) call).
BASS (Bar of supplementary service access).
BAIC (Barring of all incoming calls).
BAIC-ROAM (ODB BAIC when roaming outside home PLMN).
Roaming (Barring of roaming outside home PLMN).
Roaming CT (Barring of roaming outside home PLMN country).

[para]9[Name]ODB specific data
[sqlName]odb_specific[t]checkbox[unit]OSB1[u]00.0-00.0[u]
[v]0[opt]Disable
[v]1[opt]Enable
[t]checkbox[unit]OSB2[u]00.1-00.1[u]
[v]0[opt]Disable
[v]1[opt]Enable
[remark]
Operator Specific Barring (OSB)

[para]10[Name]Tele service
[sqlName]tele_data[t]checkbox[unit]Telephony[u]00.0-00.0[u]
[v]0[opt]Not provide
[v]1[opt]Provide
[t]checkbox[unit]Emergency call[u]00.1-00.1[u]
[v]0[opt]Not provide
[v]1[opt]Provide
[t]checkbox[unit]Short message MT-PP[u]00.2-00.2[u]
[v]0[opt]Not provide
[v]1[opt]Provide
[t]checkbox[unit]Short message MO-PP[u]00.3-00.3[u]
[v]0[opt]Not provide
[v]1[opt]Provide
[remark]
Default=all services turn on.

[para]11[Name]RSZI List
[sqlName]rszi[t]input[unit]RSZI0[u]00.0-00.7[u]size
[v]toDec-high-0
[t]input[unit]RSZI1[u]01.0-01.7[u]size
[v]toDec-high-0
[t]input[unit]RSZI2[u]02.0-02.7[u]size
[v]toDec-high-0
[t]input[unit]RSZI3[u]03.0-03.7[u]size
[v]toDec-high-0
[t]input[unit]RSZI4[u]04.0-04.7[u]size
[v]toDec-high-0
[t]input[unit]RSZI5[u]05.0-05.7[u]size
[v]toDec-high-0
[t]input[unit]RSZI6[u]06.0-06.7[u]size
[v]toDec-high-0
[t]input[unit]RSZI7[u]07.0-07.7[u]size
[v]toDec-high-0
[t]input[unit]RSZI8[u]08.0-08.7[u]size
[v]toDec-high-0
[t]input[unit]RSZI9[u]09.0-09.7[u]size
[v]toDec-high-0
[remark]
Regional subscriptiong zone identity list. A PLMN specific regional subscription defines unambiguously for the entire PLMN the region in which roaming is allowed.

[para]12[Name]CSRR type
[sqlName]csr_type[t]select[unit]CSRR Type[u]00.0-00.7[u]
[v]0[opt]00
[v]1[opt]01
[v]2[opt]02
[v]3[opt]03
[v]4[opt]04
[v]5[opt]05
[v]6[opt]06
[v]7[opt]07
[v]255[opt]No Restriction
[remark]
Define 8 CSRR (county specific roaming restrictions) types' attribute to confine the international roaming range of a subscriber.Each CSRR defines roaming restrictions for 256 VPLMNs.There are 8 CSRR combination types.

[para]13[Name]CLIP state
[sqlName]clip_state[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
Calling line identification presentation state, set on called party.Provisioned=Called party displays caller number (given caller party set CLIR as Not provisioned).Not provisioned=Called party does not display caller number.

[para]14[Name]BC type
[sqlName]bc_type[t]select[unit]GsmBC id for fax[u]00.0-00.3[u]
[v]0[opt]00
[v]1[opt]01
[v]2[opt]02
[v]3[opt]03
[v]4[opt]04
[v]5[opt]05
[v]6[opt]06
[v]7[opt]07
[v]8[opt]08
[v]9[opt]09
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[t]select[unit]GsmBC id for data[u]00.4-00.7[u]
[v]0[opt]00
[v]1[opt]01
[v]2[opt]02
[v]3[opt]03
[v]4[opt]04
[v]5[opt]05
[v]6[opt]06
[v]7[opt]07
[v]8[opt]08
[v]9[opt]09
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[remark]
Define 16 BC(Bearer Capability) type's attribution respectively for fax's and data's  GsmBC id.

[para]15[Name]CLIR state
[sqlName]clir_state[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
Calling line identification restriction state, set on caller party.Provisioned=called party does not display caller number.Not provisioned=caller party displays caller number (given called party set CLIP as Provisioned).

[para]16[Name]COLP state
[sqlName]colp_state[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
Connected line identification presentation state, set on caller party.Provisioned=caller party displays called number including forwarded number (given called party set COLR as Not provsioned).Not provisioned=caller party does not display called number.

[para]17[Name]COLR state
[sqlName]colr_state[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent state[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
Connected line identification restriction state, set on called party.Provisioned=caller party does not display called number.Not provisioned=caller party displays called number (given caller party set COLP as provisioned).

[para]18[Name]Call barring subscription
[sqlName]subs_option[t]select[unit]CB subscription option[u]00.0-00.7[u]
[v]0[opt]Service provider
[v]1[opt]Subscriber using password
[v]2[opt]Subscriber not using password
[remark]
Define call barring service subscription mode for all call barring.

[para]19[Name]Call Barring password
[sqlName]passwd[t]input[unit]SS call barring password[u]00.0-03.7[u]
[v]keepAsc-low-0
[remark]
used for all call barring. Only use digit '0'-'9'.

[para]20[Name]BAOC state
[sqlName]baoc_state[t]checkbox[unit]Active[u]00.0-00.0[u]
[v]0[opt]Not active
[v]1[opt]Active
[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
Barring of all outgoing calls.

[para]21[Name]BOIC state
[sqlName]boic_state[t]checkbox[unit]Active[u]00.0-00.0[u]
[v]0[opt]Not active
[v]1[opt]Active
[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
Barring of all outgoing international calls.

[para]22[Name]BOIC-HPLMN state
[sqlName]boichc_state[t]checkbox[unit]Active[u]00.0-00.0[u]
[v]0[opt]Not active
[v]1[opt]Active
[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
BOIC except directed to home HPLMN.

[para]23[Name]BAIC state
[sqlName]baic_state[t]checkbox[unit]Active[u]00.0-00.0[u]
[v]0[opt]Not active
[v]1[opt]Active
[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
Barring of all incoming calls.

[para]24[Name]BIC ROAM state
[sqlName]bicroam_state[t]checkbox[unit]Active[u]00.0-00.0[u]
[v]0[opt]Not active
[v]1[opt]Active
[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
BIC when roaming outside home PLMN.

[para]25[Name]CFU
[sqlName]cfu_state[t]checkbox[unit]Active[u]00.0-00.0[u]
[v]0[opt]Not active
[v]1[opt]Active
[t]checkbox[unit]Register[u]00.1-00.1[u]
[v]0[opt]Not register
[v]1[opt]Register
[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
State of call forwarding unconditional.

[para]26[Name]CFU number
[sqlName]cfu_num[t]input[unit]ISDN number plan[u]00.0-00.7[u]code
[v]keepHex-high-0
[unit]ISDN number[u]01.0-08.7[u]code
[v]keepHex-low-E
[remark]

[para]27[Name]CFB
[sqlName]cfb_state[t]checkbox[unit]Active[u]00.0-00.0[u]
[v]0[opt]Not active
[v]1[opt]Active
[t]checkbox[unit]Register[u]00.1-00.1[u]
[v]0[opt]Not register
[v]1[opt]Register
[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
State of call forwarding on mobile subscriber busy.

[para]28[Name]CFB number
[sqlName]cfb_num[t]input[unit]ISDN number plan[u]00.0-00.7[u]code
[v]keepHex-high-0
[unit]ISDN number[u]01.0-08.7[u]code
[v]keepHex-low-E
[remark]

[para]29[Name]CFNRy
[sqlName]cfnry_state[t]checkbox[unit]Active[u]00.0-00.0[u]
[v]0[opt]Not active
[v]1[opt]Active
[t]checkbox[unit]Register[u]00.1-00.1[u]
[v]0[opt]Not register
[v]1[opt]Register
[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
State of call forwarding on no reply.

[para]30[Name]CFNRy number
[sqlName]cfnry_num[t]input[unit]ISDN number plan[u]00.0-00.7[u]code
[v]keepHex-high-0
[unit]ISDN number[u]01.0-08.7[u]code
[v]keepHex-low-E
[remark]

[para]31[Name]CFNRy timer
[sqlName]cfnry_time[t]input[unit]CFNRy timer[u]00.0-00.7[u]
[v]keepHex-high-0
[remark]
Indicates "no reply condition timer", ranges from 5 to 30 seconds on a steps of 5-second.

[para]32[Name]CFNRc
[sqlName]cfnrc_state[t]checkbox[unit]Active[u]00.0-00.0[u]
[v]0[opt]Not active
[v]1[opt]Active
[t]checkbox[unit]Register[u]00.1-00.1[u]
[v]0[opt]Not register
[v]1[opt]Register
[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
State of call forwarding on mobile subscriber not reachable.

[para]33[Name]CFNRc number
[sqlName]cfnrc_num[t]input[unit]ISDN number plan[u]00.0-00.7[u]code
[v]keepHex-high-0
[unit]ISDN number[u]01.0-08.7[u]code
[v]keepHex-low-E
[remark]

[para]34[Name]Call waiting state
[sqlName]callwait_state[t]checkbox[unit]Active[u]00.0-00.0[u]
[v]0[opt]Not active
[v]1[opt]Active
[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
Call waiting stat.

[para]35[Name]Call hold state
[sqlName]callhold_state[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
Call hold state.

[para]36[Name]ECT state
[sqlName]ect_state[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
Explicit call transfer state.

[para]37[Name]Multi-party state
[sqlName]mtpy_state[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
Multi-party call state.

[para]38[Name]eMLPP State
[sqlName]emlpp_state[t]checkbox[unit]Provision[u]00.2-00.2[u]
[v]0[opt]Not provision
[v]1[opt]Provision
[t]checkbox[unit]Quiescent[u]00.3-00.3[u]
[v]0[opt]Not quiescent
[v]1[opt]Quiescent
[remark]
eMLPP State.

[para]39[Name]eMLPP Max Priority
[sqlName]emlpp_max_priority[t]select[unit]Max Priority[u]00.0-00.7[u]
[v]6[opt]Level A
[v]5[opt]Level B
[v]0[opt]Level 0
[v]1[opt]Level 1
[v]2[opt]Level 2
[v]3[opt]Level 3
[v]4[opt]Level 4
[remark]
eMLPP Max Priority

[para]40[Name]Default Priority
[sqlName]emlpp_def_priority[t]select[unit]Default Priority[u]00.0-00.7[u]
[v]6[opt]Level A
[v]5[opt]Level B
[v]0[opt]Level 0
[v]1[opt]Level 1
[v]2[opt]Level 2
[v]3[opt]Level 3
[v]4[opt]Level 4
[remark]
eMLPP Default Priority.

[para]41[Name]Camel Flag
[sqlName]camel_flag[t]checkbox[unit]CAMEL[u]00.7-00.7[u]
[v]1[opt]Supported
[v]0[opt]Not Supported
[t]checkbox[unit]O-CSI[u]01.0-01.0[u]
[v]1[opt]Provided
[v]0[opt]Not Provided
[t]checkbox[unit]T-CSI[u]01.1-01.1[u]
[v]1[opt]Provided
[v]0[opt]Not Provided
[t]checkbox[unit]SS-CSI[u]01.2-01.2[u]
[v]1[opt]Provided
[v]0[opt]Not Provided
[t]checkbox[unit]SMS-CSI[u]01.3-01.3[u]
[v]1[opt]Provided
[v]0[opt]Not Provided
[t]checkbox[unit]GPRS-CSI[u]01.4-01.4[u]
[v]1[opt]Provided
[v]0[opt]Not Provided
[remark]CAMEL service enable or disable.
Support CAMEL is a total flag of CAMEL provisioning. To enable any CAMEL service, select this option.
O-CSI: Originating CAMEL subscription information.
T-CSI: Terminating CAMEL subscription information.
SS-CSI: Supplementary service notification CAMEL subscription information.
SMS-CSI: Short message service notification CAMEL subscrition information.
GPRS-CSI: GPRS notification CAMEL subscription information.

[para]42[Name]Purge MS flag
[sqlName]purgems_flag[t]show[unit]GSM [u]00.0-00.0[u]
[v]0[opt]Online
[v]1[opt]Offline
[t]show[unit]GPRS[u]00.1-00.1[u]
[v]0[opt]Online
[v]1[opt]Offline
[remark]
Status of MS purge. Online=MS not purged. Offline=MS purged.

[para]43[Name]GPRS flag
[sqlName]gprs_flag[t]select[unit]GPRS flag[u]00.0-00.7[u]
[v]0[opt]Disable
[v]1[opt]Enable
[remark]
GPRS service flag

[para]44[Name]PDP context (group 1)
[sqlName]pdp1[t]radio[unit]PDP flag[u]00.0-00.7[u]
[v]0[opt]Disable
[v]1[opt]Enable
[t]select[unit]PDP type[u]01.0-02.7[u]
[v]289[opt]IPv4
[v]343[opt]IPv6
[v]0[opt]X.25
[t]specialInputHlr[unit]PDP address[u]04.0-19.7[u]
[v]keepHex-low-E
[t]select[unit]Reliability Class[u]20.0-20.2[u]
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[t]select[unit]Delay Class[u]20.3-20.7[u]
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[t]select[unit]Precedence Class[u]21.0-21.3[u]
[v]1[opt]High
[v]2[opt]Normal
[v]3[opt]low
[t]select[unit]Peak Throughput[u]21.4-21.7[u]
[v]1[opt]8Kbps
[v]2[opt]16Kbps
[v]3[opt]32Kbps
[v]4[opt]64Kbps
[v]5[opt]128Kbps
[v]6[opt]256Kbps
[v]7[opt]512Kbps
[v]8[opt]1024Kbps
[v]9[opt]2048Kbps
[t]select[unit]Mean Throughput[u]22.0-22.7[u]
[v]1[opt]100Bph
[v]2[opt]200Bph
[v]3[opt]500Bph
[v]4[opt]1kBph
[v]5[opt]2kBph
[v]6[opt]5kBph
[v]7[opt]10kBph
[v]8[opt]20kBph
[v]9[opt]50kBph
[v]10[opt]100kBph
[v]11[opt]200kBph
[v]12[opt]500kBph
[v]13[opt]1mBph
[v]14[opt]2mBph
[v]15[opt]5mBph
[v]16[opt]10mBph
[v]17[opt]20mBph
[v]18[opt]50mBph
[v]31[opt]Best Effort
[t]radio[unit]VPLMN Address Allowed flag[u]23.0-23.7[u]
[v]0[opt]Not allowed
[v]1[opt]Allowed
[t]input[unit]APN[u]24.0-55.7[u]
[v]toAsc-low-0
[t][unit]Ext Qos
[t]select[unit]Ext Flag[u]56.0-56.7[u]
[v]0[opt]Non-included Ext
[v]1[opt]Included Ext
[v]3[opt]Included Ext and Ext2 only 1 octet
[v]7[opt]Included Ext, Ext2
[v]15[opt]Included Ext, Ext2, EXt3
[t]select[unit]Allocation/Retention Priority[u]57.0-57.7[u]
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[t]select[unit]Delivery err SDUs[u]58.0-58.2[u]
[v]1[opt]No detect
[v]2[opt]Err SDUs delilvered
[v]3[opt]Err SDUs not delivered
[v]7[opt]Reserved
[t]select[unit]Delivery order[u]58.3-58.4[u]
[v]1[opt]delivery order
[v]2[opt]no delivery order
[v]3[opt]Reserved
[t]select[unit]Traffic class[u]58.5-58.7[u]
[v]1[opt]Conversation class
[v]2[opt]Streaming class
[v]3[opt]Interactive class
[v]4[opt]Background class
[v]7[opt]Reserved
[t]select[unit]Maximum SDU size[u]59.0-59.7[u]
[v]1[opt]10 octets
[v]20[opt]200 octets
[v]80[opt]800 octets
[v]100[opt]1000 octets
[v]148[opt]1480 octets
[v]150[opt]1500 octets
[v]151[opt]1502 octets
[v]152[opt]1510 octets
[v]153[opt]1520 octets
[v]255[opt]Reserved
[t]selectlimit[unit]Maximum bit rate for uplink range(X)[u]60.0-60.5[u]range1_1
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[v]16[opt]16
[v]17[opt]17
[v]18[opt]18
[v]19[opt]19
[v]20[opt]20
[v]21[opt]21
[v]22[opt]22
[v]23[opt]23
[v]24[opt]24
[v]25[opt]25
[v]26[opt]26
[v]27[opt]27
[v]28[opt]28
[v]29[opt]29
[v]30[opt]30
[v]31[opt]31
[v]32[opt]32
[v]33[opt]33
[v]34[opt]34
[v]35[opt]35
[v]36[opt]36
[v]37[opt]37
[v]38[opt]38
[v]39[opt]39
[v]40[opt]40
[v]41[opt]41
[v]42[opt]42
[v]43[opt]43
[v]44[opt]44
[v]45[opt]45
[v]46[opt]46
[v]47[opt]47
[v]48[opt]48
[v]49[opt]49
[v]50[opt]50
[v]51[opt]51
[v]52[opt]52
[v]53[opt]53
[v]54[opt]54
[v]55[opt]55
[v]56[opt]56
[v]57[opt]57
[v]58[opt]58
[v]59[opt]59
[v]60[opt]60
[v]61[opt]61
[v]62[opt]62
[v]63[opt]63
[t]selectlimit[unit]Maximum bit rate for uplink base[u]60.6-60.7[u]base1_1
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t]selectlimit[unit]Maximum bit rate for downlink range(X)[u]61.0-61.5[u]range2_1
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[v]16[opt]16
[v]17[opt]17
[v]18[opt]18
[v]19[opt]19
[v]20[opt]20
[v]21[opt]21
[v]22[opt]22
[v]23[opt]23
[v]24[opt]24
[v]25[opt]25
[v]26[opt]26
[v]27[opt]27
[v]28[opt]28
[v]29[opt]29
[v]30[opt]30
[v]31[opt]31
[v]32[opt]32
[v]33[opt]33
[v]34[opt]34
[v]35[opt]35
[v]36[opt]36
[v]37[opt]37
[v]38[opt]38
[v]39[opt]39
[v]40[opt]40
[v]41[opt]41
[v]42[opt]42
[v]43[opt]43
[v]44[opt]44
[v]45[opt]45
[v]46[opt]46
[v]47[opt]47
[v]48[opt]48
[v]49[opt]49
[v]50[opt]50
[v]51[opt]51
[v]52[opt]52
[v]53[opt]53
[v]54[opt]54
[v]55[opt]55
[v]56[opt]56
[v]57[opt]57
[v]58[opt]58
[v]59[opt]59
[v]60[opt]60
[v]61[opt]61
[v]62[opt]62
[v]63[opt]63
[t]selectlimit[unit]Maximum bit rate for downlink base[u]61.6-61.7[u]base2_1
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t]select[unit]SDU error ratio[u]62.0-62.3[u]
[v]1[opt]1E-2
[v]2[opt]7E-3
[v]3[opt]1E-3
[v]4[opt]1E-4
[v]5[opt]1E-5
[v]6[opt]1E-6
[v]7[opt]1E-1
[v]15[opt]Reserved
[t]select[unit]Residual Bit Error Rate[u]62.4-62.7[u]
[v]1[opt]5E-2
[v]2[opt]1E-2
[v]3[opt]5E-3
[v]4[opt]4E-3
[v]5[opt]1E-3
[v]6[opt]1E-4
[v]7[opt]1E-5
[v]8[opt]1E-6
[v]9[opt]6E-8
[v]15[opt]Reserved
[t]select[unit]Traffic handing priority[u]63.0-63.1[u]
[v]1[opt]level 1
[v]2[opt]level 2
[v]3[opt]level 3
[v]0[opt]Reserved
[t]select[unit]Transfer delay[u]63.2-63.7[u]
[v]0[opt]X*10ms
[v]1[opt]200ms+X*50ms
[v]2[opt]1000ms+X*100ms
[v]3[opt]2600ms+X*100ms
[v]63[opt]Reserved
[t]selectlimit[unit]Guaranteed bit rate uplink range(X)[u]64.0-64.5[u]range3_1
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[v]16[opt]16
[v]17[opt]17
[v]18[opt]18
[v]19[opt]19
[v]20[opt]20
[v]21[opt]21
[v]22[opt]22
[v]23[opt]23
[v]24[opt]24
[v]25[opt]25
[v]26[opt]26
[v]27[opt]27
[v]28[opt]28
[v]29[opt]29
[v]30[opt]30
[v]31[opt]31
[v]32[opt]32
[v]33[opt]33
[v]34[opt]34
[v]35[opt]35
[v]36[opt]36
[v]37[opt]37
[v]38[opt]38
[v]39[opt]39
[v]40[opt]40
[v]41[opt]41
[v]42[opt]42
[v]43[opt]43
[v]44[opt]44
[v]45[opt]45
[v]46[opt]46
[v]47[opt]47
[v]48[opt]48
[v]49[opt]49
[v]50[opt]50
[v]51[opt]51
[v]52[opt]52
[v]53[opt]53
[v]54[opt]54
[v]55[opt]55
[v]56[opt]56
[v]57[opt]57
[v]58[opt]58
[v]59[opt]59
[v]60[opt]60
[v]61[opt]61
[v]62[opt]62
[v]63[opt]63
[t]selectlimit[unit]Guaranteed bit rate uplink base[u]64.6-64.7[u]base3_1
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t]selectlimit[unit]Guaranteed bit rate downlink range(X)[u]65.0-65.5[u]range4_1
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[v]16[opt]16
[v]17[opt]17
[v]18[opt]18
[v]19[opt]19
[v]20[opt]20
[v]21[opt]21
[v]22[opt]22
[v]23[opt]23
[v]24[opt]24
[v]25[opt]25
[v]26[opt]26
[v]27[opt]27
[v]28[opt]28
[v]29[opt]29
[v]30[opt]30
[v]31[opt]31
[v]32[opt]32
[v]33[opt]33
[v]34[opt]34
[v]35[opt]35
[v]36[opt]36
[v]37[opt]37
[v]38[opt]38
[v]39[opt]39
[v]40[opt]40
[v]41[opt]41
[v]42[opt]42
[v]43[opt]43
[v]44[opt]44
[v]45[opt]45
[v]46[opt]46
[v]47[opt]47
[v]48[opt]48
[v]49[opt]49
[v]50[opt]50
[v]51[opt]51
[v]52[opt]52
[v]53[opt]53
[v]54[opt]54
[v]55[opt]55
[v]56[opt]56
[v]57[opt]57
[v]58[opt]58
[v]59[opt]59
[v]60[opt]60
[v]61[opt]61
[v]62[opt]62
[v]63[opt]63
[t]selectlimit[unit]Guaranteed bit rate downlink base[u]65.6-65.7[u]base4_1
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t][unit]Ext2 Qos
[t]select[unit]Source statistics Descriptor[u]66.0-66.3[u]
[v]0[opt]Spare
[v]1[opt]Speech
[t]select[unit]Signalling Indication[u]66.4-66.4[u]
[v]0[opt]Not optimised
[v]1[opt]Optimised
[t]select[unit]Maximum bit rate downlink (ext)[u]67.0-67.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16mbps
[v]75[opt]17mbps
[v]186[opt]128mbps
[v]187[opt]130mbps
[v]250[opt]256mbps
[t]select[unit]Guaranteed bit rate downlink (ext)[u]68.0-68.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16000kbps
[v]75[opt]17Mbps
[v]186[opt]128Mbps
[v]187[opt]130Mbps
[v]250[opt]256Mbps
[t][unit]Ext3 Qos
[t]select[unit]Maximum bit rate uplink (ext)[u]69.0-69.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16000kbps
[v]75[opt]17Mbps
[v]186[opt]128Mbps
[v]187[opt]130Mbps
[v]250[opt]256Mbps
[t]select[unit]Guaranteed bit rate uplink (ext)[u]70.0-70.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16000kbps
[v]75[opt]17Mbps
[v]186[opt]128Mbps
[v]187[opt]130Mbps
[v]250[opt]256Mbps
[remark]
PDP context identifier: 1-3.
PDP Type: 0x0121 = IPv4, 0x0157 = IPv6, 0x0000 = X.25
PDP Address:
IPv4 Len = 4, <IPv4 hex address>
IPv6 Len = 16, <IPv6 hex address>
X.25 Len = 3 to 9, <X.121 address digits>
Empty AddressĄ¤ Field of any type has Len =0
Reliability Class:
1 = Error sensitive,no error correction,limited error tolerance, non real-time traffic
2 = Error sensitive, limited error correction,good error tolerance, non real-time traffic
3 = Not error sensitive, error correction capability and/or very good error tolerance capability, non real-time traffic
4 = Real-time traffic, error sensitive, cope with data loss5 = Real-time traffic, error non-sensitive, cope with data loss
Delay Class:	1 (predictive), 2 (predictive), 3 (predictive) and 4 (Best effort)
Precedence Class: 1 = High, 2 = Normal, 3 = Low
Peak Throughput	1 through 9 (8 Kbps to 2.048 Kbps)
Mean Throughput	1 through 18 (100 to 50 Million Octets per sec), and 31(Best effort)
VPLMN Address Allowed: 0 = Not Allowed, 1 = Allowed
APN:The APN field in the HLR contains either only an APN Network Identifier (i.e. an APN without APN Operator Identifier) or the wild card value (defined in GSM 03.03).Currently we only use the wild card APN "*".
Ext Flag:
0 = Non-included Ext,1 = Included Ext,3 = Included Ext and Ext2 only 1 octet,7 = Included Ext, Ext2 Qos,15 = Included Ext, Ext2, EXt3 Qos
Ext Qos
Allocation/Retention Priority:
There are four priority : Priority 1,Priority 2,Priority 3,Priority 4.
Delivery err SDUs:
1=No detect,2=Err SDUs delilvered,3=Err SDUs not delivered,7=Reserved
Delivery order:
1 =with delivery order,2 = without delivery order,3 = Reserved
Traffic class:
1=Conversation class,2=Streaming class,3=Interactive class,4=Background class,7=Reserved
Maximum SDU size:
Giving a range of values from 10 octets to 1520 octets,1=10 octets,20=200 octets,80=800 octets,100=1000 octets,148=1480 octets,150=1500 octets,151=1502 octets,152=1510 octets,153=1520 octets,255=Reserved
Maximum bit rate for uplink range:0 through 63 (0 Kbps to 63 Kbps)
Maximum bit rate for uplink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
Maximum bit rate for downlink range:0 through 63 (0 Kbps to 63 Kbps)
Maximum bit rate for downlink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
SDU error ratio:
The range is from 5E-2 to 6E-8.1=1E-2,2=7E-3,3=1E-3,4=1E-4,5=1E-5,6=1E-6,7=1E-1,15=Reserved
Residual Bit Error Rate:
The range is from 1E-1 to 1E-6.1=5E-2,2=1E-2,3=5E-3,4=4E-3,5=1E-3 6=1E-4,7=1E-5,8=1E-6,9=6E-8,15=Reserved
Traffic handing priority:
1=priority Level 1,2=priority Level 2,3=priority Level 3,0=Reserved
Transfer delay:0=X*10ms,1=200ms+X*50ms,2=1000ms+X*100ms,3=2600ms+X*100ms
Guaranteed bit rate uplink range:0 through 63 (0 Kbps to 63 Kbps)
Guaranteed bit rate uplink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
Guaranteed bit rate downlink range:0 through 63 (0 Kbps to 63 Kbps)
Guaranteed bit rate downlink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
Ext2 Qos
Source Statistics Descriptor:0=Spare,1=Speech (MS=>NW)
Signalling Indication:
0=Not Optimised for Signalling Traffic,1=Optimised for Signalling Traffic.
Reserved:66.5-66.7
Maximum bit rate downlink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)
Guaranteed bit rate downlink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)
Ext3 Qos
Maximum bit rate uplink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)
Guaranteed bit rate uplink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)

[para]45[Name]PDP context (group 2)
[sqlName]pdp2[t]radio[unit]PDP flag[u]00.0-00.7[u]
[v]0[opt]Disable
[v]1[opt]Enable
[t]select[unit]PDP type[u]01.0-02.7[u]
[v]289[opt]IPv4
[v]343[opt]IPv6
[v]0[opt]X.25
[t]specialInputHlr[unit]PDP address[u]04.0-19.7[u]
[v]keepHex-low-E
[t]select[unit]Reliability Class[u]20.0-20.2[u]
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[t]select[unit]Delay Class[u]20.3-20.7[u]
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[t]select[unit]Precedence Class[u]21.0-21.3[u]
[v]1[opt]High
[v]2[opt]Normal
[v]3[opt]low
[t]select[unit]Peak Throughput[u]21.4-21.7[u]
[v]1[opt]8Kbps
[v]2[opt]16Kbps
[v]3[opt]32Kbps
[v]4[opt]64Kbps
[v]5[opt]128Kbps
[v]6[opt]256Kbps
[v]7[opt]512Kbps
[v]8[opt]1024Kbps
[v]9[opt]2048Kbps
[t]select[unit]Mean Throughput[u]22.0-22.7[u]
[v]1[opt]100Bph
[v]2[opt]200Bph
[v]3[opt]500Bph
[v]4[opt]1kBph
[v]5[opt]2kBph
[v]6[opt]5kBph
[v]7[opt]10kBph
[v]8[opt]20kBph
[v]9[opt]50kBph
[v]10[opt]100kBph
[v]11[opt]200kBph
[v]12[opt]500kBph
[v]13[opt]1mBph
[v]14[opt]2mBph
[v]15[opt]5mBph
[v]16[opt]10mBph
[v]17[opt]20mBph
[v]18[opt]50mBph
[v]31[opt]Best Effort
[t]radio[unit]VPLMN Address Allowed flag[u]23.0-23.7[u]
[v]0[opt]Not allowed
[v]1[opt]Allowed
[t]input[unit]APN[u]24.0-55.7[u]
[v]toAsc-low-0
[t][unit]Ext Qos
[t]select[unit]Ext Flag[u]56.0-56.7[u]
[v]0[opt]Non-included Ext
[v]1[opt]Included Ext
[v]3[opt]Included Ext and Ext2 only 1 octet
[v]7[opt]Included Ext, Ext2
[v]15[opt]Included Ext, Ext2, EXt3
[t]select[unit]Allocation/Retention Priority[u]57.0-57.7[u]
[v]0[opt]Reserved
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[t]select[unit]Delivery err SDUs[u]58.0-58.2[u]
[v]1[opt]No detect
[v]2[opt]Err SDUs delilvered
[v]3[opt]Err SDUs not delivered
[v]7[opt]Reserved
[t]select[unit]Delivery order[u]58.3-58.4[u]
[v]1[opt]delivery order
[v]2[opt]no delivery order
[v]3[opt]Reserved
[t]select[unit]Traffic class[u]58.5-58.7[u]
[v]1[opt]Conversation class
[v]2[opt]Streaming class
[v]3[opt]Interactive class
[v]4[opt]Background class
[v]7[opt]Reserved
[t]select[unit]Maximum SDU size[u]59.0-59.7[u]
[v]1[opt]10 octets
[v]20[opt]200 octets
[v]80[opt]800 octets
[v]100[opt]1000 octets
[v]148[opt]1480 octets
[v]150[opt]1500 octets
[v]151[opt]1502 octets
[v]152[opt]1510 octets
[v]153[opt]1520 octets
[v]255[opt]Reserved
[t]selectlimit[unit]Maximum bit rate for uplink range(X)[u]60.0-60.5[u]range1_2
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[v]16[opt]16
[v]17[opt]17
[v]18[opt]18
[v]19[opt]19
[v]20[opt]20
[v]21[opt]21
[v]22[opt]22
[v]23[opt]23
[v]24[opt]24
[v]25[opt]25
[v]26[opt]26
[v]27[opt]27
[v]28[opt]28
[v]29[opt]29
[v]30[opt]30
[v]31[opt]31
[v]32[opt]32
[v]33[opt]33
[v]34[opt]34
[v]35[opt]35
[v]36[opt]36
[v]37[opt]37
[v]38[opt]38
[v]39[opt]39
[v]40[opt]40
[v]41[opt]41
[v]42[opt]42
[v]43[opt]43
[v]44[opt]44
[v]45[opt]45
[v]46[opt]46
[v]47[opt]47
[v]48[opt]48
[v]49[opt]49
[v]50[opt]50
[v]51[opt]51
[v]52[opt]52
[v]53[opt]53
[v]54[opt]54
[v]55[opt]55
[v]56[opt]56
[v]57[opt]57
[v]58[opt]58
[v]59[opt]59
[v]60[opt]60
[v]61[opt]61
[v]62[opt]62
[v]63[opt]63
[t]selectlimit[unit]Maximum bit rate for uplink base[u]60.6-60.7[u]base1_2
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t]selectlimit[unit]Maximum bit rate for downlink range(X)[u]61.0-61.5[u]range2_2
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[v]16[opt]16
[v]17[opt]17
[v]18[opt]18
[v]19[opt]19
[v]20[opt]20
[v]21[opt]21
[v]22[opt]22
[v]23[opt]23
[v]24[opt]24
[v]25[opt]25
[v]26[opt]26
[v]27[opt]27
[v]28[opt]28
[v]29[opt]29
[v]30[opt]30
[v]31[opt]31
[v]32[opt]32
[v]33[opt]33
[v]34[opt]34
[v]35[opt]35
[v]36[opt]36
[v]37[opt]37
[v]38[opt]38
[v]39[opt]39
[v]40[opt]40
[v]41[opt]41
[v]42[opt]42
[v]43[opt]43
[v]44[opt]44
[v]45[opt]45
[v]46[opt]46
[v]47[opt]47
[v]48[opt]48
[v]49[opt]49
[v]50[opt]50
[v]51[opt]51
[v]52[opt]52
[v]53[opt]53
[v]54[opt]54
[v]55[opt]55
[v]56[opt]56
[v]57[opt]57
[v]58[opt]58
[v]59[opt]59
[v]60[opt]60
[v]61[opt]61
[v]62[opt]62
[v]63[opt]63
[t]selectlimit[unit]Maximum bit rate for downlink base[u]61.6-61.7[u]base2_2
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t]select[unit]SDU error ratio[u]62.0-62.3[u]
[v]1[opt]1E-2
[v]2[opt]7E-3
[v]3[opt]1E-3
[v]4[opt]1E-4
[v]5[opt]1E-5
[v]6[opt]1E-6
[v]7[opt]1E-1
[v]15[opt]Reserved
[t]select[unit]Residual Bit Error Rate[u]62.4-62.7[u]
[v]1[opt]5E-2
[v]2[opt]1E-2
[v]3[opt]5E-3
[v]4[opt]4E-3
[v]5[opt]1E-3
[v]6[opt]1E-4
[v]7[opt]1E-5
[v]8[opt]1E-6
[v]9[opt]6E-8
[v]15[opt]Reserved
[t]select[unit]Traffic handing priority[u]63.0-63.1[u]
[v]1[opt]level 1
[v]2[opt]level 2
[v]3[opt]level 3
[v]0[opt]Reserved
[t]select[unit]Transfer delay[u]63.2-63.7[u]
[v]0[opt]X*10ms
[v]1[opt]200ms+X*50ms
[v]2[opt]1000ms+X*100ms
[v]3[opt]2600ms+X*100ms
[v]63[opt]Reserved
[t]selectlimit[unit]Guaranteed bit rate uplink range(X)[u]64.0-64.5[u]range3_2
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[v]16[opt]16
[v]17[opt]17
[v]18[opt]18
[v]19[opt]19
[v]20[opt]20
[v]21[opt]21
[v]22[opt]22
[v]23[opt]23
[v]24[opt]24
[v]25[opt]25
[v]26[opt]26
[v]27[opt]27
[v]28[opt]28
[v]29[opt]29
[v]30[opt]30
[v]31[opt]31
[v]32[opt]32
[v]33[opt]33
[v]34[opt]34
[v]35[opt]35
[v]36[opt]36
[v]37[opt]37
[v]38[opt]38
[v]39[opt]39
[v]40[opt]40
[v]41[opt]41
[v]42[opt]42
[v]43[opt]43
[v]44[opt]44
[v]45[opt]45
[v]46[opt]46
[v]47[opt]47
[v]48[opt]48
[v]49[opt]49
[v]50[opt]50
[v]51[opt]51
[v]52[opt]52
[v]53[opt]53
[v]54[opt]54
[v]55[opt]55
[v]56[opt]56
[v]57[opt]57
[v]58[opt]58
[v]59[opt]59
[v]60[opt]60
[v]61[opt]61
[v]62[opt]62
[v]63[opt]63
[t]selectlimit[unit]Guaranteed bit rate uplink base[u]64.6-64.7[u]base3_2
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t]selectlimit[unit]Guaranteed bit rate downlink range(X)[u]65.0-65.5[u]range4_2
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10  
[v]11[opt]11  
[v]12[opt]12  
[v]13[opt]13  
[v]14[opt]14  
[v]15[opt]15  
[v]16[opt]16  
[v]17[opt]17  
[v]18[opt]18  
[v]19[opt]19  
[v]20[opt]20  
[v]21[opt]21  
[v]22[opt]22  
[v]23[opt]23  
[v]24[opt]24  
[v]25[opt]25  
[v]26[opt]26  
[v]27[opt]27  
[v]28[opt]28  
[v]29[opt]29  
[v]30[opt]30  
[v]31[opt]31  
[v]32[opt]32  
[v]33[opt]33  
[v]34[opt]34  
[v]35[opt]35  
[v]36[opt]36  
[v]37[opt]37  
[v]38[opt]38  
[v]39[opt]39  
[v]40[opt]40  
[v]41[opt]41  
[v]42[opt]42  
[v]43[opt]43  
[v]44[opt]44  
[v]45[opt]45  
[v]46[opt]46  
[v]47[opt]47  
[v]48[opt]48  
[v]49[opt]49  
[v]50[opt]50  
[v]51[opt]51  
[v]52[opt]52  
[v]53[opt]53  
[v]54[opt]54  
[v]55[opt]55  
[v]56[opt]56  
[v]57[opt]57  
[v]58[opt]58  
[v]59[opt]59  
[v]60[opt]60  
[v]61[opt]61  
[v]62[opt]62  
[v]63[opt]63
[t]selectlimit[unit]Guaranteed bit rate downlink base[u]65.6-65.7[u]base4_2
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t][unit]Ext2 Qos
[t]select[unit]Source statistics Descriptor[u]66.0-66.3[u]
[v]0[opt]Spare
[v]1[opt]Speech
[t]select[unit]Signalling Indication[u]66.4-66.4[u]
[v]0[opt]Not optimised
[v]1[opt]Optimised
[t]select[unit]Maximum bit rate downlink (ext)[u]67.0-67.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16mbps
[v]75[opt]17mbps
[v]186[opt]128mbps
[v]187[opt]130mbps
[v]250[opt]256mbps
[t]select[unit]Guaranteed bit rate downlink (ext)[u]68.0-68.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16000kbps
[v]75[opt]17Mbps
[v]186[opt]128Mbps
[v]187[opt]130Mbps
[v]250[opt]256Mbps
[t][unit]Ext3 Qos
[t]select[unit]Maximum bit rate uplink (ext)[u]69.0-69.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16000kbps
[v]75[opt]17Mbps
[v]186[opt]128Mbps
[v]187[opt]130Mbps
[v]250[opt]256Mbps
[t]select[unit]Guaranteed bit rate uplink (ext)[u]70.0-70.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16000kbps
[v]75[opt]17Mbps
[v]186[opt]128Mbps
[v]187[opt]130Mbps
[v]250[opt]256Mbps
[remark]
PDP context identifier: 1-3.
PDP Type: 0x0121 = IPv4, 0x0157 = IPv6, 0x0000 = X.25
PDP Address:
IPv4 Len = 4, <IPv4 hex address>
IPv6 Len = 16, <IPv6 hex address>
X.25 Len = 3 to 9, <X.121 address digits>
Empty AddressĄ¤ Field of any type has Len =0
Reliability Class:
1 = Error sensitive,no error correction,limited error tolerance, non real-time traffic
2 = Error sensitive, limited error correction,good error tolerance, non real-time traffic
3 = Not error sensitive, error correction capability and/or very good error tolerance capability, non real-time traffic
4 = Real-time traffic, error sensitive, cope with data loss5 = Real-time traffic, error non-sensitive, cope with data loss
Delay Class:	1 (predictive), 2 (predictive), 3 (predictive) and 4 (Best effort)
Precedence Class: 1 = High, 2 = Normal, 3 = Low
Peak Throughput	1 through 9 (8 Kbps to 2.048 Kbps)
Mean Throughput	1 through 18 (100 to 50 Million Octets per sec), and 31(Best effort)
VPLMN Address Allowed: 0 = Not Allowed, 1 = Allowed
APN:The APN field in the HLR contains either only an APN Network Identifier (i.e. an APN without APN Operator Identifier) or the wild card value (defined in GSM 03.03).Currently we only use the wild card APN "*".
Ext Flag:
0 = Non-included Ext,1 = Included Ext,3 = Included Ext and Ext2 only 1 octet,7 = Included Ext, Ext2 Qos,15 = Included Ext, Ext2, EXt3 Qos
Ext Qos
Allocation/Retention Priority:
There are four priority : Priority 1,Priority 2,Priority 3,Priority 4.
Delivery err SDUs:
1=No detect,2=Err SDUs delilvered,3=Err SDUs not delivered,7=Reserved
Delivery order:
1 =with delivery order,2 = without delivery order,3 = Reserved
Traffic class:
1=Conversation class,2=Streaming class,3=Interactive class,4=Background class,7=Reserved
Maximum SDU size:
Giving a range of values from 10 octets to 1520 octets,1=10 octets,20=200 octets,80=800 octets,100=1000 octets,148=1480 octets,150=1500 octets,151=1502 octets,152=1510 octets,153=1520 octets,255=Reserved
Maximum bit rate for uplink range:0 through 63 (0 Kbps to 63 Kbps)
Maximum bit rate for uplink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
Maximum bit rate for downlink range:0 through 63 (0 Kbps to 63 Kbps)
Maximum bit rate for downlink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
SDU error ratio:
The range is from 5E-2 to 6E-8.1=1E-2,2=7E-3,3=1E-3,4=1E-4,5=1E-5,6=1E-6,7=1E-1,15=Reserved
Residual Bit Error Rate:
The range is from 1E-1 to 1E-6.1=5E-2,2=1E-2,3=5E-3,4=4E-3,5=1E-3 6=1E-4,7=1E-5,8=1E-6,9=6E-8,15=Reserved
Traffic handing priority:
1=priority Level 1,2=priority Level 2,3=priority Level 3,0=Reserved
Transfer delay:0=X*10ms,1=200ms+X*50ms,2=1000ms+X*100ms,3=2600ms+X*100ms
Guaranteed bit rate uplink range:0 through 63 (0 Kbps to 63 Kbps)
Guaranteed bit rate uplink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
Guaranteed bit rate downlink range:0 through 63 (0 Kbps to 63 Kbps)
Guaranteed bit rate downlink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
Ext2 Qos
Source Statistics Descriptor:0=Spare,1=Speech (MS=>NW)
Signalling Indication:
0=Not Optimised for Signalling Traffic,1=Optimised for Signalling Traffic.
Reserved:66.5-66.7
Maximum bit rate downlink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)
Guaranteed bit rate downlink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)
Ext3 Qos
Maximum bit rate uplink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)
Guaranteed bit rate uplink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)

[para]46[Name]PDP context (group 3)
[sqlName]pdp3[t]radio[unit]PDP flag[u]00.0-00.7[u]
[v]0[opt]Disable
[v]1[opt]Enable
[t]select[unit]PDP type[u]01.0-02.7[u]
[v]289[opt]IPv4
[v]343[opt]IPv6
[v]0[opt]X.25
[t]specialInputHlr[unit]PDP address[u]04.0-19.7[u]
[v]keepHex-low-E
[t]select[unit]Reliability Class[u]20.0-20.2[u]
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[t]select[unit]Delay Class[u]20.3-20.7[u]
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[t]select[unit]Precedence Class[u]21.0-21.3[u]
[v]1[opt]High
[v]2[opt]Normal
[v]3[opt]low
[t]select[unit]Peak Throughput[u]21.4-21.7[u]
[v]1[opt]8Kbps
[v]2[opt]16Kbps
[v]3[opt]32Kbps
[v]4[opt]64Kbps
[v]5[opt]128Kbps
[v]6[opt]256Kbps
[v]7[opt]512Kbps
[v]8[opt]1024Kbps
[v]9[opt]2048Kbps
[t]select[unit]Mean Throughput[u]22.0-22.7[u]
[v]1[opt]100Bph
[v]2[opt]200Bph
[v]3[opt]500Bph
[v]4[opt]1kBph
[v]5[opt]2kBph
[v]6[opt]5kBph
[v]7[opt]10kBph
[v]8[opt]20kBph
[v]9[opt]50kBph
[v]10[opt]100kBph
[v]11[opt]200kBph
[v]12[opt]500kBph
[v]13[opt]1mBph
[v]14[opt]2mBph
[v]15[opt]5mBph
[v]16[opt]10mBph
[v]17[opt]20mBph
[v]18[opt]50mBph
[v]31[opt]Best Effort
[t]radio[unit]VPLMN Address Allowed flag[u]23.0-23.7[u]
[v]0[opt]Not allowed
[v]1[opt]Allowed
[t]input[unit]APN[u]24.0-55.7[u]
[v]toAsc-low-0
[t][unit]Ext Qos
[t]select[unit]Ext Flag[u]56.0-56.7[u]
[v]0[opt]Non-included Ext
[v]1[opt]Included Ext
[v]3[opt]Included Ext and Ext2 only 1 octet
[v]7[opt]Included Ext, Ext2
[v]15[opt]Included Ext, Ext2, EXt3
[t]select[unit]Allocation/Retention Priority[u]57.0-57.7[u]
[v]0[opt]Reserved
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[t]select[unit]Delivery err SDUs[u]58.0-58.2[u]
[v]1[opt]No detect
[v]2[opt]Err SDUs delilvered
[v]3[opt]Err SDUs not delivered
[v]7[opt]Reserved
[t]select[unit]Delivery order[u]58.3-58.4[u]
[v]1[opt]delivery order
[v]2[opt]no delivery order
[v]3[opt]Reserved
[t]select[unit]Traffic class[u]58.5-58.7[u]
[v]1[opt]Conversation class
[v]2[opt]Streaming class
[v]3[opt]Interactive class
[v]4[opt]Background class
[v]7[opt]Reserved
[t]select[unit]Maximum SDU size[u]59.0-59.7[u]
[v]1[opt]10 octets
[v]20[opt]200 octets
[v]80[opt]800 octets
[v]100[opt]1000 octets
[v]148[opt]1480 octets
[v]150[opt]1500 octets
[v]151[opt]1502 octets
[v]152[opt]1510 octets
[v]153[opt]1520 octets
[v]255[opt]Reserved
[t]selectlimit[unit]Maximum bit rate for uplink range(X)[u]60.0-60.5[u]range1_3
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[v]16[opt]16
[v]17[opt]17
[v]18[opt]18
[v]19[opt]19
[v]20[opt]20
[v]21[opt]21
[v]22[opt]22
[v]23[opt]23
[v]24[opt]24
[v]25[opt]25
[v]26[opt]26
[v]27[opt]27
[v]28[opt]28
[v]29[opt]29
[v]30[opt]30
[v]31[opt]31
[v]32[opt]32
[v]33[opt]33
[v]34[opt]34
[v]35[opt]35
[v]36[opt]36
[v]37[opt]37
[v]38[opt]38
[v]39[opt]39
[v]40[opt]40
[v]41[opt]41
[v]42[opt]42
[v]43[opt]43
[v]44[opt]44
[v]45[opt]45
[v]46[opt]46
[v]47[opt]47
[v]48[opt]48
[v]49[opt]49
[v]50[opt]50
[v]51[opt]51
[v]52[opt]52
[v]53[opt]53
[v]54[opt]54
[v]55[opt]55
[v]56[opt]56
[v]57[opt]57
[v]58[opt]58
[v]59[opt]59
[v]60[opt]60
[v]61[opt]61
[v]62[opt]62
[v]63[opt]63
[t]selectlimit[unit]Maximum bit rate for uplink base[u]60.6-60.7[u]base1_3
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t]selectlimit[unit]Maximum bit rate for downlink range(X)[u]61.0-61.5[u]range2_3
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[v]16[opt]16
[v]17[opt]17
[v]18[opt]18
[v]19[opt]19
[v]20[opt]20
[v]21[opt]21
[v]22[opt]22
[v]23[opt]23
[v]24[opt]24
[v]25[opt]25
[v]26[opt]26
[v]27[opt]27
[v]28[opt]28
[v]29[opt]29
[v]30[opt]30
[v]31[opt]31
[v]32[opt]32
[v]33[opt]33
[v]34[opt]34
[v]35[opt]35
[v]36[opt]36
[v]37[opt]37
[v]38[opt]38
[v]39[opt]39
[v]40[opt]40
[v]41[opt]41
[v]42[opt]42
[v]43[opt]43
[v]44[opt]44
[v]45[opt]45
[v]46[opt]46
[v]47[opt]47
[v]48[opt]48
[v]49[opt]49
[v]50[opt]50
[v]51[opt]51
[v]52[opt]52
[v]53[opt]53
[v]54[opt]54
[v]55[opt]55
[v]56[opt]56
[v]57[opt]57
[v]58[opt]58
[v]59[opt]59
[v]60[opt]60
[v]61[opt]61
[v]62[opt]62
[v]63[opt]63
[t]selectlimit[unit]Maximum bit rate for downlink base[u]61.6-61.7[u]base2_3
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t]select[unit]SDU error ratio[u]62.0-62.3[u]
[v]1[opt]1E-2
[v]2[opt]7E-3
[v]3[opt]1E-3
[v]4[opt]1E-4
[v]5[opt]1E-5
[v]6[opt]1E-6
[v]7[opt]1E-1
[v]15[opt]Reserved
[t]select[unit]Residual Bit Error Rate[u]62.4-62.7[u]
[v]1[opt]5E-2
[v]2[opt]1E-2
[v]3[opt]5E-3
[v]4[opt]4E-3
[v]5[opt]1E-3
[v]6[opt]1E-4
[v]7[opt]1E-5
[v]8[opt]1E-6
[v]9[opt]6E-8
[v]15[opt]Reserved
[t]select[unit]Traffic handing priority[u]63.0-63.1[u]
[v]1[opt]level 1
[v]2[opt]level 2
[v]3[opt]level 3
[v]0[opt]Reserved
[t]select[unit]Transfer delay[u]63.2-63.7[u]
[v]0[opt]X*10ms
[v]1[opt]200ms+X*50ms
[v]2[opt]1000ms+X*100ms
[v]3[opt]2600ms+X*100ms
[v]63[opt]Reserved
[t]selectlimit[unit]Guaranteed bit rate uplink range(X)[u]64.0-64.5[u]range3_3
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[v]16[opt]16
[v]17[opt]17
[v]18[opt]18
[v]19[opt]19
[v]20[opt]20
[v]21[opt]21
[v]22[opt]22
[v]23[opt]23
[v]24[opt]24
[v]25[opt]25
[v]26[opt]26
[v]27[opt]27
[v]28[opt]28
[v]29[opt]29
[v]30[opt]30
[v]31[opt]31
[v]32[opt]32
[v]33[opt]33
[v]34[opt]34
[v]35[opt]35
[v]36[opt]36
[v]37[opt]37
[v]38[opt]38
[v]39[opt]39
[v]40[opt]40
[v]41[opt]41
[v]42[opt]42
[v]43[opt]43
[v]44[opt]44
[v]45[opt]45
[v]46[opt]46
[v]47[opt]47
[v]48[opt]48
[v]49[opt]49
[v]50[opt]50
[v]51[opt]51
[v]52[opt]52
[v]53[opt]53
[v]54[opt]54
[v]55[opt]55
[v]56[opt]56
[v]57[opt]57
[v]58[opt]58
[v]59[opt]59
[v]60[opt]60
[v]61[opt]61
[v]62[opt]62
[v]63[opt]63
[t]selectlimit[unit]Guaranteed bit rate uplink base[u]64.6-64.7[u]base3_3
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t]selectlimit[unit]Guaranteed bit rate downlink range(X)[u]65.0-65.5[u]range4_3
[v]0[opt]0
[v]1[opt]1
[v]2[opt]2
[v]3[opt]3
[v]4[opt]4
[v]5[opt]5
[v]6[opt]6
[v]7[opt]7
[v]8[opt]8
[v]9[opt]9
[v]10[opt]10
[v]11[opt]11
[v]12[opt]12
[v]13[opt]13
[v]14[opt]14
[v]15[opt]15
[v]16[opt]16
[v]17[opt]17
[v]18[opt]18
[v]19[opt]19
[v]20[opt]20
[v]21[opt]21
[v]22[opt]22
[v]23[opt]23
[v]24[opt]24
[v]25[opt]25
[v]26[opt]26
[v]27[opt]27
[v]28[opt]28
[v]29[opt]29
[v]30[opt]30
[v]31[opt]31
[v]32[opt]32
[v]33[opt]33
[v]34[opt]34
[v]35[opt]35
[v]36[opt]36
[v]37[opt]37
[v]38[opt]38
[v]39[opt]39
[v]40[opt]40
[v]41[opt]41
[v]42[opt]42
[v]43[opt]43
[v]44[opt]44
[v]45[opt]45
[v]46[opt]46
[v]47[opt]47
[v]48[opt]48
[v]49[opt]49
[v]50[opt]50
[v]51[opt]51
[v]52[opt]52
[v]53[opt]53
[v]54[opt]54
[v]55[opt]55
[v]56[opt]56
[v]57[opt]57
[v]58[opt]58
[v]59[opt]59
[v]60[opt]60
[v]61[opt]61
[v]62[opt]62
[v]63[opt]63
[t]selectlimit[unit]Guaranteed bit rate downlink base[u]65.6-65.7[u]base4_3
[v]0[opt]X*1kbps
[v]1[opt]64kbps+(X*8kbps)
[v]2[opt]576kbps+(X*64kbps)
[v]3[opt]4672kbps+(X*64kbps)
[t][unit]Ext2 Qos
[t]select[unit]Source statistics Descriptor[u]66.0-66.3[u]
[v]0[opt]Spare
[v]1[opt]Speech
[t]select[unit]Signalling Indication[u]66.4-66.4[u]
[v]0[opt]Not optimised
[v]1[opt]Optimised
[t]select[unit]Maximum bit rate downlink (ext)[u]67.0-67.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16mbps
[v]75[opt]17mbps
[v]186[opt]128mbps
[v]187[opt]130mbps
[v]250[opt]256mbps
[t]select[unit]Guaranteed bit rate downlink (ext)[u]68.0-68.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16000kbps
[v]75[opt]17Mbps
[v]186[opt]128Mbps
[v]187[opt]130Mbps
[v]250[opt]256Mbps
[t][unit]Ext Qos
[t]select[unit]Maximum bit rate uplink (ext)[u]69.0-69.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16000kbps
[v]75[opt]17Mbps
[v]186[opt]128Mbps
[v]187[opt]130Mbps
[v]250[opt]256Mbps
[t]select[unit]Guaranteed bit rate uplink (ext)[u]70.0-70.7[u]
[v]0[opt]<=8600kbps
[v]1[opt]8700kbps
[v]74[opt]16000kbps
[v]75[opt]17Mbps
[v]186[opt]128Mbps
[v]187[opt]130Mbps
[v]250[opt]256Mbps
[remark]
PDP context identifier: 1-3.
PDP Type: 0x0121 = IPv4, 0x0157 = IPv6, 0x0000 = X.25
PDP Address:
IPv4 Len = 4, <IPv4 hex address>
IPv6 Len = 16, <IPv6 hex address>
X.25 Len = 3 to 9, <X.121 address digits>
Empty AddressĄ¤ Field of any type has Len =0
Reliability Class:
1 = Error sensitive,no error correction,limited error tolerance, non real-time traffic
2 = Error sensitive, limited error correction,good error tolerance, non real-time traffic
3 = Not error sensitive, error correction capability and/or very good error tolerance capability, non real-time traffic
4 = Real-time traffic, error sensitive, cope with data loss5 = Real-time traffic, error non-sensitive, cope with data loss
Delay Class:	1 (predictive), 2 (predictive), 3 (predictive) and 4 (Best effort)
Precedence Class: 1 = High, 2 = Normal, 3 = Low
Peak Throughput	1 through 9 (8 Kbps to 2.048 Kbps)
Mean Throughput	1 through 18 (100 to 50 Million Octets per sec), and 31(Best effort)
VPLMN Address Allowed: 0 = Not Allowed, 1 = Allowed
APN:The APN field in the HLR contains either only an APN Network Identifier (i.e. an APN without APN Operator Identifier) or the wild card value (defined in GSM 03.03).Currently we only use the wild card APN "*".
Ext Flag:
0 = Non-included Ext,1 = Included Ext,3 = Included Ext and Ext2 only 1 octet,7 = Included Ext, Ext2 Qos,15 = Included Ext, Ext2, EXt3 Qos
Ext Qos
Allocation/Retention Priority:
There are four priority : Priority 1,Priority 2,Priority 3,Priority 4.
Delivery err SDUs:
1=No detect,2=Err SDUs delilvered,3=Err SDUs not delivered,7=Reserved
Delivery order:
1 =with delivery order,2 = without delivery order,3 = Reserved
Traffic class:
1=Conversation class,2=Streaming class,3=Interactive class,4=Background class,7=Reserved
Maximum SDU size:
Giving a range of values from 10 octets to 1520 octets,1=10 octets,20=200 octets,80=800 octets,100=1000 octets,148=1480 octets,150=1500 octets,151=1502 octets,152=1510 octets,153=1520 octets,255=Reserved
Maximum bit rate for uplink range:0 through 63 (0 Kbps to 63 Kbps)
Maximum bit rate for uplink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
Maximum bit rate for downlink range:0 through 63 (0 Kbps to 63 Kbps)
Maximum bit rate for downlink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
SDU error ratio:
The range is from 5E-2 to 6E-8.1=1E-2,2=7E-3,3=1E-3,4=1E-4,5=1E-5,6=1E-6,7=1E-1,15=Reserved
Residual Bit Error Rate:
The range is from 1E-1 to 1E-6.1=5E-2,2=1E-2,3=5E-3,4=4E-3,5=1E-3 6=1E-4,7=1E-5,8=1E-6,9=6E-8,15=Reserved
Traffic handing priority:
1=priority Level 1,2=priority Level 2,3=priority Level 3,0=Reserved
Transfer delay:0=X*10ms,1=200ms+X*50ms,2=1000ms+X*100ms,3=2600ms+X*100ms
Guaranteed bit rate uplink range:0 through 63 (0 Kbps to 63 Kbps)
Guaranteed bit rate uplink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
Guaranteed bit rate downlink range:0 through 63 (0 Kbps to 63 Kbps)
Guaranteed bit rate downlink base:
0=X*1kbps,1=64kbps+(X*8kbps),2=576kbps+(X*64kbps),3=4672kbps+(X*64kbps)
Ext2 Qos
Source Statistics Descriptor:0=Spare,1=Speech (MS=>NW)
Signalling Indication:
0=Not Optimised for Signalling Traffic,1=Optimised for Signalling Traffic.
Reserved:66.5-66.7
Maximum bit rate downlink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)
Guaranteed bit rate downlink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)
Ext3 Qos
Maximum bit rate uplink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)
Guaranteed bit rate uplink (extended):0(<=8600kbps),1(8700kbps),74(16000kbps),75(17Mbps),186(128Mbps),187(130Mbps),250(256Mbps)

[para]47[Name]User name
[sqlName]user_name[t]input[unit]User name[u]00.0-23.7[u]
[v]keepAsc-low-0
[remark]User real name. For post-pay subscriber registration.

[para]48[Name]User certificate
[sqlName]user_certifiacate[t]input[unit]User cetificate[u]00.0-15.7[u]
[v]keepAsc-low-0
[remark]
User ID

[para]49[Name]VLR Number
[sqlName]vlr_num[t]readOnly[unit]ISDN number plan[u]00.0-00.7[u]code
[v]keepHex-high-0
[unit]ISDN number[u]01.0-08.7[u]
[v]keepHex-low-E
[remark]
VLR E.164 number

[para]50[Name]MSC Number
[sqlName]msc_num[t]readOnly[unit]MSC Number[u]00.0-00.7[u]code
[v]keepHex-high-0
[unit]ISDN number[u]01.0-08.7[u]
[v]keepHex-low-E
[remark]
MSC E.164 number
