[para]0[Name]MSISDN
[sqlName]MSISDN[t]input[unit]MSISDN[u]00.0-08.7[u]
[v]keepHex-low-F
[remark]

[para]1[Name]IMSI
[sqlName]IMSI[t]readOnly[unit]IMSI[u]00.0-15.7[u]
[v]keepAsc-low-F
[remark]

[para]2[Name]MSISDN
[sqlName]MSISDN[t]readOnly[unit]MSISDN[u]00.0-08.7[u]
[v]keepHex-low-F
[remark]

[para]3[Name]MS category
[sqlName]MS_Category[t]show[unit]MS category[u]00.0-00.7[u]
[v]00[opt]Unknown
[v]01[opt]French language
[v]02[opt]English language
[v]03[opt]German language
[v]04[opt]Russian language
[v]05[opt]Spanish language
[v]10[opt]Ordinary
[v]11[opt]Subscriber with priority
[remark]

[para]4[Name]ODB status
[sqlName]Sub_status[t]show[unit]ODB status[u]00.0-00.7[u]
[v]00[opt]Service granted
[v]01[opt]Operator determined barring
[remark]

[para]5[Name]ODB general
[sqlName]ODB_General[t]checkbox[unit]BAOC[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BOIC[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BOIC_exHC[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BPRIC[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BPREC[u]00.4-00.4[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]SS_Access[u]00.5-00.5[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BAIC[u]00.6-00.6[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]BAICRoam[u]00.7-00.7[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]6[Name]Provisioned tele service
[sqlName]Provision_ts[t]checkbox[unit]Telephony provision[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Emergency call provision[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Short message MT provision[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Short message MO provision[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]7[Name]TMSI
[sqlName]TMSI[t]readOnly[unit]TMSI[u]00.0-03.7[u]
[v]keepHex-high-0
[remark]

[para]8[Name]LAI(MCC-MNC-LAC)
[sqlName]LAI[t]vlrSpecialRead[unit]CC[u]00.0-04.7[u]
[v]keepHex-low-F
[remark]

[para]9[Name]Cell ID
[sqlName]Cell_ID[t]readOnly[unit]Cell ID[u]00.0-01.7[u]
[v]keepHex-high-0
[remark]

[para]10[Name]Location confirm
[sqlName]LocationConfirm[t]show[unit]Location confirm[u]00.0-00.7[u]
[v]0[opt]Not Confirmed
[v]1[opt]Confirmed
[remark]

[para]11[Name]Data confirm
[sqlName]DataConfirmFlag[t]show[unit]Data confirm[u]00.0-00.7[u]
[v]0[opt]Not Confirmed
[v]1[opt]Confirmed
[remark]

[para]12[Name]Radio confirm
[sqlName]RadioConfirmFlag[t]show[unit]Radio confirm[u]00.0-00.7[u]
[v]0[opt]Not Confirmed
[v]1[opt]Confirmed
[remark]

[para]13[Name]IMSI detach
[sqlName]IMSIDetachFlag[t]show[unit]IMSI detach[u]00.0-00.7[u]
[v]0[opt]Attached
[v]1[opt]Detached
[remark]
 
[para]14[Name]MNRF
[sqlName]MNRF[t]show[unit]MNRF[u]00.0-00.7[u]
[v]0[opt]Reachable
[v]1[opt]Not Reachable
[remark]  

[para]15[Name]LA_Not_allowed
[sqlName]LANotAllowedFlag[t]show[unit]LA_Not_allowed[u]00.0-00.7[u]
[v]0[opt]Not allowed
[v]1[opt]Allowed
[remark]  

[para]16[Name]Roaming restricted
[sqlName]RoamRestricFlag[t]show[unit]Roaming restricted[u]00.0-00.7[u]
[v]0[opt]Not restricted
[v]1[opt]Restricted
[remark] 

[para]17[Name]CFU status
[sqlName]CFU_ST[t]checkbox[unit]A bit (indicate active state[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Notification to calling party[u]00.5-00.5[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Notification to forwarding party[u]00.7-00.7[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]18[Name]CFU: Forward to number
[sqlName]CFU_Num[t]readOnly[unit]CFU: Forward to number[u]00.0-08.7[u]
[v]keepHex-low-F
[remark]

[para]19[Name]CFB status
[sqlName]CFB_ST[t]checkbox[unit]A bit (indicate active state[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Notification to calling party[u]00.5-00.5[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Notification to forwarding party[u]00.7-00.7[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]20[Name]CFB: Forward to number
[sqlName]CFB_Num[t]readOnly[unit]CFB: Forward to number[u]00.0-08.7[u]
[v]keepHex-low-F
[remark]

[para]21[Name]CFNRy status
[sqlName]CFNRy_ST[t]checkbox[unit]A bit (indicate active state[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Notification to calling party[u]00.5-00.5[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Notification to forwarding party[u]00.7-00.7[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]22[Name]CFNRy: Forward to number
[sqlName]CFNRy_Num[t]readOnly[unit]CFNRy: Forward to number[u]00.0-08.7[u]
[v]keepHex-low-F
[remark]

[para]23[Name]CFNRc status
[sqlName]CFNRc_ST[t]checkbox[unit]A bit (indicate active state[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Notification to calling party[u]00.5-00.5[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Notification to forwarding party[u]00.7-00.7[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]24[Name]CFNRc: Forward to number
[sqlName]CFNRc_Num[t]readOnly[unit]CFNRc: Forward to number[u]00.0-08.7[u]
[v]keepHex-low-F
[remark]

[para]25[Name]Barring all calls
[sqlName]ALLBAR[t]show[unit]Roaming restricted[u]00.0-03.7[u]
[v]00[opt]No
[v]01[opt]Yes
[remark] 

[para]26[Name]BAOC
[sqlName]BAOC[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]27[Name]BOIC
[sqlName]BOIC[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]28[Name]BOIC-ExHC
[sqlName]BOICexHC[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]29[Name]BAIC
[sqlName]BAIC[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]30[Name]BICRoam
[sqlName]BICRoam[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]31[Name]CLIP
[sqlName]CLIP[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]32[Name]CLIR
[sqlName]CLIR[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]33[Name]COLP
[sqlName]COLP[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]34[Name]COLR
[sqlName]COLR[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]35[Name]AOCI
[sqlName]AOCI[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]36[Name]AOCC
[sqlName]AOCC[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]37[Name]Call hold
[sqlName]CallHold[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]38[Name]Call wait
[sqlName]CallWait[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]38[Name]ECT
[sqlName]ECT[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]39[Name]MPTY
[sqlName]MPTY[t]checkbox[unit]A bit (indicate active state)[u]00.0-00.0[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]R bit (indicate registration state)[u]00.1-00.1[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]P bit (indicate provision state)[u]00.2-00.2[u]
[v]0[opt]not support
[v]1[opt]support
[t]checkbox[unit]Q bit (indicate quiescent state)[u]00.3-00.3[u]
[v]0[opt]not support
[v]1[opt]support
[remark]

[para]40[Name]O-CSI
[sqlName]O_CSI[t]show[unit]O-CSI[u]00.0-03.7[u]
[v]00[opt]Not Provisioned
[v]01[opt]Provisioned
SCF Number:$oCsiScpNum
[remark]

[para]41[Name]SMS-CSI
[sqlName]SMS_CSI[t]show[unit]SMS-CSI[u]00.0-03.7[u]
[v]00[opt]Not Provisioned
[v]01[opt]Provisioned
SCF Number:$oCsiScpNum
[remark]

[para]42[Name]MSISDN(Opt)
[sqlName]MSISDN_opt[t]readOnly[unit]MSISDN(Opt)[u]00.0-15.7[u]--
[v]keepAsc-low-E
[remark]

[para]43[Name]OPPS Flag
[sqlName]MSISDN_opt[t]show[unit]]OPPS Flag[u]00.0-03.7[u]
[v]0[opt]OPR Not Registerd
[v]1[opt]OPR WithOut Roam Agreement OPRState
[v]2[opt]OPR With Roam Agreeement OPRState
[v]3[opt]OPR With Roam Agreeement RoamingState
[v]4[opt]IMDXPrivate
[v]5[opt]IMDXHbrid
[v]6[opt]IMDXPublic
[remark]