-- ASN1START
-- **************************************************************
--
-- Elementary Procedure definitions
--
-- **************************************************************

NGAP-PDU-Descriptions  { 
itu-t (0) identified-organization (4) etsi (0) mobileDomain (0) 
ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-PDU-Descriptions (0)}

DEFINITIONS AUTOMATIC TAGS ::= 

BEGIN

-- **************************************************************
--
-- IE parameter types from other modules.
--
-- **************************************************************

IMPORTS

	Criticality,
	ProcedureCode
FROM NGAP-CommonDataTypes

	AMFConfigurationUpdate,
	AMFConfigurationUpdateAcknowledge,
	AMFConfigurationUpdateFailure,
	AMFStatusIndication,
	CellTrafficTrace,
	DeactivateTrace,
	DownlinkNASTransport,
	DownlinkNonUEAssociatedNRPPaTransport,
	DownlinkRANConfigurationTransfer,
	DownlinkRANStatusTransfer,
	DownlinkUEAssociatedNRPPaTransport,
	ErrorIndication,
	HandoverCancel,
	HandoverCancelAcknowledge,
	HandoverCommand,
	HandoverFailure,
	HandoverNotify,
	HandoverPreparationFailure,
	HandoverRequest,
	HandoverRequestAcknowledge,
	HandoverRequired,
	InitialContextSetupFailure,
	InitialContextSetupRequest,
	InitialContextSetupResponse,
	InitialUEMessage,
	LocationReport,
	LocationReportingControl,
	LocationReportingFailureIndication,
	NASNonDeliveryIndication,
	NGReset,
	NGResetAcknowledge,
	NGSetupFailure,
	NGSetupRequest,
	NGSetupResponse,
	OverloadStart,
	OverloadStop,
	Paging,
	PathSwitchRequest,
	PathSwitchRequestAcknowledge,
	PathSwitchRequestFailure,	
	PDUSessionResourceModifyConfirm,
	PDUSessionResourceModifyIndication,
	PDUSessionResourceModifyRequest,
	PDUSessionResourceModifyResponse,
	PDUSessionResourceNotify,
	PDUSessionResourceReleaseCommand,
	PDUSessionResourceReleaseResponse,
	PDUSessionResourceSetupRequest,
	PDUSessionResourceSetupResponse,
	PrivateMessage,
	PWSCancelRequest,
	PWSCancelResponse,
	PWSFailureIndication,
	PWSRestartIndication,
	RANConfigurationUpdate,
	RANConfigurationUpdateAcknowledge,
	RANConfigurationUpdateFailure,
	RerouteNASRequest,
	RRCInactiveTransitionReport,
	SecondaryRATDataUsageReport,
	TraceFailureIndication,
	TraceStart,
	UEContextModificationFailure,
	UEContextModificationRequest,
	UEContextModificationResponse,
	UEContextReleaseCommand,
	UEContextReleaseComplete,
	UEContextReleaseRequest,
	UERadioCapabilityCheckRequest,
	UERadioCapabilityCheckResponse,
	UERadioCapabilityInfoIndication,
	UETNLABindingReleaseRequest,
	UplinkNASTransport,
	UplinkNonUEAssociatedNRPPaTransport,
	UplinkRANConfigurationTransfer,
	UplinkRANStatusTransfer,
	UplinkUEAssociatedNRPPaTransport,
	WriteReplaceWarningRequest,
	WriteReplaceWarningResponse
FROM NGAP-PDU-Contents

	id-AMFConfigurationUpdate,
	id-AMFStatusIndication,
	id-CellTrafficTrace,
	id-DeactivateTrace,
	id-DownlinkNASTransport,
	id-DownlinkNonUEAssociatedNRPPaTransport,
	id-DownlinkRANConfigurationTransfer,
	id-DownlinkRANStatusTransfer,
	id-DownlinkUEAssociatedNRPPaTransport,
	id-ErrorIndication,
	id-HandoverCancel,
	id-HandoverNotification,
	id-HandoverPreparation,
	id-HandoverResourceAllocation,
	id-InitialContextSetup,
	id-InitialUEMessage,
	id-LocationReport,
	id-LocationReportingControl,
	id-LocationReportingFailureIndication,
	id-NASNonDeliveryIndication,
	id-NGReset,
	id-NGSetup,
	id-OverloadStart,
	id-OverloadStop,
	id-Paging,
	id-PathSwitchRequest,
	id-PDUSessionResourceModify,
	id-PDUSessionResourceModifyIndication,
	id-PDUSessionResourceNotify,
	id-PDUSessionResourceRelease,
	id-PDUSessionResourceSetup,
	id-PrivateMessage,
	id-PWSCancel,
	id-PWSFailureIndication,
	id-PWSRestartIndication,
	id-RANConfigurationUpdate,
	id-RerouteNASRequest,
	id-RRCInactiveTransitionReport,
	id-SecondaryRATDataUsageReport,
	id-TraceFailureIndication,
	id-TraceStart,
	id-UEContextModification,
	id-UEContextRelease,
	id-UEContextReleaseRequest,
	id-UERadioCapabilityCheck,
	id-UERadioCapabilityInfoIndication,
	id-UETNLABindingRelease,
	id-UplinkNASTransport,
	id-UplinkNonUEAssociatedNRPPaTransport,
	id-UplinkRANConfigurationTransfer,
	id-UplinkRANStatusTransfer,
	id-UplinkUEAssociatedNRPPaTransport,
	id-WriteReplaceWarning
FROM NGAP-Constants;

-- **************************************************************
--
-- Interface Elementary Procedure Class
--
-- **************************************************************

NGAP-ELEMENTARY-PROCEDURE ::= CLASS {
	&InitiatingMessage				,
	&SuccessfulOutcome							OPTIONAL,
	&UnsuccessfulOutcome						OPTIONAL,
	&procedureCode				ProcedureCode	UNIQUE,
	&criticality				Criticality	DEFAULT ignore
}

WITH SYNTAX {
	INITIATING MESSAGE			&InitiatingMessage
	[SUCCESSFUL OUTCOME			&SuccessfulOutcome]
	[UNSUCCESSFUL OUTCOME		&UnsuccessfulOutcome]
	PROCEDURE CODE				&procedureCode
	[CRITICALITY				&criticality]
}

-- **************************************************************
--
-- Interface PDU Definition
--
-- **************************************************************

NGAP-PDU ::= CHOICE {
	initiatingMessage			InitiatingMessage,
	successfulOutcome			SuccessfulOutcome,
	unsuccessfulOutcome			UnsuccessfulOutcome,
	...
}

InitiatingMessage ::= SEQUENCE {
	procedureCode	NGAP-ELEMENTARY-PROCEDURE.&procedureCode		({NGAP-ELEMENTARY-PROCEDURES}),
	criticality		NGAP-ELEMENTARY-PROCEDURE.&criticality			({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode}),
	value			NGAP-ELEMENTARY-PROCEDURE.&InitiatingMessage	({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode})
}

SuccessfulOutcome ::= SEQUENCE {
	procedureCode	NGAP-ELEMENTARY-PROCEDURE.&procedureCode		({NGAP-ELEMENTARY-PROCEDURES}),
	criticality		NGAP-ELEMENTARY-PROCEDURE.&criticality			({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode}),
	value			NGAP-ELEMENTARY-PROCEDURE.&SuccessfulOutcome	({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode})
}

UnsuccessfulOutcome ::= SEQUENCE {
	procedureCode	NGAP-ELEMENTARY-PROCEDURE.&procedureCode		({NGAP-ELEMENTARY-PROCEDURES}),
	criticality		NGAP-ELEMENTARY-PROCEDURE.&criticality			({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode}),
	value			NGAP-ELEMENTARY-PROCEDURE.&UnsuccessfulOutcome	({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode})
}

-- **************************************************************
--
-- Interface Elementary Procedure List
--
-- **************************************************************

NGAP-ELEMENTARY-PROCEDURES NGAP-ELEMENTARY-PROCEDURE ::= {
	NGAP-ELEMENTARY-PROCEDURES-CLASS-1			|
	NGAP-ELEMENTARY-PROCEDURES-CLASS-2,	
	...
}

NGAP-ELEMENTARY-PROCEDURES-CLASS-1 NGAP-ELEMENTARY-PROCEDURE ::= {
	aMFConfigurationUpdate			|
	handoverCancel					|
	handoverPreparation				|
	handoverResourceAllocation		|
	initialContextSetup				|
	nGReset							|
	nGSetup							|
	pathSwitchRequest				|
	pDUSessionResourceModify		|
	pDUSessionResourceModifyIndication			|
	pDUSessionResourceRelease		|
	pDUSessionResourceSetup			|
	pWSCancel						|
	rANConfigurationUpdate			|
	uEContextModification			|
	uEContextRelease				|
	uERadioCapabilityCheck			|
	writeReplaceWarning
}

NGAP-ELEMENTARY-PROCEDURES-CLASS-2 NGAP-ELEMENTARY-PROCEDURE ::= {	
	aMFStatusIndication				|
	cellTrafficTrace				|
	deactivateTrace					|
	downlinkNASTransport			|
	downlinkNonUEAssociatedNRPPaTransport	|
	downlinkRANConfigurationTransfer	|
	downlinkRANStatusTransfer		|
	downlinkUEAssociatedNRPPaTransport	|
	errorIndication					|
	handoverNotification			|
	initialUEMessage				|
	locationReport					|
	locationReportingControl		|
	locationReportingFailureIndication	|
	nASNonDeliveryIndication		|
	overloadStart					|
	overloadStop					|
	paging							|
	pDUSessionResourceNotify		|
	privateMessage					|
	pWSFailureIndication						|
	pWSRestartIndication			|
	rerouteNASRequest				|
	rRCInactiveTransitionReport					|
	secondaryRATDataUsageReport		|
	traceFailureIndication			|
	traceStart						|
	uEContextReleaseRequest			|
	uERadioCapabilityInfoIndication	|
	uETNLABindingRelease			|
	uplinkNASTransport				|
	uplinkNonUEAssociatedNRPPaTransport	|
	uplinkRANConfigurationTransfer	|
	uplinkRANStatusTransfer			|
	uplinkUEAssociatedNRPPaTransport
}

-- **************************************************************
--
-- Interface Elementary Procedures
--
-- **************************************************************

aMFConfigurationUpdate NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		AMFConfigurationUpdate
	SUCCESSFUL OUTCOME		AMFConfigurationUpdateAcknowledge
	UNSUCCESSFUL OUTCOME	AMFConfigurationUpdateFailure
	PROCEDURE CODE			id-AMFConfigurationUpdate
	CRITICALITY				reject
}

aMFStatusIndication NGAP-ELEMENTARY-PROCEDURE ::={
	INITIATING MESSAGE		AMFStatusIndication
	PROCEDURE CODE			id-AMFStatusIndication
	CRITICALITY				ignore
}

cellTrafficTrace NGAP-ELEMENTARY-PROCEDURE ::={
	INITIATING MESSAGE		CellTrafficTrace
	PROCEDURE CODE			id-CellTrafficTrace
	CRITICALITY				ignore
}

deactivateTrace NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DeactivateTrace
	PROCEDURE CODE			id-DeactivateTrace
	CRITICALITY				ignore
}

downlinkNASTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkNASTransport
	PROCEDURE CODE			id-DownlinkNASTransport
	CRITICALITY				ignore
}

downlinkNonUEAssociatedNRPPaTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkNonUEAssociatedNRPPaTransport
	PROCEDURE CODE			id-DownlinkNonUEAssociatedNRPPaTransport
	CRITICALITY				ignore
}

downlinkRANConfigurationTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkRANConfigurationTransfer
	PROCEDURE CODE			id-DownlinkRANConfigurationTransfer
	CRITICALITY				ignore
}

downlinkRANStatusTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkRANStatusTransfer
	PROCEDURE CODE			id-DownlinkRANStatusTransfer
	CRITICALITY				ignore
}

downlinkUEAssociatedNRPPaTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkUEAssociatedNRPPaTransport
	PROCEDURE CODE			id-DownlinkUEAssociatedNRPPaTransport
	CRITICALITY				ignore
}

errorIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		ErrorIndication
	PROCEDURE CODE			id-ErrorIndication
	CRITICALITY				ignore
}

handoverCancel NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		HandoverCancel
	SUCCESSFUL OUTCOME		HandoverCancelAcknowledge
	PROCEDURE CODE			id-HandoverCancel
	CRITICALITY				reject
}

handoverNotification NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		HandoverNotify
	PROCEDURE CODE			id-HandoverNotification
	CRITICALITY				ignore
}

handoverPreparation NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		HandoverRequired
	SUCCESSFUL OUTCOME		HandoverCommand
	UNSUCCESSFUL OUTCOME	HandoverPreparationFailure
	PROCEDURE CODE			id-HandoverPreparation
	CRITICALITY				reject
}

handoverResourceAllocation NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		HandoverRequest
	SUCCESSFUL OUTCOME		HandoverRequestAcknowledge
	UNSUCCESSFUL OUTCOME	HandoverFailure
	PROCEDURE CODE			id-HandoverResourceAllocation
	CRITICALITY				reject
}

initialContextSetup NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		InitialContextSetupRequest
	SUCCESSFUL OUTCOME		InitialContextSetupResponse
	UNSUCCESSFUL OUTCOME	InitialContextSetupFailure
	PROCEDURE CODE			id-InitialContextSetup
	CRITICALITY				reject
}

initialUEMessage NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		InitialUEMessage
	PROCEDURE CODE			id-InitialUEMessage
	CRITICALITY				ignore
}

locationReport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		LocationReport
	PROCEDURE CODE			id-LocationReport
	CRITICALITY				ignore
}

locationReportingControl NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		LocationReportingControl
	PROCEDURE CODE			id-LocationReportingControl
	CRITICALITY				ignore
}

locationReportingFailureIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		LocationReportingFailureIndication
	PROCEDURE CODE			id-LocationReportingFailureIndication
	CRITICALITY				ignore
}

nASNonDeliveryIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		NASNonDeliveryIndication
	PROCEDURE CODE			id-NASNonDeliveryIndication
	CRITICALITY				ignore
}

nGReset NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		NGReset
	SUCCESSFUL OUTCOME		NGResetAcknowledge
	PROCEDURE CODE			id-NGReset
	CRITICALITY				reject
}

nGSetup NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		NGSetupRequest
	SUCCESSFUL OUTCOME		NGSetupResponse
	UNSUCCESSFUL OUTCOME	NGSetupFailure
	PROCEDURE CODE			id-NGSetup
	CRITICALITY				reject
}

overloadStart NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		OverloadStart
	PROCEDURE CODE			id-OverloadStart
	CRITICALITY				ignore
}

overloadStop NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		OverloadStop
	PROCEDURE CODE			id-OverloadStop
	CRITICALITY				reject
}

paging NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		Paging
	PROCEDURE CODE			id-Paging
	CRITICALITY				ignore
}

pathSwitchRequest NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PathSwitchRequest
	SUCCESSFUL OUTCOME		PathSwitchRequestAcknowledge
	UNSUCCESSFUL OUTCOME	PathSwitchRequestFailure
	PROCEDURE CODE			id-PathSwitchRequest
	CRITICALITY				reject
}

pDUSessionResourceModify NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PDUSessionResourceModifyRequest
	SUCCESSFUL OUTCOME		PDUSessionResourceModifyResponse
	PROCEDURE CODE			id-PDUSessionResourceModify
	CRITICALITY				reject
}

pDUSessionResourceModifyIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PDUSessionResourceModifyIndication
	SUCCESSFUL OUTCOME		PDUSessionResourceModifyConfirm
	PROCEDURE CODE			id-PDUSessionResourceModifyIndication
	CRITICALITY				reject
}

pDUSessionResourceNotify NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PDUSessionResourceNotify
	PROCEDURE CODE			id-PDUSessionResourceNotify
	CRITICALITY				ignore
}

pDUSessionResourceRelease NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PDUSessionResourceReleaseCommand
	SUCCESSFUL OUTCOME		PDUSessionResourceReleaseResponse
	PROCEDURE CODE			id-PDUSessionResourceRelease
	CRITICALITY				reject
}

pDUSessionResourceSetup NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PDUSessionResourceSetupRequest
	SUCCESSFUL OUTCOME		PDUSessionResourceSetupResponse
	PROCEDURE CODE			id-PDUSessionResourceSetup
	CRITICALITY				reject
}

privateMessage NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PrivateMessage
	PROCEDURE CODE			id-PrivateMessage
	CRITICALITY				ignore
}

pWSCancel NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PWSCancelRequest
	SUCCESSFUL OUTCOME		PWSCancelResponse
	PROCEDURE CODE			id-PWSCancel
	CRITICALITY				reject
}

pWSFailureIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PWSFailureIndication
	PROCEDURE CODE			id-PWSFailureIndication
	CRITICALITY				ignore
}

pWSRestartIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PWSRestartIndication
	PROCEDURE CODE			id-PWSRestartIndication
	CRITICALITY				ignore
}

rANConfigurationUpdate NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		RANConfigurationUpdate
	SUCCESSFUL OUTCOME		RANConfigurationUpdateAcknowledge
	UNSUCCESSFUL OUTCOME	RANConfigurationUpdateFailure
	PROCEDURE CODE			id-RANConfigurationUpdate
	CRITICALITY				reject
}

rerouteNASRequest NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		RerouteNASRequest
	PROCEDURE CODE			id-RerouteNASRequest
	CRITICALITY				reject
}

rRCInactiveTransitionReport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		RRCInactiveTransitionReport
	PROCEDURE CODE			id-RRCInactiveTransitionReport
	CRITICALITY				ignore
}

secondaryRATDataUsageReport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		SecondaryRATDataUsageReport
	PROCEDURE CODE			id-SecondaryRATDataUsageReport
	CRITICALITY				ignore
}

traceFailureIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		TraceFailureIndication
	PROCEDURE CODE			id-TraceFailureIndication
	CRITICALITY				ignore
}

traceStart NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		TraceStart
	PROCEDURE CODE			id-TraceStart
	CRITICALITY				ignore
}

uEContextModification NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UEContextModificationRequest
	SUCCESSFUL OUTCOME		UEContextModificationResponse
	UNSUCCESSFUL OUTCOME	UEContextModificationFailure
	PROCEDURE CODE			id-UEContextModification
	CRITICALITY				reject
}

uEContextRelease NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UEContextReleaseCommand
	SUCCESSFUL OUTCOME		UEContextReleaseComplete
	PROCEDURE CODE			id-UEContextRelease
	CRITICALITY				reject
}

uEContextReleaseRequest NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UEContextReleaseRequest
	PROCEDURE CODE			id-UEContextReleaseRequest
	CRITICALITY				ignore
}

uERadioCapabilityCheck NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UERadioCapabilityCheckRequest
	SUCCESSFUL OUTCOME		UERadioCapabilityCheckResponse
	PROCEDURE CODE			id-UERadioCapabilityCheck
	CRITICALITY				reject
}

uERadioCapabilityInfoIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UERadioCapabilityInfoIndication
	PROCEDURE CODE			id-UERadioCapabilityInfoIndication
	CRITICALITY				ignore
}

uETNLABindingRelease NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UETNLABindingReleaseRequest
	PROCEDURE CODE			id-UETNLABindingRelease
	CRITICALITY				ignore
}

uplinkNASTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkNASTransport
	PROCEDURE CODE			id-UplinkNASTransport
	CRITICALITY				ignore
}

uplinkNonUEAssociatedNRPPaTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkNonUEAssociatedNRPPaTransport
	PROCEDURE CODE			id-UplinkNonUEAssociatedNRPPaTransport
	CRITICALITY				ignore
}

uplinkRANConfigurationTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkRANConfigurationTransfer
	PROCEDURE CODE			id-UplinkRANConfigurationTransfer
	CRITICALITY				ignore
}

uplinkRANStatusTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkRANStatusTransfer
	PROCEDURE CODE			id-UplinkRANStatusTransfer
	CRITICALITY				ignore
}

uplinkUEAssociatedNRPPaTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkUEAssociatedNRPPaTransport
	PROCEDURE CODE			id-UplinkUEAssociatedNRPPaTransport
	CRITICALITY				ignore
}

writeReplaceWarning NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		WriteReplaceWarningRequest
	SUCCESSFUL OUTCOME		WriteReplaceWarningResponse
	PROCEDURE CODE			id-WriteReplaceWarning
	CRITICALITY				reject
}

END
-- ASN1STOP

-- ASN1START
-- **************************************************************
--
-- PDU definitions for NGAP.
--
-- **************************************************************

NGAP-PDU-Contents { 
itu-t (0) identified-organization (4) etsi (0) mobileDomain (0) 
ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::= 

BEGIN

-- **************************************************************
--
-- IE parameter types from other modules.
--
-- **************************************************************

IMPORTS

	AllowedNSSAI,
	AMFName,
	AMFSetID,
	AMF-TNLAssociationSetupList,
	AMF-TNLAssociationToAddList,
	AMF-TNLAssociationToRemoveList,
	AMF-TNLAssociationToUpdateList,
	AMF-UE-NGAP-ID,
	AssistanceDataForPaging,
	BroadcastCancelledAreaList,
	BroadcastCompletedAreaList,
	CancelAllWarningMessages,
	Cause,
	CellIDListForRestart,
	CNAssistedRANTuning,
	ConcurrentWarningMessageInd,
	CoreNetworkAssistanceInformationForInactive,
	CPTransportLayerInformation,
	CriticalityDiagnostics,
	DataCodingScheme,
	DirectForwardingPathAvailability,
	EmergencyAreaIDListForRestart,
	EmergencyFallbackIndicator,
	EN-DCSONConfigurationTransfer,
	EUTRA-CGI,
	FiveG-S-TMSI,
	GlobalRANNodeID,
	GUAMI,
	HandoverFlag,
	HandoverType,
	IMSVoiceSupportIndicator,
	IndexToRFSP,
	InfoOnRecommendedCellsAndRANNodesForPaging,
	LocationReportingRequestType,
	MaskedIMEISV,
	MessageIdentifier,
	MobilityRestrictionList,
	NAS-PDU,
	NASSecurityParametersFromNGRAN,
	NewSecurityContextInd,
	NGRAN-CGI,
	NGRAN-TNLAssociationToRemoveList,
	NGRANTraceID,
	NR-CGI,
	NRPPa-PDU,
	NumberOfBroadcastsRequested,
	OverloadResponse,
	OverloadStartNSSAIList,
	PagingDRX,
	PagingOrigin,
	PagingPriority,
	PDUSessionAggregateMaximumBitRate,
	PDUSessionResourceAdmittedList,
	PDUSessionResourceFailedToModifyListModCfm,
	PDUSessionResourceFailedToModifyListModRes,
	PDUSessionResourceFailedToSetupListCxtFail,
	PDUSessionResourceFailedToSetupListCxtRes,
	PDUSessionResourceFailedToSetupListHOAck,
	PDUSessionResourceFailedToSetupListPSReq,
	PDUSessionResourceFailedToSetupListSURes,
	PDUSessionResourceHandoverList,
	PDUSessionResourceListCxtRelCpl,
	PDUSessionResourceListCxtRelReq,
	PDUSessionResourceListHORqd,
	PDUSessionResourceModifyListModCfm,
	PDUSessionResourceModifyListModInd,
	PDUSessionResourceModifyListModReq,
	PDUSessionResourceModifyListModRes,
	PDUSessionResourceNotifyList,
	PDUSessionResourceReleasedListNot,
	PDUSessionResourceReleasedListPSAck,
	PDUSessionResourceReleasedListPSFail,
	PDUSessionResourceReleasedListRelRes,
	PDUSessionResourceSecondaryRATUsageList,
	PDUSessionResourceSetupListCxtReq,
	PDUSessionResourceSetupListCxtRes,
	PDUSessionResourceSetupListHOReq,
	PDUSessionResourceSetupListSUReq,
	PDUSessionResourceSetupListSURes,
	PDUSessionResourceSwitchedList,
	PDUSessionResourceToBeSwitchedDLList,
	PDUSessionResourceToReleaseListHOCmd,
	PDUSessionResourceToReleaseListRelCmd,
	PLMNIdentity,
	PLMNSupportList,
	PWSFailedCellIDList,
	RANNodeName,
	RANPagingPriority,
	RANStatusTransfer-TransparentContainer,
	RAN-UE-NGAP-ID,
	RedirectionVoiceFallback,
	RelativeAMFCapacity,
	RepetitionPeriod,
	ResetType,
	RoutingID,
	RRCEstablishmentCause,
	RRCInactiveTransitionReportRequest,
	RRCState,
	SecurityContext,
	SecurityKey,
	SerialNumber,
	ServedGUAMIList,
	SliceSupportList,
	S-NSSAI,
	SONConfigurationTransfer,
	SourceToTarget-TransparentContainer,
	SourceToTarget-AMFInformationReroute,
	SupportedTAList,
	TAIListForPaging,
	TAIListForRestart,
	TargetID,
	TargetToSource-TransparentContainer,
	TimeToWait,
	TNLAssociationList,
	TraceActivation,
	TrafficLoadReductionIndication,
	TransportLayerAddress,
	UEAggregateMaximumBitRate,
	UE-associatedLogicalNG-connectionList,
	UEContextRequest,
	UE-NGAP-IDs,
	UEPagingIdentity,
	UEPresenceInAreaOfInterestList,
	UERadioCapability,
	UERadioCapabilityForPaging,
	UERetentionInformation,
	UESecurityCapabilities,
	UnavailableGUAMIList,
	UserLocationInformation,
	WarningAreaCoordinates,
	WarningAreaList,
	WarningMessageContents,
	WarningSecurityInfo,
	WarningType

FROM NGAP-IEs

	PrivateIE-Container{},
	ProtocolExtensionContainer{},
	ProtocolIE-Container{},
	ProtocolIE-ContainerList{},
	ProtocolIE-ContainerPair{},
	ProtocolIE-SingleContainer{},
	NGAP-PRIVATE-IES,
	NGAP-PROTOCOL-EXTENSION,
	NGAP-PROTOCOL-IES,
	NGAP-PROTOCOL-IES-PAIR
FROM NGAP-Containers

	id-AllowedNSSAI,
	id-AMFName,
	id-AMFOverloadResponse,
	id-AMFSetID,
	id-AMF-TNLAssociationFailedToSetupList,
	id-AMF-TNLAssociationSetupList,
	id-AMF-TNLAssociationToAddList,
	id-AMF-TNLAssociationToRemoveList,
	id-AMF-TNLAssociationToUpdateList,
	id-AMFTrafficLoadReductionIndication,
	id-AMF-UE-NGAP-ID,
	id-AssistanceDataForPaging,
	id-BroadcastCancelledAreaList,
	id-BroadcastCompletedAreaList,
	id-CancelAllWarningMessages,
	id-Cause,
	id-CellIDListForRestart,
	id-CNAssistedRANTuning,
	id-ConcurrentWarningMessageInd,
	id-CoreNetworkAssistanceInformationForInactive,
	id-CriticalityDiagnostics,
	id-DataCodingScheme,
	id-DefaultPagingDRX,
	id-DirectForwardingPathAvailability,
	id-EmergencyAreaIDListForRestart,
	id-EmergencyFallbackIndicator,
	id-ENDC-SONConfigurationTransferDL,
	id-ENDC-SONConfigurationTransferUL,
	id-EUTRA-CGI,
	id-FiveG-S-TMSI,
	id-GlobalRANNodeID,
	id-GUAMI,
	id-HandoverFlag,
	id-HandoverType,
	id-IMSVoiceSupportIndicator,
	id-IndexToRFSP,
	id-InfoOnRecommendedCellsAndRANNodesForPaging,
	id-LocationReportingRequestType,
	id-MaskedIMEISV,
	id-MessageIdentifier,
	id-MobilityRestrictionList,
	id-NAS-PDU,
	id-NASC,
	id-NASSecurityParametersFromNGRAN,
	id-NewAMF-UE-NGAP-ID,
	id-NewGUAMI,
	id-NewSecurityContextInd,
	id-NGAP-Message,
	id-NGRAN-CGI,
	id-NGRAN-TNLAssociationToRemoveList,
	id-NGRANTraceID,
	id-NR-CGI,
	id-NRPPa-PDU,
	id-NumberOfBroadcastsRequested,
	id-OldAMF,
	id-OverloadStartNSSAIList,
	id-PagingDRX,
	id-PagingOrigin,
	id-PagingPriority,
	id-PDUSessionResourceAdmittedList,
	id-PDUSessionResourceFailedToModifyListModCfm,
	id-PDUSessionResourceFailedToModifyListModRes,
	id-PDUSessionResourceFailedToSetupListCxtFail,
	id-PDUSessionResourceFailedToSetupListCxtRes,
	id-PDUSessionResourceFailedToSetupListHOAck,
	id-PDUSessionResourceFailedToSetupListPSReq,
	id-PDUSessionResourceFailedToSetupListSURes,
	id-PDUSessionResourceHandoverList,
	id-PDUSessionResourceListCxtRelCpl,
	id-PDUSessionResourceListCxtRelReq,
	id-PDUSessionResourceListHORqd,
	id-PDUSessionResourceModifyListModCfm,
	id-PDUSessionResourceModifyListModInd,
	id-PDUSessionResourceModifyListModReq,
	id-PDUSessionResourceModifyListModRes,
	id-PDUSessionResourceNotifyList,
	id-PDUSessionResourceReleasedListNot,
	id-PDUSessionResourceReleasedListPSAck,
	id-PDUSessionResourceReleasedListPSFail,
	id-PDUSessionResourceReleasedListRelRes,
	id-PDUSessionResourceSecondaryRATUsageList,
	id-PDUSessionResourceSetupListCxtReq,
	id-PDUSessionResourceSetupListCxtRes,
	id-PDUSessionResourceSetupListHOReq,
	id-PDUSessionResourceSetupListSUReq,
	id-PDUSessionResourceSetupListSURes,
	id-PDUSessionResourceSwitchedList,
	id-PDUSessionResourceToBeSwitchedDLList,
	id-PDUSessionResourceToReleaseListHOCmd,
	id-PDUSessionResourceToReleaseListRelCmd,
	id-PLMNSupportList,
	id-PWSFailedCellIDList,
	id-RANNodeName,
	id-RANPagingPriority,
	id-RANStatusTransfer-TransparentContainer,
	id-RAN-UE-NGAP-ID, 
	id-RedirectionVoiceFallback,
	id-RelativeAMFCapacity,
	id-RepetitionPeriod,
	id-ResetType,
	id-RoutingID,
	id-RRCEstablishmentCause,
	id-RRCInactiveTransitionReportRequest,
	id-RRCState,
	id-SecurityContext,
	id-SecurityKey,
	id-SelectedPLMNIdentity,
	id-SerialNumber,
	id-ServedGUAMIList,
	id-SliceSupportList,
	id-SONConfigurationTransferDL,
	id-SONConfigurationTransferUL,
	id-SourceAMF-UE-NGAP-ID,
	id-SourceToTarget-TransparentContainer,
	id-SourceToTarget-AMFInformationReroute,
	id-SupportedTAList,
	id-TAIListForPaging,
	id-TAIListForRestart,
	id-TargetID,
	id-TargetToSource-TransparentContainer,
	id-TimeToWait,
	id-TraceActivation,
	id-TraceCollectionEntityIPAddress,
	id-UEAggregateMaximumBitRate,
	id-UE-associatedLogicalNG-connectionList,
	id-UEContextRequest,
	id-UE-NGAP-IDs,
	id-UEPagingIdentity,
	id-UEPresenceInAreaOfInterestList,
	id-UERadioCapability,
	id-UERadioCapabilityForPaging,
	id-UERetentionInformation,
	id-UESecurityCapabilities,
	id-UnavailableGUAMIList,
	id-UserLocationInformation,
	id-WarningAreaCoordinates,
	id-WarningAreaList,
	id-WarningMessageContents,
	id-WarningSecurityInfo,
	id-WarningType

FROM NGAP-Constants;

-- **************************************************************
--
-- PDU SESSION MANAGEMENT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- PDU Session Resource Setup Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PDU SESSION RESOURCE SETUP REQUEST
--
-- **************************************************************

PDUSessionResourceSetupRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceSetupRequestIEs} },
	...
}

PDUSessionResourceSetupRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-RANPagingPriority						CRITICALITY ignore	TYPE RANPagingPriority							PRESENCE optional		}|
	{ ID id-NAS-PDU									CRITICALITY reject	TYPE NAS-PDU									PRESENCE optional		}|
	{ ID id-PDUSessionResourceSetupListSUReq		CRITICALITY reject	TYPE PDUSessionResourceSetupListSUReq		PRESENCE mandatory	}|
	{ ID id-UEAggregateMaximumBitRate				CRITICALITY ignore	TYPE UEAggregateMaximumBitRate				PRESENCE optional		},
	...
}

-- **************************************************************
--
-- PDU SESSION RESOURCE SETUP RESPONSE
--
-- **************************************************************

PDUSessionResourceSetupResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceSetupResponseIEs} },
	...
}

PDUSessionResourceSetupResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceSetupListSURes			CRITICALITY ignore	TYPE PDUSessionResourceSetupListSURes				PRESENCE optional		}|
	{ ID id-PDUSessionResourceFailedToSetupListSURes	CRITICALITY ignore	TYPE PDUSessionResourceFailedToSetupListSURes		PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...	
}


-- **************************************************************
--
-- PDU Session Resource Release Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PDU SESSION RESOURCE RELEASE COMMAND
--
-- **************************************************************

PDUSessionResourceReleaseCommand ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceReleaseCommandIEs} },
	...
}

PDUSessionResourceReleaseCommandIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY reject	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RANPagingPriority							CRITICALITY ignore	TYPE RANPagingPriority								PRESENCE optional		}|
	{ ID id-NAS-PDU										CRITICALITY ignore	TYPE NAS-PDU											PRESENCE optional		}|
	{ ID id-PDUSessionResourceToReleaseListRelCmd		CRITICALITY reject	TYPE PDUSessionResourceToReleaseListRelCmd		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- PDU SESSION RESOURCE RELEASE RESPONSE
--
-- **************************************************************

PDUSessionResourceReleaseResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceReleaseResponseIEs} },
	...
}

PDUSessionResourceReleaseResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceReleasedListRelRes			CRITICALITY ignore	TYPE PDUSessionResourceReleasedListRelRes		PRESENCE mandatory	}|
	{ ID id-UserLocationInformation						CRITICALITY ignore	TYPE UserLocationInformation						PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		},
	...
}

-- **************************************************************
--
-- PDU Session Resource Modify Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PDU SESSION RESOURCE MODIFY REQUEST
--
-- **************************************************************

PDUSessionResourceModifyRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceModifyRequestIEs} },
	...
}

PDUSessionResourceModifyRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-RANPagingPriority						CRITICALITY ignore	TYPE RANPagingPriority							PRESENCE optional		}|
	{ ID id-PDUSessionResourceModifyListModReq		CRITICALITY reject	TYPE PDUSessionResourceModifyListModReq	PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- PDU SESSION RESOURCE MODIFY RESPONSE
--
-- **************************************************************

PDUSessionResourceModifyResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceModifyResponseIEs} },
	...
}

PDUSessionResourceModifyResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID									CRITICALITY ignore	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID									CRITICALITY ignore	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceModifyListModRes				CRITICALITY ignore	TYPE PDUSessionResourceModifyListModRes			PRESENCE optional		}|
	{ ID id-PDUSessionResourceFailedToModifyListModRes		CRITICALITY ignore	TYPE PDUSessionResourceFailedToModifyListModRes		PRESENCE optional	}|
	{ ID id-UserLocationInformation							CRITICALITY ignore	TYPE UserLocationInformation							PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics							CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		},
	...
}


-- **************************************************************
--
-- PDU Session Resource Notify Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PDU SESSION RESOURCE NOTIFY
--
-- **************************************************************

PDUSessionResourceNotify ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceNotifyIEs} },
	...
}

PDUSessionResourceNotifyIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceNotifyList			CRITICALITY reject	TYPE PDUSessionResourceNotifyList				PRESENCE optional		}|
	{ ID id-PDUSessionResourceReleasedListNot		CRITICALITY ignore	TYPE PDUSessionResourceReleasedListNot		PRESENCE optional		}|
	{ ID id-UserLocationInformation					CRITICALITY ignore	TYPE UserLocationInformation						PRESENCE optional		},
	...
}


-- **************************************************************
--
-- PDU Session Resource Modify Indication Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PDU SESSION RESOURCE MODIFY INDICATION
--
-- **************************************************************

PDUSessionResourceModifyIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceModifyIndicationIEs} },
	...
}

PDUSessionResourceModifyIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceModifyListModInd		CRITICALITY reject	TYPE PDUSessionResourceModifyListModInd		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- PDU SESSION RESOURCE MODIFY CONFIRM
--
-- **************************************************************

PDUSessionResourceModifyConfirm ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceModifyConfirmIEs} },
	...
}

PDUSessionResourceModifyConfirmIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceModifyListModCfm			CRITICALITY ignore	TYPE PDUSessionResourceModifyListModCfm		PRESENCE optional	}|
	{ ID id-PDUSessionResourceFailedToModifyListModCfm	CRITICALITY ignore	TYPE PDUSessionResourceFailedToModifyListModCfm		PRESENCE optional	}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics						PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE CONTEXT MANAGEMENT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- Initial Context Setup Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- INITIAL CONTEXT SETUP REQUEST
--
-- **************************************************************

InitialContextSetupRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {InitialContextSetupRequestIEs} },
	...
}

InitialContextSetupRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-OldAMF									CRITICALITY reject	TYPE AMFName											PRESENCE optional		}|
	{ ID id-UEAggregateMaximumBitRate				CRITICALITY reject	TYPE UEAggregateMaximumBitRate						PRESENCE conditional	}|
	{ ID id-CoreNetworkAssistanceInformationForInactive		CRITICALITY ignore	TYPE CoreNetworkAssistanceInformationForInactive		PRESENCE optional		}|
	{ ID id-GUAMI									CRITICALITY reject	TYPE GUAMI												PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceSetupListCxtReq		CRITICALITY reject	TYPE PDUSessionResourceSetupListCxtReq			PRESENCE optional		}|
	{ ID id-AllowedNSSAI							CRITICALITY reject	TYPE AllowedNSSAI										PRESENCE mandatory	}|
	{ ID id-UESecurityCapabilities					CRITICALITY reject	TYPE UESecurityCapabilities							PRESENCE mandatory	}|
	{ ID id-SecurityKey								CRITICALITY reject	TYPE SecurityKey										PRESENCE mandatory	}|
	{ ID id-TraceActivation							CRITICALITY ignore	TYPE TraceActivation									PRESENCE optional		}|
	{ ID id-MobilityRestrictionList					CRITICALITY ignore	TYPE MobilityRestrictionList							PRESENCE optional		}|
	{ ID id-UERadioCapability						CRITICALITY ignore	TYPE UERadioCapability									PRESENCE optional		}|
	{ ID id-IndexToRFSP								CRITICALITY ignore	TYPE IndexToRFSP										PRESENCE optional		}|
	{ ID id-MaskedIMEISV							CRITICALITY ignore	TYPE MaskedIMEISV										PRESENCE optional		}|
	{ ID id-NAS-PDU									CRITICALITY ignore	TYPE NAS-PDU											PRESENCE optional		}|
	{ ID id-EmergencyFallbackIndicator				CRITICALITY reject	TYPE EmergencyFallbackIndicator						PRESENCE optional		}|
	{ ID id-RRCInactiveTransitionReportRequest		CRITICALITY ignore	TYPE RRCInactiveTransitionReportRequest			PRESENCE optional		}|
	{ ID id-UERadioCapabilityForPaging				CRITICALITY ignore	TYPE UERadioCapabilityForPaging						PRESENCE optional		}|
	{ ID id-RedirectionVoiceFallback				CRITICALITY ignore	TYPE RedirectionVoiceFallback						PRESENCE optional		}|
	{ ID id-LocationReportingRequestType			CRITICALITY ignore	TYPE LocationReportingRequestType					PRESENCE optional		}|
	{ ID id-CNAssistedRANTuning						CRITICALITY ignore	TYPE CNAssistedRANTuning								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- INITIAL CONTEXT SETUP RESPONSE
--
-- **************************************************************

InitialContextSetupResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {InitialContextSetupResponseIEs} },
	...
}

InitialContextSetupResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceSetupListCxtRes			CRITICALITY ignore	TYPE PDUSessionResourceSetupListCxtRes					PRESENCE optional		}|
	{ ID id-PDUSessionResourceFailedToSetupListCxtRes	CRITICALITY ignore	TYPE PDUSessionResourceFailedToSetupListCxtRes		PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics									PRESENCE optional		},
	...
}


-- **************************************************************
--
-- INITIAL CONTEXT SETUP FAILURE
--
-- **************************************************************

InitialContextSetupFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {InitialContextSetupFailureIEs} },
	...
}

InitialContextSetupFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceFailedToSetupListCxtFail	CRITICALITY ignore	TYPE PDUSessionResourceFailedToSetupListCxtFail		PRESENCE optional		}|
	{ ID id-Cause										CRITICALITY ignore	TYPE Cause														PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics									PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE Context Release Request Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UE CONTEXT RELEASE REQUEST
--
-- **************************************************************

UEContextReleaseRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextReleaseRequest-IEs} },
	...
}

UEContextReleaseRequest-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID						CRITICALITY reject	TYPE AMF-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID						CRITICALITY reject	TYPE RAN-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceListCxtRelReq		CRITICALITY reject	TYPE PDUSessionResourceListCxtRelReq		PRESENCE optional		}|
	{ ID id-Cause								CRITICALITY ignore	TYPE Cause										PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UE Context Release Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UE CONTEXT RELEASE COMMAND
--
-- **************************************************************

UEContextReleaseCommand ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextReleaseCommand-IEs} },
	...
}

UEContextReleaseCommand-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-UE-NGAP-IDs				CRITICALITY reject	TYPE UE-NGAP-IDs			PRESENCE mandatory	}|
	{ ID id-Cause					CRITICALITY ignore	TYPE Cause					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UE CONTEXT RELEASE COMPLETE
--
-- **************************************************************

UEContextReleaseComplete ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextReleaseComplete-IEs} },
	...
}

UEContextReleaseComplete-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-UserLocationInformation						CRITICALITY ignore	TYPE UserLocationInformation							PRESENCE optional		}|
	{ ID id-InfoOnRecommendedCellsAndRANNodesForPaging	CRITICALITY ignore	TYPE InfoOnRecommendedCellsAndRANNodesForPaging	PRESENCE optional		}|
	{ ID id-PDUSessionResourceListCxtRelCpl				CRITICALITY	reject	TYPE PDUSessionResourceListCxtRelCpl					PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE Context Modification Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UE CONTEXT MODIFICATION REQUEST
--
-- **************************************************************

UEContextModificationRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextModificationRequestIEs} },
	...
}

UEContextModificationRequestIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RANPagingPriority						CRITICALITY ignore	TYPE RANPagingPriority								PRESENCE optional		}|
	{ ID id-SecurityKey								CRITICALITY reject	TYPE SecurityKey									PRESENCE optional		}|
	{ ID id-IndexToRFSP								CRITICALITY ignore	TYPE IndexToRFSP									PRESENCE optional		}|
	{ ID id-UEAggregateMaximumBitRate				CRITICALITY ignore	TYPE UEAggregateMaximumBitRate					PRESENCE optional		}|
	{ ID id-UESecurityCapabilities					CRITICALITY reject	TYPE UESecurityCapabilities						PRESENCE optional		}|
	{ ID id-CoreNetworkAssistanceInformationForInactive		CRITICALITY ignore	TYPE CoreNetworkAssistanceInformationForInactive			PRESENCE optional		}|
	{ ID id-EmergencyFallbackIndicator				CRITICALITY reject	TYPE EmergencyFallbackIndicator					PRESENCE optional		}|
	{ ID id-NewAMF-UE-NGAP-ID						CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE optional		}|
	{ ID id-RRCInactiveTransitionReportRequest		CRITICALITY ignore	TYPE RRCInactiveTransitionReportRequest		PRESENCE optional		}|
	{ ID id-NewGUAMI								CRITICALITY reject	TYPE GUAMI											PRESENCE optional		}|
	{ ID id-CNAssistedRANTuning						CRITICALITY ignore	TYPE CNAssistedRANTuning							PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE CONTEXT MODIFICATION RESPONSE
--
-- **************************************************************

UEContextModificationResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextModificationResponseIEs} },
	...
}

UEContextModificationResponseIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RRCState					CRITICALITY ignore	TYPE RRCState					PRESENCE optional		}|
	{ ID id-UserLocationInformation		CRITICALITY ignore	TYPE UserLocationInformation	PRESENCE optional 	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE CONTEXT MODIFICATION FAILURE
--
-- **************************************************************

UEContextModificationFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextModificationFailureIEs} },
	...
}

UEContextModificationFailureIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- RRC INACTIVE TRANSITION REPORT
--
-- **************************************************************

RRCInactiveTransitionReport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {RRCInactiveTransitionReportIEs} },
	...
}

RRCInactiveTransitionReportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RRCState					CRITICALITY ignore	TYPE RRCState						PRESENCE mandatory	}|
	{ ID id-UserLocationInformation		CRITICALITY ignore	TYPE UserLocationInformation		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UE MOBILITY MANAGEMENT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- Handover Preparation Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- HANDOVER REQUIRED
--
-- **************************************************************

HandoverRequired ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {HandoverRequiredIEs} },
	...
}

HandoverRequiredIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-HandoverType							CRITICALITY reject	TYPE HandoverType									PRESENCE mandatory	}|
	{ ID id-Cause									CRITICALITY ignore	TYPE Cause											PRESENCE mandatory	}|
	{ ID id-TargetID								CRITICALITY reject	TYPE TargetID										PRESENCE mandatory	}|
	{ ID id-DirectForwardingPathAvailability		CRITICALITY ignore	TYPE DirectForwardingPathAvailability			PRESENCE optional		}|
	{ ID id-PDUSessionResourceListHORqd				CRITICALITY reject	TYPE PDUSessionResourceListHORqd				PRESENCE mandatory	}|
	{ ID id-SourceToTarget-TransparentContainer		CRITICALITY reject	TYPE SourceToTarget-TransparentContainer		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- HANDOVER COMMAND
--
-- **************************************************************

HandoverCommand ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {HandoverCommandIEs} },
	...
}

HandoverCommandIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY reject	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-HandoverType								CRITICALITY reject	TYPE HandoverType											PRESENCE mandatory	}|
	{ ID id-NASSecurityParametersFromNGRAN				CRITICALITY reject	TYPE NASSecurityParametersFromNGRAN					PRESENCE conditional	}|
	-- This IE shall be present if HandoverType IE is set to value "5GStoEPPS" --
	{ ID id-PDUSessionResourceHandoverList				CRITICALITY ignore	TYPE PDUSessionResourceHandoverList					PRESENCE optional	}|
	{ ID id-PDUSessionResourceToReleaseListHOCmd		CRITICALITY ignore	TYPE PDUSessionResourceToReleaseListHOCmd			PRESENCE optional		}|
	{ ID id-TargetToSource-TransparentContainer			CRITICALITY reject	TYPE TargetToSource-TransparentContainer			PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}


-- **************************************************************
--
-- HANDOVER PREPARATION FAILURE
--
-- **************************************************************

HandoverPreparationFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {HandoverPreparationFailureIEs} },
	...
}

HandoverPreparationFailureIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Handover Resource Allocation Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- HANDOVER REQUEST
--
-- **************************************************************

HandoverRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {HandoverRequestIEs} },
	...
}

HandoverRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-HandoverType							CRITICALITY reject	TYPE HandoverType									PRESENCE mandatory	}|
	{ ID id-Cause									CRITICALITY ignore	TYPE Cause											PRESENCE mandatory	}|
	{ ID id-UEAggregateMaximumBitRate				CRITICALITY reject	TYPE UEAggregateMaximumBitRate					PRESENCE mandatory	}|
	{ ID id-CoreNetworkAssistanceInformationForInactive		CRITICALITY ignore	TYPE CoreNetworkAssistanceInformationForInactive			PRESENCE optional		}|
	{ ID id-UESecurityCapabilities					CRITICALITY reject	TYPE UESecurityCapabilities						PRESENCE mandatory	}|
	{ ID id-SecurityContext							CRITICALITY reject	TYPE SecurityContext								PRESENCE mandatory	}|
	{ ID id-NewSecurityContextInd					CRITICALITY reject	TYPE NewSecurityContextInd						PRESENCE optional		}|
	{ ID id-NASC									CRITICALITY reject	TYPE NAS-PDU										PRESENCE optional		}|
	{ ID id-PDUSessionResourceSetupListHOReq		CRITICALITY reject	TYPE PDUSessionResourceSetupListHOReq			PRESENCE mandatory	}|
	{ ID id-AllowedNSSAI							CRITICALITY reject	TYPE AllowedNSSAI									PRESENCE mandatory	}|
	{ ID id-TraceActivation							CRITICALITY ignore	TYPE TraceActivation								PRESENCE optional		}|
	{ ID id-MaskedIMEISV							CRITICALITY ignore	TYPE MaskedIMEISV									PRESENCE optional		}|
	{ ID id-SourceToTarget-TransparentContainer		CRITICALITY reject	TYPE SourceToTarget-TransparentContainer		PRESENCE mandatory	}|
	{ ID id-MobilityRestrictionList					CRITICALITY ignore	TYPE MobilityRestrictionList						PRESENCE optional		}|
	{ ID id-LocationReportingRequestType			CRITICALITY ignore	TYPE LocationReportingRequestType				PRESENCE optional		}|
	{ ID id-RRCInactiveTransitionReportRequest		CRITICALITY ignore	TYPE RRCInactiveTransitionReportRequest		PRESENCE optional		}|
	{ ID id-GUAMI									CRITICALITY reject	TYPE GUAMI											PRESENCE mandatory	}|
	{ ID id-RedirectionVoiceFallback				CRITICALITY ignore	TYPE RedirectionVoiceFallback					PRESENCE optional		}|
	{ ID id-CNAssistedRANTuning						CRITICALITY ignore	TYPE CNAssistedRANTuning							PRESENCE optional		},
	...
}

-- **************************************************************
--
-- HANDOVER REQUEST ACKNOWLEDGE
--
-- **************************************************************

HandoverRequestAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {HandoverRequestAcknowledgeIEs} },
	...
}

HandoverRequestAcknowledgeIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceAdmittedList				CRITICALITY ignore	TYPE PDUSessionResourceAdmittedList					PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceFailedToSetupListHOAck	CRITICALITY ignore	TYPE PDUSessionResourceFailedToSetupListHOAck		PRESENCE optional		}|
	{ ID id-TargetToSource-TransparentContainer			CRITICALITY reject	TYPE TargetToSource-TransparentContainer			PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}


-- **************************************************************
--
-- HANDOVER FAILURE
--
-- **************************************************************

HandoverFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { HandoverFailureIEs} },
	...
}

HandoverFailureIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Handover Notification Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- HANDOVER NOTIFY
--
-- **************************************************************

HandoverNotify ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { HandoverNotifyIEs} },
	...
}

HandoverNotifyIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-UserLocationInformation		CRITICALITY ignore	TYPE UserLocationInformation	PRESENCE mandatory		},
	...
}

-- **************************************************************
--
-- Path Switch Request Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PATH SWITCH REQUEST
--
-- **************************************************************

PathSwitchRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { PathSwitchRequestIEs} },
	...
}

PathSwitchRequestIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-SourceAMF-UE-NGAP-ID						CRITICALITY reject	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-UserLocationInformation						CRITICALITY ignore	TYPE UserLocationInformation							PRESENCE mandatory	}|
	{ ID id-UESecurityCapabilities						CRITICALITY ignore	TYPE UESecurityCapabilities								PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceToBeSwitchedDLList		CRITICALITY reject	TYPE PDUSessionResourceToBeSwitchedDLList			PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceFailedToSetupListPSReq	CRITICALITY ignore	TYPE PDUSessionResourceFailedToSetupListPSReq		PRESENCE optional		},
	...
}


-- **************************************************************
--
-- PATH SWITCH REQUEST ACKNOWLEDGE
--
-- **************************************************************

PathSwitchRequestAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { PathSwitchRequestAcknowledgeIEs} },
	...
}

PathSwitchRequestAcknowledgeIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-UESecurityCapabilities						CRITICALITY reject	TYPE UESecurityCapabilities							PRESENCE optional		}|
	{ ID id-SecurityContext								CRITICALITY reject	TYPE SecurityContext									PRESENCE mandatory	}|
	{ ID id-NewSecurityContextInd						CRITICALITY reject	TYPE NewSecurityContextInd							PRESENCE optional		}|
	{ ID id-PDUSessionResourceSwitchedList				CRITICALITY ignore	TYPE PDUSessionResourceSwitchedList				PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceReleasedListPSAck			CRITICALITY ignore	TYPE PDUSessionResourceReleasedListPSAck		PRESENCE optional		}|
	{ ID id-AllowedNSSAI								CRITICALITY reject	TYPE AllowedNSSAI										PRESENCE mandatory	}|
	{ ID id-CoreNetworkAssistanceInformationForInactive			CRITICALITY ignore	TYPE CoreNetworkAssistanceInformationForInactive			PRESENCE optional		}|
	{ ID id-RRCInactiveTransitionReportRequest			CRITICALITY ignore	TYPE RRCInactiveTransitionReportRequest			PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		}|
	{ ID id-RedirectionVoiceFallback					CRITICALITY ignore	TYPE RedirectionVoiceFallback						PRESENCE optional		}|
	{ ID id-CNAssistedRANTuning							CRITICALITY ignore	TYPE CNAssistedRANTuning								PRESENCE optional		},
	...
}


-- **************************************************************
--
-- PATH SWITCH REQUEST FAILURE
--
-- **************************************************************

PathSwitchRequestFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { PathSwitchRequestFailureIEs} },
	...
}

PathSwitchRequestFailureIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY ignore	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY ignore	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceReleasedListPSFail	CRITICALITY ignore	TYPE PDUSessionResourceReleasedListPSFail	PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics					CRITICALITY ignore	TYPE CriticalityDiagnostics						PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Handover Cancellation Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- HANDOVER CANCEL
--
-- **************************************************************

HandoverCancel ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { HandoverCancelIEs} },
	...
}

HandoverCancelIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID		CRITICALITY reject	TYPE AMF-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID		CRITICALITY reject	TYPE RAN-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-Cause				CRITICALITY ignore	TYPE Cause				PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- HANDOVER CANCEL ACKNOWLEDGE
--
-- **************************************************************

HandoverCancelAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { HandoverCancelAcknowledgeIEs} },
	...
}

HandoverCancelAcknowledgeIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional	},
	...
}

-- **************************************************************
--
-- Uplink RAN Status Transfer Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UPLINK RAN STATUS TRANSFER
--
-- **************************************************************

UplinkRANStatusTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UplinkRANStatusTransferIEs} },
	...
}

UplinkRANStatusTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY reject	TYPE AMF-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-RANStatusTransfer-TransparentContainer		CRITICALITY reject	TYPE RANStatusTransfer-TransparentContainer	PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- Downlink RAN Status Transfer Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- DOWNLINK RAN STATUS TRANSFER
--
-- **************************************************************

DownlinkRANStatusTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DownlinkRANStatusTransferIEs} },
	...
}

DownlinkRANStatusTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY reject	TYPE AMF-UE-NGAP-ID			PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID			PRESENCE mandatory	}|
	{ ID id-RANStatusTransfer-TransparentContainer		CRITICALITY reject	TYPE RANStatusTransfer-TransparentContainer		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- PAGING ELEMENTARY PROCEDURE
--
-- **************************************************************

-- **************************************************************
--
-- PAGING
--
-- **************************************************************

Paging ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PagingIEs} },
	...
}

PagingIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-UEPagingIdentity				CRITICALITY ignore	TYPE UEPagingIdentity				PRESENCE mandatory	}|
	{ ID id-PagingDRX						CRITICALITY ignore	TYPE PagingDRX						PRESENCE optional		}|
	{ ID id-TAIListForPaging				CRITICALITY ignore	TYPE TAIListForPaging				PRESENCE mandatory	}|
	{ ID id-PagingPriority					CRITICALITY ignore	TYPE PagingPriority					PRESENCE optional		}|
	{ ID id-UERadioCapabilityForPaging		CRITICALITY ignore	TYPE UERadioCapabilityForPaging		PRESENCE optional		}|
	{ ID id-PagingOrigin					CRITICALITY ignore	TYPE PagingOrigin					PRESENCE optional		}|
	{ ID id-AssistanceDataForPaging			CRITICALITY ignore	TYPE AssistanceDataForPaging		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- NAS TRANSPORT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- INITIAL UE MESSAGE
--
-- **************************************************************

InitialUEMessage ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {InitialUEMessage-IEs} },
	...
}

InitialUEMessage-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-NAS-PDU									CRITICALITY reject	TYPE NAS-PDU										PRESENCE mandatory	}|
	{ ID id-UserLocationInformation					CRITICALITY reject	TYPE UserLocationInformation						PRESENCE mandatory	}|
	{ ID id-RRCEstablishmentCause					CRITICALITY ignore	TYPE RRCEstablishmentCause						PRESENCE mandatory	}|
	{ ID id-FiveG-S-TMSI							CRITICALITY reject	TYPE FiveG-S-TMSI									PRESENCE optional		}|
	{ ID id-AMFSetID								CRITICALITY ignore	TYPE AMFSetID										PRESENCE optional		}|
	{ ID id-UEContextRequest						CRITICALITY ignore	TYPE UEContextRequest								PRESENCE optional		}|
	{ ID id-AllowedNSSAI							CRITICALITY reject	TYPE AllowedNSSAI									PRESENCE optional		}|
	{ ID id-SourceToTarget-AMFInformationReroute	CRITICALITY ignore	TYPE SourceToTarget-AMFInformationReroute	PRESENCE optional		}|
	{ ID id-SelectedPLMNIdentity					CRITICALITY ignore	TYPE PLMNIdentity									PRESENCE optional		},
	...
}

-- **************************************************************
--
-- DOWNLINK NAS TRANSPORT
--
-- **************************************************************

DownlinkNASTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DownlinkNASTransport-IEs} },
	...
}

DownlinkNASTransport-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID					CRITICALITY reject	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY reject	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-OldAMF							CRITICALITY reject	TYPE AMFName						PRESENCE optional		}|
	{ ID id-RANPagingPriority				CRITICALITY ignore	TYPE RANPagingPriority				PRESENCE optional		}|
	{ ID id-NAS-PDU							CRITICALITY reject	TYPE NAS-PDU						PRESENCE mandatory	}|
	{ ID id-MobilityRestrictionList			CRITICALITY ignore	TYPE MobilityRestrictionList		PRESENCE optional		}|
	{ ID id-IndexToRFSP						CRITICALITY ignore	TYPE IndexToRFSP					PRESENCE optional		}|
	{ ID id-UEAggregateMaximumBitRate		CRITICALITY ignore	TYPE UEAggregateMaximumBitRate		PRESENCE optional		}|
	{ ID id-AllowedNSSAI					CRITICALITY reject	TYPE AllowedNSSAI					PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UPLINK NAS TRANSPORT
--
-- **************************************************************

UplinkNASTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container	{ {UplinkNASTransport-IEs} },
	...
}

UplinkNASTransport-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-NAS-PDU						CRITICALITY reject	TYPE NAS-PDU						PRESENCE mandatory	}|
	{ ID id-UserLocationInformation		CRITICALITY ignore	TYPE UserLocationInformation		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- NAS NON DELIVERY INDICATION
--
-- **************************************************************

NASNonDeliveryIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NASNonDeliveryIndication-IEs} },
	...
}

NASNonDeliveryIndication-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID		CRITICALITY reject	TYPE AMF-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID		CRITICALITY reject	TYPE RAN-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-NAS-PDU				CRITICALITY ignore	TYPE NAS-PDU			PRESENCE mandatory	}|
	{ ID id-Cause				CRITICALITY ignore	TYPE Cause				PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- REROUTE NAS REQUEST
--
-- **************************************************************

RerouteNASRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {RerouteNASRequest-IEs} },
	...
}

RerouteNASRequest-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY ignore	TYPE AMF-UE-NGAP-ID									PRESENCE optional	}|
	{ ID id-NGAP-Message							CRITICALITY reject	TYPE OCTET STRING									PRESENCE mandatory	}|
	{ ID id-AMFSetID								CRITICALITY reject	TYPE AMFSetID										PRESENCE mandatory	}|
	{ ID id-AllowedNSSAI							CRITICALITY reject	TYPE AllowedNSSAI									PRESENCE optional	}|
	{ ID id-SourceToTarget-AMFInformationReroute	CRITICALITY ignore	TYPE SourceToTarget-AMFInformationReroute	PRESENCE optional },
	...
}

-- **************************************************************
--
-- INTERFACE MANAGEMENT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- NG Setup Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- NG SETUP REQUEST
--
-- **************************************************************

NGSetupRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGSetupRequestIEs} },
	...
}

NGSetupRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-GlobalRANNodeID			CRITICALITY reject	TYPE GlobalRANNodeID			PRESENCE mandatory	}|
	{ ID id-RANNodeName				CRITICALITY ignore	TYPE RANNodeName				PRESENCE optional}|
	{ ID id-SupportedTAList			CRITICALITY reject	TYPE SupportedTAList			PRESENCE mandatory	}|
	{ ID id-DefaultPagingDRX		CRITICALITY ignore	TYPE PagingDRX					PRESENCE mandatory	}|
	{ ID id-UERetentionInformation	CRITICALITY ignore	TYPE UERetentionInformation		PRESENCE optional	},
	...
}

-- **************************************************************
--
-- NG SETUP RESPONSE
--
-- **************************************************************

NGSetupResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGSetupResponseIEs} },
	...
}

NGSetupResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMFName						CRITICALITY reject	TYPE AMFName					PRESENCE mandatory	}|
	{ ID id-ServedGUAMIList				CRITICALITY reject	TYPE ServedGUAMIList			PRESENCE mandatory	}|
	{ ID id-RelativeAMFCapacity			CRITICALITY ignore	TYPE RelativeAMFCapacity		PRESENCE mandatory	}|
	{ ID id-PLMNSupportList				CRITICALITY reject	TYPE PLMNSupportList			PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional	}|
	{ ID id-UERetentionInformation		CRITICALITY ignore	TYPE UERetentionInformation		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- NG SETUP FAILURE
--
-- **************************************************************

NGSetupFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGSetupFailureIEs} },
	...
}

NGSetupFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-TimeToWait					CRITICALITY ignore	TYPE TimeToWait					PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- RAN Configuration Update Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- RAN CONFIGURATION UPDATE 
--
-- **************************************************************

RANConfigurationUpdate ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {RANConfigurationUpdateIEs} },
	...
}

RANConfigurationUpdateIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RANNodeName								CRITICALITY ignore	TYPE RANNodeName									PRESENCE optional	}|
	{ ID id-SupportedTAList							CRITICALITY reject	TYPE SupportedTAList								PRESENCE optional	}|
	{ ID id-DefaultPagingDRX						CRITICALITY ignore	TYPE PagingDRX										PRESENCE optional	}|
	{ ID id-GlobalRANNodeID							CRITICALITY ignore	TYPE GlobalRANNodeID								PRESENCE optional	}|
	{ ID id-NGRAN-TNLAssociationToRemoveList		CRITICALITY reject	TYPE NGRAN-TNLAssociationToRemoveList			PRESENCE optional	},
	...
}

-- **************************************************************
--
-- RAN CONFIGURATION UPDATE ACKNOWLEDGE
--
-- **************************************************************

RANConfigurationUpdateAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {RANConfigurationUpdateAcknowledgeIEs} },
	...
}

RANConfigurationUpdateAcknowledgeIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- RAN CONFIGURATION UPDATE FAILURE
--
-- **************************************************************

RANConfigurationUpdateFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {RANConfigurationUpdateFailureIEs} },
	...
}

RANConfigurationUpdateFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-TimeToWait					CRITICALITY ignore	TYPE TimeToWait					PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
...
}

-- **************************************************************
--
-- AMF Configuration Update Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- AMF CONFIGURATION UPDATE 
--
-- **************************************************************

AMFConfigurationUpdate ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {AMFConfigurationUpdateIEs} },
	...
}

AMFConfigurationUpdateIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMFName								CRITICALITY reject	TYPE AMFName								PRESENCE optional		}|
	{ ID id-ServedGUAMIList						CRITICALITY reject	TYPE ServedGUAMIList						PRESENCE optional		}|
	{ ID id-RelativeAMFCapacity					CRITICALITY ignore	TYPE RelativeAMFCapacity					PRESENCE optional		}|
	{ ID id-PLMNSupportList						CRITICALITY reject	TYPE PLMNSupportList						PRESENCE optional		}|
	{ ID id-AMF-TNLAssociationToAddList			CRITICALITY ignore	TYPE AMF-TNLAssociationToAddList			PRESENCE optional		}|
	{ ID id-AMF-TNLAssociationToRemoveList		CRITICALITY ignore	TYPE AMF-TNLAssociationToRemoveList		PRESENCE optional		}|
	{ ID id-AMF-TNLAssociationToUpdateList		CRITICALITY ignore	TYPE AMF-TNLAssociationToUpdateList		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- AMF CONFIGURATION UPDATE ACKNOWLEDGE
--
-- **************************************************************

AMFConfigurationUpdateAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {AMFConfigurationUpdateAcknowledgeIEs} },
	...
}

AMFConfigurationUpdateAcknowledgeIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-TNLAssociationSetupList				CRITICALITY ignore	TYPE AMF-TNLAssociationSetupList			PRESENCE optional		}|
	{ ID id-AMF-TNLAssociationFailedToSetupList		CRITICALITY ignore	TYPE TNLAssociationList							PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics					CRITICALITY ignore	TYPE CriticalityDiagnostics					PRESENCE optional		},
	...
}

-- **************************************************************
--
-- AMF CONFIGURATION UPDATE FAILURE
--
-- **************************************************************

AMFConfigurationUpdateFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {AMFConfigurationUpdateFailureIEs} },
	...
}

AMFConfigurationUpdateFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-TimeToWait					CRITICALITY ignore	TYPE TimeToWait					PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- AMF Status Indication Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- AMF STATUS INDICATION
--
-- **************************************************************

AMFStatusIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {AMFStatusIndicationIEs} },
	...
}

AMFStatusIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-UnavailableGUAMIList		CRITICALITY reject	TYPE UnavailableGUAMIList		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- NG Reset Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- NG RESET
--
-- **************************************************************

NGReset ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGResetIEs} },
	...
}

NGResetIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-ResetType					CRITICALITY reject	TYPE ResetType					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- NG RESET ACKNOWLEDGE
--
-- **************************************************************

NGResetAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGResetAcknowledgeIEs} },
	...
}

NGResetAcknowledgeIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-UE-associatedLogicalNG-connectionList			CRITICALITY ignore	TYPE UE-associatedLogicalNG-connectionList			PRESENCE optional	}|
	{ ID id-CriticalityDiagnostics							CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional	},
	...
}

-- **************************************************************
--
-- Error Indication Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- ERROR INDICATION
--
-- **************************************************************

ErrorIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {ErrorIndicationIEs} },
	...
}

ErrorIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE optional		}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE optional		}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- OVERLOAD START
--
-- **************************************************************

OverloadStart ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {OverloadStartIEs} },
	...
}

OverloadStartIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMFOverloadResponse						CRITICALITY reject	TYPE OverloadResponse							PRESENCE optional 	}|
	{ ID id-AMFTrafficLoadReductionIndication		CRITICALITY ignore	TYPE TrafficLoadReductionIndication		PRESENCE optional		}|
	{ ID id-OverloadStartNSSAIList					CRITICALITY ignore	TYPE OverloadStartNSSAIList					PRESENCE optional		},
	...
}

-- **************************************************************
--
-- OVERLOAD STOP
--
-- **************************************************************

OverloadStop ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {OverloadStopIEs} },
	...
}

OverloadStopIEs NGAP-PROTOCOL-IES ::= {	
	...
}

-- **************************************************************
--
-- CONFIGURATION TRANSFER ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- UPLINK RAN CONFIGURATION TRANSFER
--
-- **************************************************************

UplinkRANConfigurationTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UplinkRANConfigurationTransferIEs} },
	...
}

UplinkRANConfigurationTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-SONConfigurationTransferUL			CRITICALITY ignore	TYPE SONConfigurationTransfer			PRESENCE optional	}|
	{ ID id-ENDC-SONConfigurationTransferUL		CRITICALITY ignore	TYPE EN-DCSONConfigurationTransfer	PRESENCE optional	},
	...
}

-- **************************************************************
--
-- DOWNLINK RAN CONFIGURATION TRANSFER
--
-- **************************************************************

DownlinkRANConfigurationTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DownlinkRANConfigurationTransferIEs} },
	...
}

DownlinkRANConfigurationTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-SONConfigurationTransferDL			CRITICALITY ignore	TYPE SONConfigurationTransfer			PRESENCE optional	}|
	{ ID id-ENDC-SONConfigurationTransferDL		CRITICALITY ignore	TYPE EN-DCSONConfigurationTransfer	PRESENCE optional	},
	...
}

-- **************************************************************
--
-- WARNING MESSAGE TRANSMISSION ELEMENTARY PROCEDURES 
--
-- **************************************************************

-- **************************************************************
--
-- Write-Replace Warning Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- WRITE-REPLACE WARNING REQUEST
--
-- **************************************************************

WriteReplaceWarningRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {WriteReplaceWarningRequestIEs} },
	...
}

WriteReplaceWarningRequestIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-MessageIdentifier				CRITICALITY reject	TYPE MessageIdentifier					PRESENCE mandatory	}|
	{ ID id-SerialNumber					CRITICALITY reject	TYPE SerialNumber						PRESENCE mandatory	}|
	{ ID id-WarningAreaList					CRITICALITY ignore	TYPE WarningAreaList					PRESENCE optional		}|
	{ ID id-RepetitionPeriod				CRITICALITY reject	TYPE RepetitionPeriod					PRESENCE mandatory	}|
	{ ID id-NumberOfBroadcastsRequested		CRITICALITY reject	TYPE NumberOfBroadcastsRequested		PRESENCE mandatory	}|
	{ ID id-WarningType						CRITICALITY ignore	TYPE WarningType						PRESENCE optional		}|
	{ ID id-WarningSecurityInfo				CRITICALITY ignore	TYPE WarningSecurityInfo				PRESENCE optional		}|
	{ ID id-DataCodingScheme				CRITICALITY ignore	TYPE DataCodingScheme					PRESENCE optional		}|
	{ ID id-WarningMessageContents			CRITICALITY ignore	TYPE WarningMessageContents				PRESENCE optional		}|
	{ ID id-ConcurrentWarningMessageInd		CRITICALITY reject	TYPE ConcurrentWarningMessageInd		PRESENCE optional		}|
	{ ID id-WarningAreaCoordinates			CRITICALITY ignore	TYPE WarningAreaCoordinates				PRESENCE optional		},
	...
}

-- **************************************************************
--
-- WRITE-REPLACE WARNING RESPONSE
--
-- **************************************************************

WriteReplaceWarningResponse ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {WriteReplaceWarningResponseIEs} },
	...
}

WriteReplaceWarningResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MessageIdentifier				CRITICALITY reject	TYPE MessageIdentifier					PRESENCE mandatory	}|
	{ ID id-SerialNumber					CRITICALITY reject	TYPE SerialNumber						PRESENCE mandatory	}|
	{ ID id-BroadcastCompletedAreaList		CRITICALITY ignore	TYPE BroadcastCompletedAreaList			PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics			CRITICALITY ignore	TYPE CriticalityDiagnostics				PRESENCE optional		},
	...
}

-- **************************************************************
--
-- PWS Cancel Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PWS CANCEL REQUEST
--
-- **************************************************************

PWSCancelRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PWSCancelRequestIEs} },
	...
}

PWSCancelRequestIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-MessageIdentifier			CRITICALITY reject	TYPE MessageIdentifier				PRESENCE mandatory	}|
	{ ID id-SerialNumber				CRITICALITY reject	TYPE SerialNumber					PRESENCE mandatory	}|
	{ ID id-WarningAreaList				CRITICALITY ignore	TYPE WarningAreaList				PRESENCE optional	}|
	{ ID id-CancelAllWarningMessages	CRITICALITY reject	TYPE CancelAllWarningMessages		PRESENCE optional	},
	...
}

-- **************************************************************
--
-- PWS CANCEL RESPONSE
--
-- **************************************************************

PWSCancelResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PWSCancelResponseIEs} },
	...
}

PWSCancelResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MessageIdentifier			CRITICALITY reject	TYPE MessageIdentifier				PRESENCE mandatory	}|
	{ ID id-SerialNumber				CRITICALITY reject	TYPE SerialNumber					PRESENCE mandatory	}|
	{ ID id-BroadcastCancelledAreaList	CRITICALITY ignore	TYPE BroadcastCancelledAreaList		PRESENCE optional	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics			PRESENCE optional	},
	...
}

-- **************************************************************
--
-- PWS Restart Indication Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PWS RESTART INDICATION
--
-- **************************************************************

PWSRestartIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PWSRestartIndicationIEs} },
	...
}

PWSRestartIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-CellIDListForRestart			CRITICALITY reject	TYPE CellIDListForRestart				PRESENCE mandatory	}|
	{ ID id-GlobalRANNodeID					CRITICALITY reject	TYPE GlobalRANNodeID					PRESENCE mandatory	}|
	{ ID id-TAIListForRestart				CRITICALITY reject	TYPE TAIListForRestart					PRESENCE mandatory	}|
	{ ID id-EmergencyAreaIDListForRestart	CRITICALITY reject	TYPE EmergencyAreaIDListForRestart	PRESENCE optional		},
	...
}

-- **************************************************************
--
-- PWS Failure Indication Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PWS FAILURE INDICATION
--
-- **************************************************************

PWSFailureIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PWSFailureIndicationIEs} },
	...
}

PWSFailureIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-PWSFailedCellIDList			CRITICALITY reject	TYPE PWSFailedCellIDList	PRESENCE mandatory	}|
	{ ID id-GlobalRANNodeID				CRITICALITY reject	TYPE GlobalRANNodeID		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- NRPPA TRANSPORT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- DOWNLINK UE ASSOCIATED NRPPA TRANSPORT
--
-- **************************************************************

DownlinkUEAssociatedNRPPaTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DownlinkUEAssociatedNRPPaTransportIEs} },
	...
}

DownlinkUEAssociatedNRPPaTransportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID			CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID			CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RoutingID				CRITICALITY reject	TYPE RoutingID					PRESENCE mandatory	}|
	{ ID id-NRPPa-PDU				CRITICALITY reject	TYPE NRPPa-PDU					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UPLINK UE ASSOCIATED NRPPA TRANSPORT
--
-- **************************************************************

UplinkUEAssociatedNRPPaTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UplinkUEAssociatedNRPPaTransportIEs} },
	...
}

UplinkUEAssociatedNRPPaTransportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID			CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID			CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RoutingID				CRITICALITY reject	TYPE RoutingID					PRESENCE mandatory	}|
	{ ID id-NRPPa-PDU				CRITICALITY reject	TYPE NRPPa-PDU					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- DOWNLINK NON UE ASSOCIATED NRPPA TRANSPORT
--
-- **************************************************************

DownlinkNonUEAssociatedNRPPaTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DownlinkNonUEAssociatedNRPPaTransportIEs} },
	...
}

DownlinkNonUEAssociatedNRPPaTransportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RoutingID				CRITICALITY reject	TYPE RoutingID					PRESENCE mandatory	}|
	{ ID id-NRPPa-PDU				CRITICALITY reject	TYPE NRPPa-PDU					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UPLINK NON UE ASSOCIATED NRPPA TRANSPORT
--
-- **************************************************************

UplinkNonUEAssociatedNRPPaTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UplinkNonUEAssociatedNRPPaTransportIEs} },
	...
}

UplinkNonUEAssociatedNRPPaTransportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RoutingID				CRITICALITY reject	TYPE RoutingID					PRESENCE mandatory	}|
	{ ID id-NRPPa-PDU				CRITICALITY reject	TYPE NRPPa-PDU					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- TRACE ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- TRACE START
--
-- **************************************************************

TraceStart ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {TraceStartIEs} },
	...
}

TraceStartIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-TraceActivation				CRITICALITY ignore	TYPE TraceActivation			PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- TRACE FAILURE INDICATION
--
-- **************************************************************

TraceFailureIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {TraceFailureIndicationIEs} },
	...
}

TraceFailureIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-NGRANTraceID				CRITICALITY ignore	TYPE NGRANTraceID				PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- DEACTIVATE TRACE
--
-- **************************************************************

DeactivateTrace ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DeactivateTraceIEs} },
	...
}

DeactivateTraceIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-NGRANTraceID				CRITICALITY ignore	TYPE NGRANTraceID				PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- CELL TRAFFIC TRACE
--
-- **************************************************************

CellTrafficTrace ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {CellTrafficTraceIEs} },
	...
}

CellTrafficTraceIEs NGAP-PROTOCOL-IES ::= {
	{ID id-AMF-UE-NGAP-ID					CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ID id-RAN-UE-NGAP-ID					CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ID id-NGRANTraceID						CRITICALITY ignore	TYPE NGRANTraceID				PRESENCE mandatory	}|
	{ID id-NGRAN-CGI						CRITICALITY ignore	TYPE NGRAN-CGI					PRESENCE mandatory	}|
	{ID id-TraceCollectionEntityIPAddress	CRITICALITY ignore	TYPE TransportLayerAddress		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- LOCATION REPORTING ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- LOCATION REPORTING CONTROL
--
-- **************************************************************

LocationReportingControl ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {LocationReportingControlIEs} },
	...
}

LocationReportingControlIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID					CRITICALITY reject	TYPE AMF-UE-NGAP-ID						PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY reject	TYPE RAN-UE-NGAP-ID						PRESENCE mandatory	}|
	{ ID id-LocationReportingRequestType	CRITICALITY ignore	TYPE LocationReportingRequestType		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- LOCATION REPORTING FAILURE INDICATION
--
-- **************************************************************

LocationReportingFailureIndication ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {LocationReportingFailureIndicationIEs} },
	...
}

LocationReportingFailureIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID			CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID			CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-Cause					CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- LOCATION REPORT
--
-- **************************************************************

LocationReport ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {LocationReportIEs} },
	...
}

LocationReportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID						CRITICALITY reject	TYPE AMF-UE-NGAP-ID							PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID						CRITICALITY reject	TYPE RAN-UE-NGAP-ID							PRESENCE mandatory	}|
	{ ID id-UserLocationInformation				CRITICALITY ignore	TYPE UserLocationInformation				PRESENCE mandatory	}|
	{ ID id-UEPresenceInAreaOfInterestList		CRITICALITY ignore	TYPE UEPresenceInAreaOfInterestList		PRESENCE optional		}|
	{ ID id-LocationReportingRequestType		CRITICALITY ignore	TYPE LocationReportingRequestType		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UE TNLA BINDING ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- UE TNLA BINDING RELEASE REQUEST
--
-- **************************************************************

UETNLABindingReleaseRequest ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {UETNLABindingReleaseRequestIEs} },
	...
}

UETNLABindingReleaseRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID		CRITICALITY reject	TYPE AMF-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID		CRITICALITY reject	TYPE RAN-UE-NGAP-ID		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UE RADIO CAPABILITY MANAGEMENT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- UE RADIO CAPABILITY INFO INDICATION
--
-- **************************************************************

UERadioCapabilityInfoIndication ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {UERadioCapabilityInfoIndicationIEs} },
	...
}

UERadioCapabilityInfoIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID					CRITICALITY reject	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY reject	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-UERadioCapability				CRITICALITY ignore	TYPE UERadioCapability				PRESENCE mandatory	}|
	{ ID id-UERadioCapabilityForPaging		CRITICALITY ignore	TYPE UERadioCapabilityForPaging		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE Radio Capability Check Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UE RADIO CAPABILITY CHECK REQUEST
--
-- **************************************************************

UERadioCapabilityCheckRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UERadioCapabilityCheckRequestIEs} },
	...
}

UERadioCapabilityCheckRequestIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID			CRITICALITY reject	TYPE AMF-UE-NGAP-ID			PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID			CRITICALITY reject	TYPE RAN-UE-NGAP-ID			PRESENCE mandatory	}|
	{ ID id-UERadioCapability		CRITICALITY ignore	TYPE UERadioCapability		PRESENCE optional	},
	...
}

-- **************************************************************
--
-- UE RADIO CAPABILITY CHECK RESPONSE
--
-- **************************************************************

UERadioCapabilityCheckResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UERadioCapabilityCheckResponseIEs} },
	...
}

UERadioCapabilityCheckResponseIEs NGAP-PROTOCOL-IES ::= {	
	{ ID id-AMF-UE-NGAP-ID					CRITICALITY ignore	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY ignore	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-IMSVoiceSupportIndicator		CRITICALITY reject	TYPE IMSVoiceSupportIndicator		PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics			CRITICALITY ignore	TYPE CriticalityDiagnostics			PRESENCE optional		},
	...
}

-- **************************************************************
--
-- PRIVATE MESSAGE ELEMENTARY PROCEDURE
--
-- **************************************************************

-- **************************************************************
--
-- PRIVATE MESSAGE
--
-- **************************************************************

PrivateMessage ::= SEQUENCE {
	privateIEs		PrivateIE-Container		{ { PrivateMessageIEs } },
	...
}

PrivateMessageIEs NGAP-PRIVATE-IES ::= {
	...
}


-- **************************************************************
--
-- DATA USAGE REPORTING ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- SECONDARY RAT DATA USAGE REPORT
--
-- **************************************************************

SecondaryRATDataUsageReport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {SecondaryRATDataUsageReportIEs} },
	...
}

SecondaryRATDataUsageReportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceSecondaryRATUsageList		CRITICALITY ignore	TYPE PDUSessionResourceSecondaryRATUsageList			PRESENCE mandatory	}|
	{ ID id-HandoverFlag								CRITICALITY ignore	TYPE HandoverFlag												PRESENCE optional		}|
	{ ID id-UserLocationInformation						CRITICALITY ignore	TYPE UserLocationInformation								PRESENCE optional },
	...
}


END
-- ASN1STOP

-- ASN1START
-- **************************************************************
--
-- Information Element Definitions
--
-- **************************************************************

NGAP-IEs {
itu-t (0) identified-organization (4) etsi (0) mobileDomain (0) 
ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::= 

BEGIN

IMPORTS

	id-AdditionalDLForwardingUPTNLInformation,
	id-AdditionalULForwardingUPTNLInformation,
	id-AdditionalDLQosFlowPerTNLInformation,
	id-AdditionalDLUPTNLInformationForHOList,
	id-AdditionalNGU-UP-TNLInformation,
	id-AdditionalUL-NGU-UP-TNLInformation,
	id-Cause,
	id-CNTypeRestrictionsForEquivalent,
	id-CNTypeRestrictionsForServing,
	id-CommonNetworkInstance,
	id-DataForwardingNotPossible,
	id-DL-NGU-UP-TNLInformation,
	id-EndpointIPAddressAndPort,
	id-LastEUTRAN-PLMNIdentity,
	id-LocationReportingAdditionalInfo,
	id-MaximumIntegrityProtectedDataRate-DL,
	id-NetworkInstance,
	id-OldAssociatedQosFlowList-ULendmarkerexpected,
	id-PDUSessionAggregateMaximumBitRate,
	id-PDUSessionResourceFailedToSetupListCxtFail,
	id-PDUSessionResourceReleaseResponseTransfer,
	id-PDUSessionType,
	id-PSCellInformation,
	id-QosFlowAddOrModifyRequestList,
	id-QosFlowSetupRequestList,
	id-QosFlowToReleaseList,
	id-SCTP-TLAs,
	id-SecondaryRATUsageInformation,
	id-SecurityIndication,
	id-SecurityResult,
	id-S-NSSAI,
	id-TNLAssociationTransportLayerAddressNGRAN,
	id-UL-NGU-UP-TNLInformation,
	id-UL-NGU-UP-TNLModifyList,
	id-ULForwarding,
	id-ULForwardingUP-TNLInformation,
	maxnoofAllowedAreas,
	maxnoofAllowedS-NSSAIs,
	maxnoofBPLMNs,
	maxnoofCellIDforWarning,
	maxnoofCellinAoI,
	maxnoofCellinEAI,
	maxnoofCellsingNB,
	maxnoofCellsinngeNB,
	maxnoofCellinTAI,
	maxnoofCellsinUEHistoryInfo,
	maxnoofCellsUEMovingTrajectory,
	maxnoofDRBs,
	maxnoofEmergencyAreaID,
	maxnoofEAIforRestart,
	maxnoofEPLMNs,
	maxnoofEPLMNsPlusOne,
	maxnoofE-RABs,
	maxnoofErrors,
	maxnoofForbTACs,
	maxnoofMultiConnectivity,
	maxnoofMultiConnectivityMinusOne,
	maxnoofNGConnectionsToReset,
	maxnoofPDUSessions,
	maxnoofPLMNs,
	maxnoofQosFlows,
	maxnoofRANNodeinAoI,
	maxnoofRecommendedCells,
	maxnoofRecommendedRANNodes,
	maxnoofAoI,
	maxnoofServedGUAMIs,
	maxnoofSliceItems,
	maxnoofTACs,
	maxnoofTAIforInactive,
	maxnoofTAIforPaging,
	maxnoofTAIforRestart,
	maxnoofTAIforWarning,
	maxnoofTAIinAoI,
	maxnoofTimePeriods,
	maxnoofTNLAssociations,
	maxnoofXnExtTLAs,
	maxnoofXnGTP-TLAs,
	maxnoofXnTLAs

FROM NGAP-Constants

	Criticality,
	ProcedureCode,
	ProtocolIE-ID,
	TriggeringMessage
FROM NGAP-CommonDataTypes

	ProtocolExtensionContainer{},
	ProtocolIE-Container{},
	NGAP-PROTOCOL-EXTENSION,
	ProtocolIE-SingleContainer{},
	NGAP-PROTOCOL-IES
FROM NGAP-Containers;

-- A

AdditionalDLUPTNLInformationForHOList ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivityMinusOne)) OF AdditionalDLUPTNLInformationForHOItem

AdditionalDLUPTNLInformationForHOItem ::= SEQUENCE {
	additionalDL-NGU-UP-TNLInformation				UPTransportLayerInformation,
	additionalQosFlowSetupResponseList				QosFlowListWithDataForwarding,
	additionalDLForwardingUPTNLInformation			UPTransportLayerInformation 							OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { AdditionalDLUPTNLInformationForHOItem-ExtIEs} }	OPTIONAL,
	...
}

AdditionalDLUPTNLInformationForHOItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AdditionalQosFlowInformation ::= ENUMERATED {
	more-likely,
	...
}

AllocationAndRetentionPriority ::= SEQUENCE {
	priorityLevelARP				PriorityLevelARP,
	pre-emptionCapability			Pre-emptionCapability,
	pre-emptionVulnerability		Pre-emptionVulnerability,
	iE-Extensions		ProtocolExtensionContainer { {AllocationAndRetentionPriority-ExtIEs} } OPTIONAL,
	...
}

AllocationAndRetentionPriority-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AllowedNSSAI ::= SEQUENCE (SIZE(1..maxnoofAllowedS-NSSAIs)) OF AllowedNSSAI-Item

AllowedNSSAI-Item ::= SEQUENCE {
	s-NSSAI				S-NSSAI,
	iE-Extensions		ProtocolExtensionContainer { {AllowedNSSAI-Item-ExtIEs} } OPTIONAL,
	...
}

AllowedNSSAI-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AllowedTACs ::= SEQUENCE (SIZE(1..maxnoofAllowedAreas)) OF TAC

AMFName ::= PrintableString (SIZE(1..150, ...))

AMFPagingTarget ::= CHOICE {
	globalRANNodeID			GlobalRANNodeID,
	tAI						TAI,
	choice-Extensions		ProtocolIE-SingleContainer { {AMFPagingTarget-ExtIEs} }
}

AMFPagingTarget-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

AMFPointer ::= BIT STRING (SIZE(6))

AMFRegionID ::= BIT STRING (SIZE(8))

AMFSetID ::= BIT STRING (SIZE(10))

AMF-TNLAssociationSetupList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF AMF-TNLAssociationSetupItem

AMF-TNLAssociationSetupItem ::= SEQUENCE {
	aMF-TNLAssociationAddress		CPTransportLayerInformation,
	iE-Extensions		ProtocolExtensionContainer { {AMF-TNLAssociationSetupItem-ExtIEs} }	OPTIONAL,
	...
}

AMF-TNLAssociationSetupItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AMF-TNLAssociationToAddList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF AMF-TNLAssociationToAddItem

AMF-TNLAssociationToAddItem ::= SEQUENCE {
	aMF-TNLAssociationAddress		CPTransportLayerInformation,
	tNLAssociationUsage				TNLAssociationUsage										OPTIONAL,
	tNLAddressWeightFactor			TNLAddressWeightFactor,
	iE-Extensions		ProtocolExtensionContainer { {AMF-TNLAssociationToAddItem-ExtIEs} }	OPTIONAL,
	...
}

AMF-TNLAssociationToAddItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AMF-TNLAssociationToRemoveList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF AMF-TNLAssociationToRemoveItem

AMF-TNLAssociationToRemoveItem ::= SEQUENCE {
	aMF-TNLAssociationAddress		CPTransportLayerInformation,
	iE-Extensions		ProtocolExtensionContainer { {AMF-TNLAssociationToRemoveItem-ExtIEs} }	OPTIONAL,
	...
}

AMF-TNLAssociationToRemoveItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-TNLAssociationTransportLayerAddressNGRAN	CRITICALITY reject	EXTENSION CPTransportLayerInformation	PRESENCE optional},
	...
}

AMF-TNLAssociationToUpdateList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF AMF-TNLAssociationToUpdateItem

AMF-TNLAssociationToUpdateItem ::= SEQUENCE {
	aMF-TNLAssociationAddress		CPTransportLayerInformation,
	tNLAssociationUsage				TNLAssociationUsage											OPTIONAL,
	tNLAddressWeightFactor			TNLAddressWeightFactor										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {AMF-TNLAssociationToUpdateItem-ExtIEs} }	OPTIONAL,
	...
}

AMF-TNLAssociationToUpdateItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AMF-UE-NGAP-ID ::= INTEGER (0..1099511627775)

AreaOfInterest ::= SEQUENCE {
	areaOfInterestTAIList			AreaOfInterestTAIList						OPTIONAL,
	areaOfInterestCellList			AreaOfInterestCellList						OPTIONAL,
 	areaOfInterestRANNodeList		AreaOfInterestRANNodeList					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {AreaOfInterest-ExtIEs} }	OPTIONAL,
	...
}

AreaOfInterest-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AreaOfInterestCellList ::= SEQUENCE (SIZE(1..maxnoofCellinAoI)) OF AreaOfInterestCellItem

AreaOfInterestCellItem ::= SEQUENCE {
	nGRAN-CGI			NGRAN-CGI,
	iE-Extensions		ProtocolExtensionContainer { {AreaOfInterestCellItem-ExtIEs} }	OPTIONAL,
	...
}

AreaOfInterestCellItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AreaOfInterestList ::= SEQUENCE (SIZE(1..maxnoofAoI)) OF AreaOfInterestItem

AreaOfInterestItem ::= SEQUENCE {
	areaOfInterest						AreaOfInterest,
	locationReportingReferenceID		LocationReportingReferenceID,
	iE-Extensions		ProtocolExtensionContainer { {AreaOfInterestItem-ExtIEs} }	OPTIONAL,
	...
}

AreaOfInterestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AreaOfInterestRANNodeList ::= SEQUENCE (SIZE(1..maxnoofRANNodeinAoI)) OF AreaOfInterestRANNodeItem

AreaOfInterestRANNodeItem ::= SEQUENCE {
	globalRANNodeID		GlobalRANNodeID,
	iE-Extensions		ProtocolExtensionContainer { {AreaOfInterestRANNodeItem-ExtIEs} }	OPTIONAL,
	...
}

AreaOfInterestRANNodeItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AreaOfInterestTAIList ::= SEQUENCE (SIZE(1..maxnoofTAIinAoI)) OF AreaOfInterestTAIItem

AreaOfInterestTAIItem ::= SEQUENCE {
	tAI					TAI,
	iE-Extensions		ProtocolExtensionContainer { {AreaOfInterestTAIItem-ExtIEs} }	OPTIONAL,
	...
}

AreaOfInterestTAIItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AssistanceDataForPaging ::= SEQUENCE {
	assistanceDataForRecommendedCells		AssistanceDataForRecommendedCells			OPTIONAL,
	pagingAttemptInformation				PagingAttemptInformation					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {AssistanceDataForPaging-ExtIEs} } OPTIONAL,
	...
}

AssistanceDataForPaging-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AssistanceDataForRecommendedCells ::= SEQUENCE {
	recommendedCellsForPaging		RecommendedCellsForPaging, 
	iE-Extensions		ProtocolExtensionContainer { {AssistanceDataForRecommendedCells-ExtIEs} }	OPTIONAL,
	...
}

AssistanceDataForRecommendedCells-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AssociatedQosFlowList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF AssociatedQosFlowItem

AssociatedQosFlowItem ::= SEQUENCE {
	qosFlowIdentifier				QosFlowIdentifier,
	qosFlowMappingIndication		ENUMERATED {ul, dl, ...}							OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {AssociatedQosFlowItem-ExtIEs} }	OPTIONAL,
	...
}

AssociatedQosFlowItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AveragingWindow ::= INTEGER (0..4095, ...)

-- B

BitRate	::= INTEGER (0..4000000000000, ...) 

BroadcastCancelledAreaList ::= CHOICE {
	cellIDCancelledEUTRA				CellIDCancelledEUTRA,
	tAICancelledEUTRA					TAICancelledEUTRA,
	emergencyAreaIDCancelledEUTRA		EmergencyAreaIDCancelledEUTRA,
	cellIDCancelledNR					CellIDCancelledNR,
	tAICancelledNR						TAICancelledNR,
	emergencyAreaIDCancelledNR			EmergencyAreaIDCancelledNR,
	choice-Extensions		ProtocolIE-SingleContainer { {BroadcastCancelledAreaList-ExtIEs} }
}

BroadcastCancelledAreaList-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

BroadcastCompletedAreaList ::= CHOICE {
	cellIDBroadcastEUTRA				CellIDBroadcastEUTRA,
	tAIBroadcastEUTRA					TAIBroadcastEUTRA,
	emergencyAreaIDBroadcastEUTRA		EmergencyAreaIDBroadcastEUTRA,
	cellIDBroadcastNR					CellIDBroadcastNR,
	tAIBroadcastNR						TAIBroadcastNR,
	emergencyAreaIDBroadcastNR			EmergencyAreaIDBroadcastNR,
	choice-Extensions		ProtocolIE-SingleContainer { {BroadcastCompletedAreaList-ExtIEs} }
}

BroadcastCompletedAreaList-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

BroadcastPLMNList ::= SEQUENCE (SIZE(1..maxnoofBPLMNs)) OF BroadcastPLMNItem

BroadcastPLMNItem ::= SEQUENCE {
	pLMNIdentity			PLMNIdentity,
	tAISliceSupportList		SliceSupportList,
	iE-Extensions		ProtocolExtensionContainer { {BroadcastPLMNItem-ExtIEs} } OPTIONAL,
	...
}

BroadcastPLMNItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- C

CancelAllWarningMessages ::= ENUMERATED {
	true,
	...
}

CancelledCellsInEAI-EUTRA ::= SEQUENCE (SIZE(1..maxnoofCellinEAI)) OF CancelledCellsInEAI-EUTRA-Item

CancelledCellsInEAI-EUTRA-Item ::= SEQUENCE {
	eUTRA-CGI				EUTRA-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CancelledCellsInEAI-EUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CancelledCellsInEAI-EUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CancelledCellsInEAI-NR ::= SEQUENCE (SIZE(1..maxnoofCellinEAI)) OF CancelledCellsInEAI-NR-Item

CancelledCellsInEAI-NR-Item ::= SEQUENCE {
	nR-CGI					NR-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CancelledCellsInEAI-NR-Item-ExtIEs} } OPTIONAL,
	...
}

CancelledCellsInEAI-NR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CancelledCellsInTAI-EUTRA ::= SEQUENCE (SIZE(1..maxnoofCellinTAI)) OF CancelledCellsInTAI-EUTRA-Item

CancelledCellsInTAI-EUTRA-Item ::= SEQUENCE {
	eUTRA-CGI				EUTRA-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CancelledCellsInTAI-EUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CancelledCellsInTAI-EUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CancelledCellsInTAI-NR ::= SEQUENCE (SIZE(1..maxnoofCellinTAI)) OF CancelledCellsInTAI-NR-Item

CancelledCellsInTAI-NR-Item ::= SEQUENCE{
	nR-CGI					NR-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CancelledCellsInTAI-NR-Item-ExtIEs} } OPTIONAL,
	...
}

CancelledCellsInTAI-NR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

Cause ::= CHOICE {
	radioNetwork		CauseRadioNetwork,
	transport			CauseTransport,
	nas					CauseNas,
	protocol			CauseProtocol,
	misc				CauseMisc,
	choice-Extensions		ProtocolIE-SingleContainer { {Cause-ExtIEs} }
}

Cause-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

CauseMisc ::= ENUMERATED {
	control-processing-overload,
	not-enough-user-plane-processing-resources,
	hardware-failure,
	om-intervention,
	unknown-PLMN,
	unspecified,
	...
}

CauseNas ::= ENUMERATED {
	normal-release,
	authentication-failure,
	deregister,
	unspecified,
	...
}

CauseProtocol ::= ENUMERATED {
	transfer-syntax-error,
	abstract-syntax-error-reject,
	abstract-syntax-error-ignore-and-notify,
	message-not-compatible-with-receiver-state,
	semantic-error,
	abstract-syntax-error-falsely-constructed-message,
	unspecified,
	...
}

CauseRadioNetwork ::= ENUMERATED {
	unspecified,
	txnrelocoverall-expiry,
	successful-handover,
	release-due-to-ngran-generated-reason,
	release-due-to-5gc-generated-reason,
	handover-cancelled,	
	partial-handover,	
	ho-failure-in-target-5GC-ngran-node-or-target-system,
	ho-target-not-allowed,
	tngrelocoverall-expiry,
	tngrelocprep-expiry,
	cell-not-available,
	unknown-targetID,
	no-radio-resources-available-in-target-cell,
	unknown-local-UE-NGAP-ID,
	inconsistent-remote-UE-NGAP-ID,
	handover-desirable-for-radio-reason,
	time-critical-handover,
	resource-optimisation-handover,
	reduce-load-in-serving-cell,
	user-inactivity,
	radio-connection-with-ue-lost,
	radio-resources-not-available,
	invalid-qos-combination,
	failure-in-radio-interface-procedure,
	interaction-with-other-procedure,
	unknown-PDU-session-ID,
	unkown-qos-flow-ID,
	multiple-PDU-session-ID-instances,
	multiple-qos-flow-ID-instances,
	encryption-and-or-integrity-protection-algorithms-not-supported,
	ng-intra-system-handover-triggered,
	ng-inter-system-handover-triggered,
	xn-handover-triggered,
	not-supported-5QI-value,
	ue-context-transfer,
	ims-voice-eps-fallback-or-rat-fallback-triggered,
	up-integrity-protection-not-possible,
	up-confidentiality-protection-not-possible,
	slice-not-supported,
	ue-in-rrc-inactive-state-not-reachable,
	redirection,
	resources-not-available-for-the-slice,
	ue-max-integrity-protected-data-rate-reason,
	release-due-to-cn-detected-mobility,
	...,
	n26-interface-not-available,
	release-due-to-pre-emption,
	multiple-location-reporting-reference-ID-instances
}

CauseTransport ::= ENUMERATED {
	transport-resource-unavailable,
	unspecified,
	...
}

CellIDBroadcastEUTRA ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF CellIDBroadcastEUTRA-Item

CellIDBroadcastEUTRA-Item ::= SEQUENCE {
	eUTRA-CGI			EUTRA-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CellIDBroadcastEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CellIDBroadcastEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellIDBroadcastNR ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF CellIDBroadcastNR-Item

CellIDBroadcastNR-Item ::= SEQUENCE {
	nR-CGI				NR-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CellIDBroadcastNR-Item-ExtIEs} } OPTIONAL,
	...
}

CellIDBroadcastNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellIDCancelledEUTRA ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF CellIDCancelledEUTRA-Item

CellIDCancelledEUTRA-Item ::= SEQUENCE {
	eUTRA-CGI				EUTRA-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CellIDCancelledEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CellIDCancelledEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellIDCancelledNR ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF CellIDCancelledNR-Item

CellIDCancelledNR-Item ::= SEQUENCE {
	nR-CGI					NR-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CellIDCancelledNR-Item-ExtIEs} } OPTIONAL,
	...
}

CellIDCancelledNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellIDListForRestart ::= CHOICE {
	eUTRA-CGIListforRestart		EUTRA-CGIList,
	nR-CGIListforRestart		NR-CGIList,
	choice-Extensions		ProtocolIE-SingleContainer { {CellIDListForRestart-ExtIEs} }
}

CellIDListForRestart-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

CellSize ::= ENUMERATED {verysmall, small, medium, large, ...}


CellType ::= SEQUENCE {
	cellSize		CellSize,
	iE-Extensions		ProtocolExtensionContainer { {CellType-ExtIEs} }	OPTIONAL,
	...
}

CellType-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CNAssistedRANTuning ::= SEQUENCE {
	expectedUEBehaviour					ExpectedUEBehaviour												OPTIONAL,
	iE-Extensions						ProtocolExtensionContainer { {CNAssistedRANTuning-ExtIEs} }	OPTIONAL,
	...
}

CNAssistedRANTuning-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CNTypeRestrictionsForEquivalent ::= SEQUENCE (SIZE(1..maxnoofEPLMNs)) OF CNTypeRestrictionsForEquivalentItem

CNTypeRestrictionsForEquivalentItem ::= SEQUENCE {
	plmnIdentity						PLMNIdentity,
	cn-Type								ENUMERATED {epc-forbidden, fiveGC-forbidden, ...},
	iE-Extensions						ProtocolExtensionContainer { {CNTypeRestrictionsForEquivalentItem-ExtIEs} }				OPTIONAL,
	...
}

CNTypeRestrictionsForEquivalentItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::={
	...
}

CNTypeRestrictionsForServing ::= ENUMERATED {
	epc-forbidden,
	...
}

CommonNetworkInstance ::= OCTET STRING

CompletedCellsInEAI-EUTRA ::= SEQUENCE (SIZE(1..maxnoofCellinEAI)) OF CompletedCellsInEAI-EUTRA-Item

CompletedCellsInEAI-EUTRA-Item ::= SEQUENCE {
	eUTRA-CGI			EUTRA-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CompletedCellsInEAI-EUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CompletedCellsInEAI-EUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CompletedCellsInEAI-NR ::= SEQUENCE (SIZE(1..maxnoofCellinEAI)) OF CompletedCellsInEAI-NR-Item

CompletedCellsInEAI-NR-Item ::= SEQUENCE {
	nR-CGI				NR-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CompletedCellsInEAI-NR-Item-ExtIEs} }	OPTIONAL,
	...
}

CompletedCellsInEAI-NR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CompletedCellsInTAI-EUTRA ::= SEQUENCE (SIZE(1..maxnoofCellinTAI)) OF CompletedCellsInTAI-EUTRA-Item

CompletedCellsInTAI-EUTRA-Item ::= SEQUENCE{
	eUTRA-CGI			EUTRA-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CompletedCellsInTAI-EUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CompletedCellsInTAI-EUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CompletedCellsInTAI-NR ::= SEQUENCE (SIZE(1..maxnoofCellinTAI)) OF CompletedCellsInTAI-NR-Item

CompletedCellsInTAI-NR-Item ::= SEQUENCE{
	nR-CGI				NR-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CompletedCellsInTAI-NR-Item-ExtIEs} } OPTIONAL,
	...
}

CompletedCellsInTAI-NR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ConcurrentWarningMessageInd ::= ENUMERATED {
	true,
	...
}

ConfidentialityProtectionIndication ::= ENUMERATED {
	required,
	preferred,
	not-needed,
	...
}

ConfidentialityProtectionResult ::= ENUMERATED {
	performed,
	not-performed,
	...
}

CoreNetworkAssistanceInformationForInactive ::= SEQUENCE {
	uEIdentityIndexValue				UEIdentityIndexValue,
	uESpecificDRX						PagingDRX													OPTIONAL,
	periodicRegistrationUpdateTimer		PeriodicRegistrationUpdateTimer,
	mICOModeIndication					MICOModeIndication											OPTIONAL,
	tAIListForInactive					TAIListForInactive,
	expectedUEBehaviour					ExpectedUEBehaviour											OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {CoreNetworkAssistanceInformationForInactive-ExtIEs} }	OPTIONAL,
	...
}

CoreNetworkAssistanceInformationForInactive-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

COUNTValueForPDCP-SN12 ::= SEQUENCE {
	pDCP-SN12			INTEGER (0..4095),
	hFN-PDCP-SN12		INTEGER (0..1048575),
	iE-Extensions		ProtocolExtensionContainer { {COUNTValueForPDCP-SN12-ExtIEs} }	OPTIONAL,
	...
}

COUNTValueForPDCP-SN12-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

COUNTValueForPDCP-SN18 ::= SEQUENCE {
	pDCP-SN18			INTEGER (0..262143),
	hFN-PDCP-SN18		INTEGER (0..16383),
	iE-Extensions		ProtocolExtensionContainer { {COUNTValueForPDCP-SN18-ExtIEs} }	OPTIONAL,
	...
}

COUNTValueForPDCP-SN18-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CPTransportLayerInformation ::= CHOICE {
	endpointIPAddress		TransportLayerAddress,
	choice-Extensions		ProtocolIE-SingleContainer { {CPTransportLayerInformation-ExtIEs} }
}

CPTransportLayerInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-EndpointIPAddressAndPort		CRITICALITY reject	TYPE EndpointIPAddressAndPort		PRESENCE mandatory},
	...
}

CriticalityDiagnostics ::= SEQUENCE {
	procedureCode					ProcedureCode											OPTIONAL,
	triggeringMessage				TriggeringMessage										OPTIONAL,
	procedureCriticality			Criticality												OPTIONAL,
	iEsCriticalityDiagnostics		CriticalityDiagnostics-IE-List							OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer {{CriticalityDiagnostics-ExtIEs}}		OPTIONAL,
	...
}

CriticalityDiagnostics-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CriticalityDiagnostics-IE-List ::= SEQUENCE (SIZE(1..maxnoofErrors)) OF CriticalityDiagnostics-IE-Item

CriticalityDiagnostics-IE-Item ::= SEQUENCE {
	iECriticality		Criticality,
	iE-ID				ProtocolIE-ID,
	typeOfError			TypeOfError,
	iE-Extensions		ProtocolExtensionContainer {{CriticalityDiagnostics-IE-Item-ExtIEs}} OPTIONAL,
	...
}

CriticalityDiagnostics-IE-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- D

DataCodingScheme ::= BIT STRING (SIZE(8))

DataForwardingAccepted ::= ENUMERATED {
	data-forwarding-accepted,
	...
}

DataForwardingNotPossible ::= ENUMERATED {
	data-forwarding-not-possible,
	...
}

DataForwardingResponseDRBList ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DataForwardingResponseDRBItem

DataForwardingResponseDRBItem ::= SEQUENCE {
	dRB-ID								DRB-ID,
	dLForwardingUP-TNLInformation		UPTransportLayerInformation								OPTIONAL,
	uLForwardingUP-TNLInformation		UPTransportLayerInformation								OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer {{DataForwardingResponseDRBItem-ExtIEs}}		OPTIONAL,
	...
}

DataForwardingResponseDRBItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DelayCritical ::= ENUMERATED {
	delay-critical,
	non-delay-critical,
	...
}

DLForwarding ::= ENUMERATED {
	dl-forwarding-proposed,
	...
}

DL-NGU-TNLInformationReused ::= ENUMERATED {
	true,
	...
}

DirectForwardingPathAvailability ::= ENUMERATED {
	direct-path-available,
	...
}

DRB-ID ::= INTEGER (1..32, ...)

DRBsSubjectToStatusTransferList ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsSubjectToStatusTransferItem

DRBsSubjectToStatusTransferItem ::= SEQUENCE {
	dRB-ID				DRB-ID,
	dRBStatusUL			DRBStatusUL,
	dRBStatusDL			DRBStatusDL,
	iE-Extension		ProtocolExtensionContainer { {DRBsSubjectToStatusTransferItem-ExtIEs} }	OPTIONAL,
	...
}

DRBsSubjectToStatusTransferItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-OldAssociatedQosFlowList-ULendmarkerexpected	CRITICALITY reject EXTENSION AssociatedQosFlowList	 PRESENCE optional },
	...
}

DRBStatusDL ::= CHOICE {
	dRBStatusDL12			DRBStatusDL12,
	dRBStatusDL18			DRBStatusDL18,
	choice-Extensions		ProtocolIE-SingleContainer { {DRBStatusDL-ExtIEs} }
}

DRBStatusDL-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

DRBStatusDL12 ::= SEQUENCE {
	dL-COUNTValue		COUNTValueForPDCP-SN12,
	iE-Extension		ProtocolExtensionContainer { {DRBStatusDL12-ExtIEs} }		OPTIONAL,
	...
}

DRBStatusDL12-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DRBStatusDL18 ::= SEQUENCE {
	dL-COUNTValue		COUNTValueForPDCP-SN18,
	iE-Extension		ProtocolExtensionContainer { {DRBStatusDL18-ExtIEs} }		OPTIONAL,
	...
}

DRBStatusDL18-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DRBStatusUL ::= CHOICE {
	dRBStatusUL12			DRBStatusUL12,
	dRBStatusUL18			DRBStatusUL18,
	choice-Extensions		ProtocolIE-SingleContainer { {DRBStatusUL-ExtIEs} }
}

DRBStatusUL-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

DRBStatusUL12 ::= SEQUENCE {
	uL-COUNTValue					COUNTValueForPDCP-SN12,
	receiveStatusOfUL-PDCP-SDUs		BIT STRING (SIZE(1..2048))						OPTIONAL,
	iE-Extension		ProtocolExtensionContainer { {DRBStatusUL12-ExtIEs} }		OPTIONAL,
	...
}

DRBStatusUL12-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DRBStatusUL18 ::= SEQUENCE {
	uL-COUNTValue					COUNTValueForPDCP-SN18,
	receiveStatusOfUL-PDCP-SDUs		BIT STRING (SIZE(1..131072))					OPTIONAL,
	iE-Extension		ProtocolExtensionContainer { {DRBStatusUL18-ExtIEs} }		OPTIONAL,
	...
}

DRBStatusUL18-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DRBsToQosFlowsMappingList ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsToQosFlowsMappingItem

DRBsToQosFlowsMappingItem ::= SEQUENCE {
	dRB-ID								DRB-ID,
	associatedQosFlowList				AssociatedQosFlowList,
	iE-Extensions		ProtocolExtensionContainer { {DRBsToQosFlowsMappingItem-ExtIEs} }		OPTIONAL,
	...
}

DRBsToQosFlowsMappingItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

Dynamic5QIDescriptor ::= SEQUENCE {
	priorityLevelQos			PriorityLevelQos,
	packetDelayBudget			PacketDelayBudget,
	packetErrorRate				PacketErrorRate,
	fiveQI						FiveQI													OPTIONAL,
	delayCritical				DelayCritical											OPTIONAL,
-- The above IE shall be present in case of GBR QoS flow
	averagingWindow				AveragingWindow											OPTIONAL,
-- The above IE shall be present in case of GBR QoS flow
	maximumDataBurstVolume		MaximumDataBurstVolume									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {Dynamic5QIDescriptor-ExtIEs} }	OPTIONAL,
	...
}

Dynamic5QIDescriptor-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- E

EmergencyAreaID ::= OCTET STRING (SIZE(3))

EmergencyAreaIDBroadcastEUTRA ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaIDBroadcastEUTRA-Item

EmergencyAreaIDBroadcastEUTRA-Item ::= SEQUENCE {
	emergencyAreaID					EmergencyAreaID,
	completedCellsInEAI-EUTRA		CompletedCellsInEAI-EUTRA,
	iE-Extensions		ProtocolExtensionContainer { {EmergencyAreaIDBroadcastEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

EmergencyAreaIDBroadcastEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EmergencyAreaIDBroadcastNR ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaIDBroadcastNR-Item

EmergencyAreaIDBroadcastNR-Item ::= SEQUENCE {
	emergencyAreaID				EmergencyAreaID,
	completedCellsInEAI-NR		CompletedCellsInEAI-NR,
	iE-Extensions		ProtocolExtensionContainer { {EmergencyAreaIDBroadcastNR-Item-ExtIEs} }	OPTIONAL,
	...
}

EmergencyAreaIDBroadcastNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EmergencyAreaIDCancelledEUTRA ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaIDCancelledEUTRA-Item

EmergencyAreaIDCancelledEUTRA-Item ::= SEQUENCE {
	emergencyAreaID					EmergencyAreaID,
	cancelledCellsInEAI-EUTRA		CancelledCellsInEAI-EUTRA,
	iE-Extensions		ProtocolExtensionContainer { {EmergencyAreaIDCancelledEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

EmergencyAreaIDCancelledEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EmergencyAreaIDCancelledNR ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaIDCancelledNR-Item

EmergencyAreaIDCancelledNR-Item ::= SEQUENCE {
	emergencyAreaID				EmergencyAreaID,
	cancelledCellsInEAI-NR		CancelledCellsInEAI-NR,
	iE-Extensions		ProtocolExtensionContainer { {EmergencyAreaIDCancelledNR-Item-ExtIEs} }	OPTIONAL,
	...
}

EmergencyAreaIDCancelledNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EmergencyAreaIDList ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaID

EmergencyAreaIDListForRestart ::= SEQUENCE (SIZE(1..maxnoofEAIforRestart)) OF EmergencyAreaID

EmergencyFallbackIndicator ::= SEQUENCE {
	emergencyFallbackRequestIndicator		EmergencyFallbackRequestIndicator,
	emergencyServiceTargetCN				EmergencyServiceTargetCN						OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {EmergencyFallbackIndicator-ExtIEs} }	OPTIONAL,
	...
}

EmergencyFallbackIndicator-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EmergencyFallbackRequestIndicator ::= ENUMERATED {
	emergency-fallback-requested,
	...
}

EmergencyServiceTargetCN ::= ENUMERATED {
	fiveGC,
	epc,
	...
}

EN-DCSONConfigurationTransfer ::= OCTET STRING

EndpointIPAddressAndPort ::=SEQUENCE {
	endpointIPAddress TransportLayerAddress,
	portNumber			PortNumber,
	iE-Extensions					ProtocolExtensionContainer { { EndpointIPAddressAndPort-ExtIEs} } OPTIONAL
}

EndpointIPAddressAndPort-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EquivalentPLMNs ::= SEQUENCE (SIZE(1..maxnoofEPLMNs)) OF PLMNIdentity

EPS-TAC ::= OCTET STRING (SIZE(2))

EPS-TAI ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	ePS-TAC				EPS-TAC,
	iE-Extensions		ProtocolExtensionContainer { {EPS-TAI-ExtIEs} } OPTIONAL,
	...
}

EPS-TAI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

E-RAB-ID ::= INTEGER (0..15, ...)

E-RABInformationList ::= SEQUENCE (SIZE(1..maxnoofE-RABs)) OF E-RABInformationItem

E-RABInformationItem ::= SEQUENCE {
	e-RAB-ID			E-RAB-ID,
	dLForwarding		DLForwarding													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {E-RABInformationItem-ExtIEs} }	OPTIONAL,
	...
}

E-RABInformationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EUTRACellIdentity ::= BIT STRING (SIZE(28))

EUTRA-CGI ::= SEQUENCE {
	pLMNIdentity			PLMNIdentity,
	eUTRACellIdentity		EUTRACellIdentity,
	iE-Extensions		ProtocolExtensionContainer { {EUTRA-CGI-ExtIEs} } OPTIONAL,
	...
}

EUTRA-CGI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EUTRA-CGIList ::= SEQUENCE (SIZE(1..maxnoofCellsinngeNB)) OF EUTRA-CGI

EUTRA-CGIListForWarning ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF EUTRA-CGI

EUTRAencryptionAlgorithms ::= BIT STRING (SIZE(16, ...))

EUTRAintegrityProtectionAlgorithms ::= BIT STRING (SIZE(16, ...))

EventType ::= ENUMERATED {
	direct,
	change-of-serve-cell,
	ue-presence-in-area-of-interest,
	stop-change-of-serve-cell,
	stop-ue-presence-in-area-of-interest,
	cancel-location-reporting-for-the-ue,
	...
}

ExpectedActivityPeriod ::= INTEGER (1..30|40|50|60|80|100|120|150|180|181, ...)

ExpectedHOInterval ::= ENUMERATED {
	sec15, sec30, sec60, sec90, sec120, sec180, long-time,
	...
}

ExpectedIdlePeriod ::= INTEGER (1..30|40|50|60|80|100|120|150|180|181, ...)

ExpectedUEActivityBehaviour ::= SEQUENCE {
	expectedActivityPeriod						ExpectedActivityPeriod						OPTIONAL,
	expectedIdlePeriod							ExpectedIdlePeriod							OPTIONAL,
	sourceOfUEActivityBehaviourInformation		SourceOfUEActivityBehaviourInformation		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {ExpectedUEActivityBehaviour-ExtIEs} }	OPTIONAL,
	...
}

ExpectedUEActivityBehaviour-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ExpectedUEBehaviour ::= SEQUENCE {
	expectedUEActivityBehaviour		ExpectedUEActivityBehaviour 					OPTIONAL,
	expectedHOInterval				ExpectedHOInterval		 						OPTIONAL,
	expectedUEMobility				ExpectedUEMobility								OPTIONAL,
	expectedUEMovingTrajectory		ExpectedUEMovingTrajectory						OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {ExpectedUEBehaviour-ExtIEs} }	OPTIONAL,
	...
}

ExpectedUEBehaviour-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ExpectedUEMobility ::= ENUMERATED {
	stationary,
	mobile,
	...
}

ExpectedUEMovingTrajectory ::= SEQUENCE (SIZE(1..maxnoofCellsUEMovingTrajectory)) OF ExpectedUEMovingTrajectoryItem

ExpectedUEMovingTrajectoryItem ::= SEQUENCE {
	nGRAN-CGI				NGRAN-CGI,
	timeStayedInCell		INTEGER (0..4095)													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {ExpectedUEMovingTrajectoryItem-ExtIEs} }	OPTIONAL,
	...
}

ExpectedUEMovingTrajectoryItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- F

FiveG-S-TMSI ::= SEQUENCE {
	aMFSetID			AMFSetID,
	aMFPointer			AMFPointer,
	fiveG-TMSI			FiveG-TMSI,
	iE-Extensions		ProtocolExtensionContainer { {FiveG-S-TMSI-ExtIEs} }	OPTIONAL,
	...
}

FiveG-S-TMSI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

FiveG-TMSI ::= OCTET STRING (SIZE(4))

FiveQI ::= INTEGER (0..255, ...)

ForbiddenAreaInformation ::= SEQUENCE (SIZE(1.. maxnoofEPLMNsPlusOne)) OF ForbiddenAreaInformation-Item

ForbiddenAreaInformation-Item ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	forbiddenTACs		ForbiddenTACs,
	iE-Extensions		ProtocolExtensionContainer { {ForbiddenAreaInformation-Item-ExtIEs} } OPTIONAL,
	...
}

ForbiddenAreaInformation-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ForbiddenTACs ::= SEQUENCE (SIZE(1..maxnoofForbTACs)) OF TAC

-- G

GBR-QosInformation ::= SEQUENCE {
	maximumFlowBitRateDL		BitRate,
	maximumFlowBitRateUL		BitRate,
	guaranteedFlowBitRateDL		BitRate,
	guaranteedFlowBitRateUL		BitRate,
	notificationControl			NotificationControl									OPTIONAL,
	maximumPacketLossRateDL		PacketLossRate										OPTIONAL,
	maximumPacketLossRateUL		PacketLossRate										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {GBR-QosInformation-ExtIEs} }	OPTIONAL,
	...
}

GBR-QosInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...}

GlobalGNB-ID ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	gNB-ID				GNB-ID,
	iE-Extensions		ProtocolExtensionContainer { {GlobalGNB-ID-ExtIEs} } OPTIONAL,
	...
}

GlobalGNB-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GlobalN3IWF-ID ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	n3IWF-ID			N3IWF-ID,
	iE-Extensions		ProtocolExtensionContainer { {GlobalN3IWF-ID-ExtIEs} } OPTIONAL,
	...
}

GlobalN3IWF-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GlobalNgENB-ID ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	ngENB-ID			NgENB-ID,
	iE-Extensions		ProtocolExtensionContainer { {GlobalNgENB-ID-ExtIEs} } OPTIONAL,
	...
}

GlobalNgENB-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GlobalRANNodeID ::= CHOICE {
	globalGNB-ID		GlobalGNB-ID,
	globalNgENB-ID		GlobalNgENB-ID,
	globalN3IWF-ID		GlobalN3IWF-ID,
	choice-Extensions		ProtocolIE-SingleContainer { {GlobalRANNodeID-ExtIEs} }
}

GlobalRANNodeID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

GNB-ID ::= CHOICE {
	gNB-ID		BIT STRING (SIZE(22..32)),
	choice-Extensions		ProtocolIE-SingleContainer { {GNB-ID-ExtIEs} }
}

GNB-ID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

GTP-TEID ::= OCTET STRING (SIZE(4))

GTPTunnel ::= SEQUENCE {
	transportLayerAddress		TransportLayerAddress,
	gTP-TEID					GTP-TEID,
	iE-Extensions		ProtocolExtensionContainer { {GTPTunnel-ExtIEs} } OPTIONAL,
	...
}

GTPTunnel-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GUAMI ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	aMFRegionID			AMFRegionID,
	aMFSetID			AMFSetID,
	aMFPointer			AMFPointer,
	iE-Extensions		ProtocolExtensionContainer { {GUAMI-ExtIEs} } OPTIONAL,
	...
}

GUAMI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


-- H

HandoverCommandTransfer ::= SEQUENCE {
	dLForwardingUP-TNLInformation		UPTransportLayerInformation						OPTIONAL,
	qosFlowToBeForwardedList			QosFlowToBeForwardedList						OPTIONAL,
	dataForwardingResponseDRBList		DataForwardingResponseDRBList					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {HandoverCommandTransfer-ExtIEs} } OPTIONAL,
	...
}

HandoverCommandTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AdditionalDLForwardingUPTNLInformation	CRITICALITY ignore	EXTENSION QosFlowPerTNLInformationList		PRESENCE optional}|
	{ ID id-ULForwardingUP-TNLInformation			CRITICALITY reject	EXTENSION UPTransportLayerInformation			PRESENCE optional}|
	{ ID id-AdditionalULForwardingUPTNLInformation	CRITICALITY reject	EXTENSION UPTransportLayerInformationList	PRESENCE optional},
	...
}

HandoverFlag ::= ENUMERATED {
	handover-preparation,
	...
}

HandoverPreparationUnsuccessfulTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {HandoverPreparationUnsuccessfulTransfer-ExtIEs} }	OPTIONAL,
	...
}

HandoverPreparationUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

HandoverRequestAcknowledgeTransfer ::= SEQUENCE {
	dL-NGU-UP-TNLInformation			UPTransportLayerInformation,
	dLForwardingUP-TNLInformation		UPTransportLayerInformation										OPTIONAL,
	securityResult						SecurityResult													OPTIONAL,
	qosFlowSetupResponseList			QosFlowListWithDataForwarding,
	qosFlowFailedToSetupList			QosFlowListWithCause											OPTIONAL,
	dataForwardingResponseDRBList		DataForwardingResponseDRBList									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {HandoverRequestAcknowledgeTransfer-ExtIEs} }	OPTIONAL,
	...
}

HandoverRequestAcknowledgeTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AdditionalDLUPTNLInformationForHOList		CRITICALITY ignore	EXTENSION AdditionalDLUPTNLInformationForHOList		PRESENCE optional	}|
	{ ID id-ULForwardingUP-TNLInformation				CRITICALITY reject	EXTENSION UPTransportLayerInformation					PRESENCE optional}|
	{ ID id-AdditionalULForwardingUPTNLInformation		CRITICALITY reject	EXTENSION UPTransportLayerInformationList				PRESENCE optional},
	...
}

HandoverRequiredTransfer ::= SEQUENCE {
	directForwardingPathAvailability		DirectForwardingPathAvailability				OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {HandoverRequiredTransfer-ExtIEs} }	OPTIONAL,
	...
}

HandoverRequiredTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

HandoverResourceAllocationUnsuccessfulTransfer ::= SEQUENCE {
	cause						Cause,
	criticalityDiagnostics		CriticalityDiagnostics																	OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {HandoverResourceAllocationUnsuccessfulTransfer-ExtIEs} }	OPTIONAL,
	...
}

HandoverResourceAllocationUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

HandoverType ::= ENUMERATED {
	intra5gs,
	fivegs-to-eps,
	eps-to-5gs,
	...
}

-- I

IMSVoiceSupportIndicator ::= ENUMERATED {
	supported,
	not-supported,
	...
}

IndexToRFSP ::= INTEGER (1..256, ...)

InfoOnRecommendedCellsAndRANNodesForPaging ::= SEQUENCE {
	recommendedCellsForPaging		RecommendedCellsForPaging,
	recommendRANNodesForPaging		RecommendedRANNodesForPaging,
	iE-Extensions		ProtocolExtensionContainer { {InfoOnRecommendedCellsAndRANNodesForPaging-ExtIEs} }	OPTIONAL,
	...
}

InfoOnRecommendedCellsAndRANNodesForPaging-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


IntegrityProtectionIndication ::= ENUMERATED {
	required,
	preferred,
	not-needed,
	...
}

IntegrityProtectionResult ::= ENUMERATED {
	performed,
	not-performed,
	...
}

IntendedNumberOfPagingAttempts ::= INTEGER (1..16, ...)

InterfacesToTrace ::= BIT STRING (SIZE(8))

-- J
-- K
-- L

LastVisitedCellInformation ::= CHOICE {
	nGRANCell		LastVisitedNGRANCellInformation,
	eUTRANCell		LastVisitedEUTRANCellInformation,
	uTRANCell		LastVisitedUTRANCellInformation,
	gERANCell		LastVisitedGERANCellInformation,
	choice-Extensions		ProtocolIE-SingleContainer { {LastVisitedCellInformation-ExtIEs} }
}

LastVisitedCellInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

LastVisitedCellItem ::= SEQUENCE {
	lastVisitedCellInformation		LastVisitedCellInformation,
	iE-Extensions		ProtocolExtensionContainer { {LastVisitedCellItem-ExtIEs} }	OPTIONAL,
	...
}

LastVisitedCellItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

LastVisitedEUTRANCellInformation ::= OCTET STRING

LastVisitedGERANCellInformation ::= OCTET STRING

LastVisitedNGRANCellInformation::= SEQUENCE {
	globalCellID								NGRAN-CGI,
	cellType									CellType,
	timeUEStayedInCell							TimeUEStayedInCell,
	timeUEStayedInCellEnhancedGranularity		TimeUEStayedInCellEnhancedGranularity 			OPTIONAL,
	hOCauseValue								Cause		 									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {LastVisitedNGRANCellInformation-ExtIEs} }	OPTIONAL,
	...
}

LastVisitedNGRANCellInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

LastVisitedUTRANCellInformation ::= OCTET STRING

LocationReportingAdditionalInfo ::= ENUMERATED {
	includePSCell,
	...
}

LocationReportingReferenceID ::= INTEGER (1..64, ...)

LocationReportingRequestType ::= SEQUENCE {
	eventType										EventType,
	reportArea										ReportArea,
	areaOfInterestList								AreaOfInterestList								OPTIONAL,
	locationReportingReferenceIDToBeCancelled		LocationReportingReferenceID					OPTIONAL,
-- The above IE shall be present if the event type is set to ¡°stop reporting UE presence in the area of interest¡±
	iE-Extensions		ProtocolExtensionContainer { {LocationReportingRequestType-ExtIEs} }		OPTIONAL,
	...
}

LocationReportingRequestType-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-LocationReportingAdditionalInfo	CRITICALITY ignore	EXTENSION LocationReportingAdditionalInfo		PRESENCE optional },
	...
}

-- M

MaskedIMEISV ::= BIT STRING (SIZE(64))

MaximumDataBurstVolume ::= INTEGER (0..4095, ...)

MessageIdentifier ::= BIT STRING (SIZE(16))

MaximumIntegrityProtectedDataRate ::= ENUMERATED {
	bitrate64kbs,
	maximum-UE-rate,
	...
}

MICOModeIndication ::= ENUMERATED {
	true,
	...
}

MobilityRestrictionList ::= SEQUENCE {
	servingPLMN					PLMNIdentity,
	equivalentPLMNs				EquivalentPLMNs											OPTIONAL,
	rATRestrictions				RATRestrictions											OPTIONAL,
	forbiddenAreaInformation	ForbiddenAreaInformation								OPTIONAL, 
	serviceAreaInformation		ServiceAreaInformation									OPTIONAL, 
	iE-Extensions		ProtocolExtensionContainer { {MobilityRestrictionList-ExtIEs} }	OPTIONAL,
	...
}

MobilityRestrictionList-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-LastEUTRAN-PLMNIdentity		CRITICALITY ignore	EXTENSION PLMNIdentity		PRESENCE optional		}|
	{ ID id-CNTypeRestrictionsForServing		CRITICALITY ignore	EXTENSION CNTypeRestrictionsForServing		PRESENCE optional}|
	{ ID id-CNTypeRestrictionsForEquivalent		CRITICALITY ignore	EXTENSION CNTypeRestrictionsForEquivalent		PRESENCE optional},
	...
}


-- N

N3IWF-ID ::= CHOICE {
	n3IWF-ID				BIT STRING (SIZE(16)),
	choice-Extensions		ProtocolIE-SingleContainer { {N3IWF-ID-ExtIEs} }
}

N3IWF-ID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

NAS-PDU ::= OCTET STRING

NASSecurityParametersFromNGRAN ::= OCTET STRING

NetworkInstance ::= INTEGER (1..256, ...)

NewSecurityContextInd ::= ENUMERATED {
	true,
	...
}

NextHopChainingCount ::= INTEGER (0..7)

NextPagingAreaScope ::= ENUMERATED {
	same,
	changed,
	...
}

NgENB-ID ::= CHOICE {
	macroNgENB-ID			BIT STRING (SIZE(20)),
	shortMacroNgENB-ID		BIT STRING (SIZE(18)),
	longMacroNgENB-ID		BIT STRING (SIZE(21)),
	choice-Extensions		ProtocolIE-SingleContainer { {NgENB-ID-ExtIEs} }
}

NgENB-ID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

NGRAN-CGI ::= CHOICE {
	nR-CGI			NR-CGI,
	eUTRA-CGI		EUTRA-CGI,
	choice-Extensions		ProtocolIE-SingleContainer { {NGRAN-CGI-ExtIEs} }
}

NGRAN-CGI-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

NGRAN-TNLAssociationToRemoveList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF NGRAN-TNLAssociationToRemoveItem

NGRAN-TNLAssociationToRemoveItem::= SEQUENCE {
	tNLAssociationTransportLayerAddress		CPTransportLayerInformation,
	tNLAssociationTransportLayerAddressAMF		CPTransportLayerInformation		OPTIONAL,
	iE-Extensions					ProtocolExtensionContainer { { NGRAN-TNLAssociationToRemoveItem-ExtIEs} } OPTIONAL
}

NGRAN-TNLAssociationToRemoveItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NGRANTraceID ::= OCTET STRING (SIZE(8))

NonDynamic5QIDescriptor ::= SEQUENCE {
	fiveQI						FiveQI,
	priorityLevelQos			PriorityLevelQos										OPTIONAL,
	averagingWindow				AveragingWindow											OPTIONAL,
	maximumDataBurstVolume		MaximumDataBurstVolume									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {NonDynamic5QIDescriptor-ExtIEs} }	OPTIONAL,
	...
}

NonDynamic5QIDescriptor-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NotAllowedTACs ::= SEQUENCE (SIZE(1..maxnoofAllowedAreas)) OF TAC

NotificationCause ::= ENUMERATED {
	fulfilled,
	not-fulfilled,
	...
}

NotificationControl ::= ENUMERATED {
	notification-requested,
	...
}

NRCellIdentity ::= BIT STRING (SIZE(36))

NR-CGI ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	nRCellIdentity		NRCellIdentity,
	iE-Extensions		ProtocolExtensionContainer { {NR-CGI-ExtIEs} } OPTIONAL,
	...
}

NR-CGI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NR-CGIList ::= SEQUENCE (SIZE(1..maxnoofCellsingNB)) OF NR-CGI

NR-CGIListForWarning ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF NR-CGI

NRencryptionAlgorithms ::= BIT STRING (SIZE(16, ...))

NRintegrityProtectionAlgorithms ::= BIT STRING (SIZE(16, ...))

NRPPa-PDU ::= OCTET STRING

NumberOfBroadcasts ::= INTEGER (0..65535)

NumberOfBroadcastsRequested ::= INTEGER (0..65535)

-- O

OverloadAction ::= ENUMERATED {
	reject-non-emergency-mo-dt,
	reject-rrc-cr-signalling,
	permit-emergency-sessions-and-mobile-terminated-services-only,
	permit-high-priority-sessions-and-mobile-terminated-services-only,
	...
}

OverloadResponse ::= CHOICE {
	overloadAction			OverloadAction,
	choice-Extensions		ProtocolIE-SingleContainer { {OverloadResponse-ExtIEs} }
}

OverloadResponse-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

OverloadStartNSSAIList ::= SEQUENCE (SIZE (1..maxnoofSliceItems)) OF OverloadStartNSSAIItem

OverloadStartNSSAIItem ::= SEQUENCE {
	sliceOverloadList						SliceOverloadList,
	sliceOverloadResponse					OverloadResponse								OPTIONAL,
	sliceTrafficLoadReductionIndication		TrafficLoadReductionIndication				OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {OverloadStartNSSAIItem-ExtIEs} }	OPTIONAL,
	...
}

OverloadStartNSSAIItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- P

PacketDelayBudget ::= INTEGER (0..1023, ...)

PacketErrorRate ::= SEQUENCE {
	pERScalar		INTEGER (0..9, ...),
	pERExponent		INTEGER (0..9, ...),
	iE-Extensions		ProtocolExtensionContainer { {PacketErrorRate-ExtIEs} }	OPTIONAL,
	...
}

PacketErrorRate-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PacketLossRate ::= INTEGER (0..1000, ...)

PagingAttemptInformation ::= SEQUENCE {
	pagingAttemptCount					PagingAttemptCount,
	intendedNumberOfPagingAttempts		IntendedNumberOfPagingAttempts,
	nextPagingAreaScope					NextPagingAreaScope									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PagingAttemptInformation-ExtIEs} }	OPTIONAL,
	...
}

PagingAttemptInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PagingAttemptCount ::= INTEGER (1..16, ...)

PagingDRX ::= ENUMERATED {
	v32,
	v64,
	v128,
	v256,
	...
}

PagingOrigin ::= ENUMERATED {
	non-3gpp,
	...
}

PagingPriority ::= ENUMERATED {
	priolevel1,
	priolevel2,
	priolevel3,
	priolevel4,
	priolevel5,
	priolevel6,
	priolevel7,
	priolevel8,
	...
}

PathSwitchRequestAcknowledgeTransfer ::= SEQUENCE {
	uL-NGU-UP-TNLInformation		UPTransportLayerInformation											OPTIONAL,
	securityIndication				SecurityIndication													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PathSwitchRequestAcknowledgeTransfer-ExtIEs} }	OPTIONAL,
	...
}

PathSwitchRequestAcknowledgeTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AdditionalNGU-UP-TNLInformation	CRITICALITY ignore	EXTENSION UPTransportLayerInformationPairList		PRESENCE optional	},
	...
}

PathSwitchRequestSetupFailedTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {PathSwitchRequestSetupFailedTransfer-ExtIEs} }	OPTIONAL,
	...
}

PathSwitchRequestSetupFailedTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PathSwitchRequestTransfer ::= SEQUENCE {
	dL-NGU-UP-TNLInformation			UPTransportLayerInformation,
	dL-NGU-TNLInformationReused			DL-NGU-TNLInformationReused							OPTIONAL,
	userPlaneSecurityInformation		UserPlaneSecurityInformation						OPTIONAL,
	qosFlowAcceptedList					QosFlowAcceptedList,
	iE-Extensions		ProtocolExtensionContainer { {PathSwitchRequestTransfer-ExtIEs} }	OPTIONAL,
	...
}

PathSwitchRequestTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AdditionalDLQosFlowPerTNLInformation	CRITICALITY ignore	EXTENSION QosFlowPerTNLInformationList	PRESENCE optional	},
	...
}

PathSwitchRequestUnsuccessfulTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {PathSwitchRequestUnsuccessfulTransfer-ExtIEs} }	OPTIONAL,
	...
}

PathSwitchRequestUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionAggregateMaximumBitRate ::= SEQUENCE {
	pDUSessionAggregateMaximumBitRateDL		BitRate,
	pDUSessionAggregateMaximumBitRateUL		BitRate,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionAggregateMaximumBitRate-ExtIEs} } OPTIONAL,
	...
}

PDUSessionAggregateMaximumBitRate-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionID ::= INTEGER (0..255)

PDUSessionResourceAdmittedList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceAdmittedItem

PDUSessionResourceAdmittedItem ::= SEQUENCE {
	pDUSessionID							PDUSessionID,
	handoverRequestAcknowledgeTransfer		OCTET STRING (CONTAINING HandoverRequestAcknowledgeTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceAdmittedItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceAdmittedItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToModifyListModCfm ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToModifyItemModCfm

PDUSessionResourceFailedToModifyItemModCfm ::= SEQUENCE {
	pDUSessionID												PDUSessionID,
	pDUSessionResourceModifyIndicationUnsuccessfulTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyIndicationUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToModifyItemModCfm-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToModifyItemModCfm-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToModifyListModRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToModifyItemModRes

PDUSessionResourceFailedToModifyItemModRes ::= SEQUENCE {
	pDUSessionID										PDUSessionID,
	pDUSessionResourceModifyUnsuccessfulTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToModifyItemModRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToModifyItemModRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToSetupListCxtFail ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToSetupItemCxtFail

PDUSessionResourceFailedToSetupItemCxtFail ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceSetupUnsuccessfulTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToSetupItemCxtFail-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToSetupItemCxtFail-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToSetupListCxtRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToSetupItemCxtRes

PDUSessionResourceFailedToSetupItemCxtRes ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceSetupUnsuccessfulTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToSetupItemCxtRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToSetupItemCxtRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToSetupListHOAck ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToSetupItemHOAck

PDUSessionResourceFailedToSetupItemHOAck ::= SEQUENCE {
	pDUSessionID										PDUSessionID,
	handoverResourceAllocationUnsuccessfulTransfer		OCTET STRING (CONTAINING HandoverResourceAllocationUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToSetupItemHOAck-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToSetupItemHOAck-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToSetupListPSReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToSetupItemPSReq

PDUSessionResourceFailedToSetupItemPSReq ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pathSwitchRequestSetupFailedTransfer		OCTET STRING (CONTAINING PathSwitchRequestSetupFailedTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToSetupItemPSReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToSetupItemPSReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToSetupListSURes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToSetupItemSURes

PDUSessionResourceFailedToSetupItemSURes ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceSetupUnsuccessfulTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToSetupItemSURes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToSetupItemSURes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceHandoverList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceHandoverItem

PDUSessionResourceHandoverItem ::= SEQUENCE {
	pDUSessionID						PDUSessionID,
	handoverCommandTransfer				OCTET STRING (CONTAINING HandoverCommandTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceHandoverItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceHandoverItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceInformationList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceInformationItem

PDUSessionResourceInformationItem ::= SEQUENCE {
	pDUSessionID					PDUSessionID,
	qosFlowInformationList			QosFlowInformationList,
	dRBsToQosFlowsMappingList		DRBsToQosFlowsMappingList										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceInformationItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceInformationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceListCxtRelCpl ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceItemCxtRelCpl

PDUSessionResourceItemCxtRelCpl ::= SEQUENCE {
	pDUSessionID		PDUSessionID,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceItemCxtRelCpl-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceItemCxtRelCpl-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-PDUSessionResourceReleaseResponseTransfer	CRITICALITY ignore	EXTENSION OCTET STRING (CONTAINING PDUSessionResourceReleaseResponseTransfer)	PRESENCE optional	},
	...
}

PDUSessionResourceListCxtRelReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceItemCxtRelReq

PDUSessionResourceItemCxtRelReq ::= SEQUENCE {
	pDUSessionID		PDUSessionID,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceItemCxtRelReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceItemCxtRelReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceListHORqd ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceItemHORqd

PDUSessionResourceItemHORqd ::= SEQUENCE {
	pDUSessionID							PDUSessionID,
	handoverRequiredTransfer				OCTET STRING (CONTAINING HandoverRequiredTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceItemHORqd-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceItemHORqd-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceModifyConfirmTransfer ::= SEQUENCE {
	qosFlowModifyConfirmList			QosFlowModifyConfirmList,
	uLNGU-UP-TNLInformation				UPTransportLayerInformation,
	additionalNG-UUPTNLInformation		UPTransportLayerInformationPairList									OPTIONAL,
	qosFlowFailedToModifyList			QosFlowListWithCause												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyConfirmTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyConfirmTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceModifyIndicationUnsuccessfulTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyIndicationUnsuccessfulTransfer-ExtIEs} }		OPTIONAL,
	...
}

PDUSessionResourceModifyIndicationUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceModifyRequestTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceModifyRequestTransferIEs} },
	...
}

PDUSessionResourceModifyRequestTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-PDUSessionAggregateMaximumBitRate	CRITICALITY reject	TYPE PDUSessionAggregateMaximumBitRate		PRESENCE	optional		}|
	{ ID id-UL-NGU-UP-TNLModifyList				CRITICALITY reject	TYPE UL-NGU-UP-TNLModifyList					PRESENCE	optional		}|
	{ ID id-NetworkInstance						CRITICALITY reject	TYPE NetworkInstance							PRESENCE optional		}|
	{ ID id-QosFlowAddOrModifyRequestList		CRITICALITY reject	TYPE QosFlowAddOrModifyRequestList			PRESENCE optional		}|
	{ ID id-QosFlowToReleaseList				CRITICALITY reject	TYPE QosFlowListWithCause						PRESENCE optional		}|
	{ ID id-AdditionalUL-NGU-UP-TNLInformation	CRITICALITY reject	TYPE UPTransportLayerInformationList		PRESENCE optional		}|
	{ ID id-CommonNetworkInstance				CRITICALITY ignore	TYPE CommonNetworkInstance						PRESENCE optional		},
	...
}	

PDUSessionResourceModifyResponseTransfer ::= SEQUENCE {
	dL-NGU-UP-TNLInformation				UPTransportLayerInformation											OPTIONAL,
	uL-NGU-UP-TNLInformation				UPTransportLayerInformation											OPTIONAL,
	qosFlowAddOrModifyResponseList			QosFlowAddOrModifyResponseList										OPTIONAL,
	additionalDLQosFlowPerTNLInformation	QosFlowPerTNLInformationList										OPTIONAL,
	qosFlowFailedToAddOrModifyList			QosFlowListWithCause												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyResponseTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyResponseTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AdditionalNGU-UP-TNLInformation	CRITICALITY ignore	EXTENSION UPTransportLayerInformationPairList	PRESENCE optional	},
	...
}

PDUSessionResourceModifyIndicationTransfer ::= SEQUENCE {
	dLQosFlowPerTNLInformation					QosFlowPerTNLInformation,
	additionalDLQosFlowPerTNLInformation		QosFlowPerTNLInformationList 									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyIndicationTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyIndicationTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-SecondaryRATUsageInformation		CRITICALITY ignore	EXTENSION SecondaryRATUsageInformation		PRESENCE optional	}|
	{ ID id-SecurityResult						CRITICALITY ignore	EXTENSION SecurityResult						PRESENCE optional	},
	...
}

PDUSessionResourceModifyListModCfm ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceModifyItemModCfm

PDUSessionResourceModifyItemModCfm ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pDUSessionResourceModifyConfirmTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyConfirmTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyItemModCfm-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyItemModCfm-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceModifyListModInd ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceModifyItemModInd

PDUSessionResourceModifyItemModInd ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceModifyIndicationTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyIndicationTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyItemModInd-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyItemModInd-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceModifyListModReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceModifyItemModReq

PDUSessionResourceModifyItemModReq ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	nAS-PDU										NAS-PDU													OPTIONAL,
	pDUSessionResourceModifyRequestTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyItemModReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyItemModReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-S-NSSAI		CRITICALITY reject	EXTENSION S-NSSAI		PRESENCE optional	},
	...
}

PDUSessionResourceModifyListModRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceModifyItemModRes

PDUSessionResourceModifyItemModRes ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceModifyResponseTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyResponseTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyItemModRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyItemModRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceModifyUnsuccessfulTransfer ::= SEQUENCE {
	cause						Cause,
	criticalityDiagnostics		CriticalityDiagnostics																OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyUnsuccessfulTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceNotifyList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceNotifyItem

PDUSessionResourceNotifyItem ::= SEQUENCE {
	pDUSessionID						PDUSessionID,
	pDUSessionResourceNotifyTransfer	OCTET STRING (CONTAINING PDUSessionResourceNotifyTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceNotifyItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceNotifyItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceNotifyReleasedTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceNotifyReleasedTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceNotifyReleasedTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {	
	{ ID id-SecondaryRATUsageInformation		CRITICALITY ignore	EXTENSION SecondaryRATUsageInformation		PRESENCE optional	},
	...
}

PDUSessionResourceNotifyTransfer ::= SEQUENCE {
	qosFlowNotifyList		QosFlowNotifyList														OPTIONAL,
	qosFlowReleasedList		QosFlowListWithCause													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceNotifyTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceNotifyTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-SecondaryRATUsageInformation		CRITICALITY ignore	EXTENSION SecondaryRATUsageInformation		PRESENCE optional	},
	...
}

PDUSessionResourceReleaseCommandTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleaseCommandTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleaseCommandTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceReleasedListNot ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceReleasedItemNot

PDUSessionResourceReleasedItemNot ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceNotifyReleasedTransfer		OCTET STRING (CONTAINING PDUSessionResourceNotifyReleasedTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleasedItemNot-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleasedItemNot-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceReleasedListPSAck ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceReleasedItemPSAck

PDUSessionResourceReleasedItemPSAck ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pathSwitchRequestUnsuccessfulTransfer		OCTET STRING (CONTAINING PathSwitchRequestUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleasedItemPSAck-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleasedItemPSAck-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceReleasedListPSFail ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceReleasedItemPSFail

PDUSessionResourceReleasedItemPSFail ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pathSwitchRequestUnsuccessfulTransfer		OCTET STRING (CONTAINING PathSwitchRequestUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleasedItemPSFail-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleasedItemPSFail-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceReleasedListRelRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceReleasedItemRelRes

PDUSessionResourceReleasedItemRelRes ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceReleaseResponseTransfer		OCTET STRING (CONTAINING PDUSessionResourceReleaseResponseTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleasedItemRelRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleasedItemRelRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceReleaseResponseTransfer ::= SEQUENCE {
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleaseResponseTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleaseResponseTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-SecondaryRATUsageInformation		CRITICALITY ignore	EXTENSION SecondaryRATUsageInformation		PRESENCE optional	},
	...
}

PDUSessionResourceSecondaryRATUsageList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSecondaryRATUsageItem

PDUSessionResourceSecondaryRATUsageItem ::= SEQUENCE {
	pDUSessionID							PDUSessionID,
	secondaryRATDataUsageReportTransfer		OCTET STRING (CONTAINING SecondaryRATDataUsageReportTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSecondaryRATUsageItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSecondaryRATUsageItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSetupListCxtReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSetupItemCxtReq

PDUSessionResourceSetupItemCxtReq ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	nAS-PDU										NAS-PDU												OPTIONAL,
	s-NSSAI										S-NSSAI,
	pDUSessionResourceSetupRequestTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupItemCxtReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupItemCxtReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSetupListCxtRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSetupItemCxtRes

PDUSessionResourceSetupItemCxtRes ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pDUSessionResourceSetupResponseTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupResponseTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupItemCxtRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupItemCxtRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSetupListHOReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSetupItemHOReq

PDUSessionResourceSetupItemHOReq ::= SEQUENCE {
	pDUSessionID				PDUSessionID,
	s-NSSAI						S-NSSAI,
	handoverRequestTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupItemHOReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupItemHOReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSetupListSUReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSetupItemSUReq

PDUSessionResourceSetupItemSUReq ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pDUSessionNAS-PDU							NAS-PDU												OPTIONAL,
	s-NSSAI										S-NSSAI,
	pDUSessionResourceSetupRequestTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupItemSUReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupItemSUReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSetupListSURes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSetupItemSURes

PDUSessionResourceSetupItemSURes ::= SEQUENCE {
	pDUSessionID											PDUSessionID,
	pDUSessionResourceSetupResponseTransfer					OCTET STRING (CONTAINING PDUSessionResourceSetupResponseTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupItemSURes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupItemSURes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSetupRequestTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceSetupRequestTransferIEs} },
	...
}

PDUSessionResourceSetupRequestTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-PDUSessionAggregateMaximumBitRate	CRITICALITY reject	TYPE PDUSessionAggregateMaximumBitRate		PRESENCE optional		}|
	{ ID id-UL-NGU-UP-TNLInformation			CRITICALITY reject	TYPE UPTransportLayerInformation				PRESENCE mandatory	}|
	{ ID id-AdditionalUL-NGU-UP-TNLInformation	CRITICALITY reject	TYPE UPTransportLayerInformationList		PRESENCE optional		}|
	{ ID id-DataForwardingNotPossible			CRITICALITY reject	TYPE DataForwardingNotPossible				PRESENCE optional		}|
	{ ID id-PDUSessionType						CRITICALITY reject	TYPE PDUSessionType								PRESENCE mandatory	}|
	{ ID id-SecurityIndication					CRITICALITY reject	TYPE SecurityIndication							PRESENCE optional		}|
	{ ID id-NetworkInstance						CRITICALITY reject	TYPE NetworkInstance							PRESENCE optional		}|
	{ ID id-QosFlowSetupRequestList				CRITICALITY reject	TYPE QosFlowSetupRequestList					PRESENCE mandatory	}|
	{ ID id-CommonNetworkInstance				CRITICALITY ignore	TYPE CommonNetworkInstance						PRESENCE optional	},
	...
}

PDUSessionResourceSetupResponseTransfer ::= SEQUENCE {
	dLQosFlowPerTNLInformation				QosFlowPerTNLInformation,
	additionalDLQosFlowPerTNLInformation	QosFlowPerTNLInformationList										OPTIONAL,
	securityResult							SecurityResult														OPTIONAL,
	qosFlowFailedToSetupList				QosFlowListWithCause												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupResponseTransfer-ExtIEs} }		OPTIONAL,
	...
}

PDUSessionResourceSetupResponseTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSetupUnsuccessfulTransfer ::= SEQUENCE {
	cause						Cause,
	criticalityDiagnostics		CriticalityDiagnostics																OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupUnsuccessfulTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSwitchedList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSwitchedItem

PDUSessionResourceSwitchedItem ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pathSwitchRequestAcknowledgeTransfer		OCTET STRING (CONTAINING PathSwitchRequestAcknowledgeTransfer),
	iE-Extensions		ProtocolExtensionContainer { { PDUSessionResourceSwitchedItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSwitchedItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceToBeSwitchedDLList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceToBeSwitchedDLItem

PDUSessionResourceToBeSwitchedDLItem ::= SEQUENCE {
	pDUSessionID					PDUSessionID,
	pathSwitchRequestTransfer		OCTET STRING (CONTAINING PathSwitchRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { { PDUSessionResourceToBeSwitchedDLItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceToBeSwitchedDLItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceToReleaseListHOCmd ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceToReleaseItemHOCmd

PDUSessionResourceToReleaseItemHOCmd ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	handoverPreparationUnsuccessfulTransfer		OCTET STRING (CONTAINING HandoverPreparationUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceToReleaseItemHOCmd-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceToReleaseItemHOCmd-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceToReleaseListRelCmd ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceToReleaseItemRelCmd

PDUSessionResourceToReleaseItemRelCmd ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceReleaseCommandTransfer		OCTET STRING (CONTAINING PDUSessionResourceReleaseCommandTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceToReleaseItemRelCmd-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceToReleaseItemRelCmd-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}
PDUSessionType ::= ENUMERATED {
	ipv4,
	ipv6,
	ipv4v6,
	ethernet,
	unstructured,
	...
}

PDUSessionUsageReport ::= SEQUENCE {
	rATType								ENUMERATED {nr, eutra, ...},
	pDUSessionTimedReportList			VolumeTimedReportList,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionUsageReport-ExtIEs} } OPTIONAL,
...
}

PDUSessionUsageReport-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PeriodicRegistrationUpdateTimer ::= BIT STRING (SIZE(8))

PLMNIdentity ::= OCTET STRING (SIZE(3)) 

PLMNSupportList ::= SEQUENCE (SIZE(1..maxnoofPLMNs)) OF PLMNSupportItem

PLMNSupportItem ::= SEQUENCE {
	pLMNIdentity			PLMNIdentity,
	sliceSupportList		SliceSupportList,
	iE-Extensions		ProtocolExtensionContainer { {PLMNSupportItem-ExtIEs} } OPTIONAL,
	...
}

PLMNSupportItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PortNumber ::= OCTET STRING (SIZE(2))

Pre-emptionCapability ::= ENUMERATED {
	shall-not-trigger-pre-emption,
	may-trigger-pre-emption,
	...
}

Pre-emptionVulnerability ::= ENUMERATED {
	not-pre-emptable,
	pre-emptable,
	...
}

PriorityLevelARP ::= INTEGER (1..15)

PriorityLevelQos ::= INTEGER (1..127, ...)

PWSFailedCellIDList ::= CHOICE {
	eUTRA-CGI-PWSFailedList		EUTRA-CGIList,
	nR-CGI-PWSFailedList		NR-CGIList,
	choice-Extensions		ProtocolIE-SingleContainer { {PWSFailedCellIDList-ExtIEs} }
}

PWSFailedCellIDList-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

-- Q

QosCharacteristics ::= CHOICE {
	nonDynamic5QI		NonDynamic5QIDescriptor,
	dynamic5QI			Dynamic5QIDescriptor,
	choice-Extensions		ProtocolIE-SingleContainer { {QosCharacteristics-ExtIEs} }
}

QosCharacteristics-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

QosFlowAcceptedList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowAcceptedItem

QosFlowAcceptedItem ::= SEQUENCE {
	qosFlowIdentifier		QosFlowIdentifier,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowAcceptedItem-ExtIEs} } OPTIONAL,
	...
}

QosFlowAcceptedItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowAddOrModifyRequestList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowAddOrModifyRequestItem

QosFlowAddOrModifyRequestItem ::= SEQUENCE {
	qosFlowIdentifier				QosFlowIdentifier,
	qosFlowLevelQosParameters		QosFlowLevelQosParameters									OPTIONAL,
	e-RAB-ID						E-RAB-ID													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowAddOrModifyRequestItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowAddOrModifyRequestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowAddOrModifyResponseList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowAddOrModifyResponseItem

QosFlowAddOrModifyResponseItem ::= SEQUENCE {
	qosFlowIdentifier		QosFlowIdentifier,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowAddOrModifyResponseItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowAddOrModifyResponseItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowIdentifier ::= INTEGER (0..63, ...)

QosFlowInformationList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowInformationItem

QosFlowInformationItem ::= SEQUENCE {
	qosFlowIdentifier	QosFlowIdentifier,
	dLForwarding		DLForwarding													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowInformationItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowInformationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-ULForwarding	CRITICALITY reject	EXTENSION ULForwarding	PRESENCE optional},
	...
}

QosFlowLevelQosParameters ::= SEQUENCE {
	qosCharacteristics					QosCharacteristics,
	allocationAndRetentionPriority		AllocationAndRetentionPriority,
	gBR-QosInformation					GBR-QosInformation									OPTIONAL,
	reflectiveQosAttribute				ReflectiveQosAttribute								OPTIONAL,
	additionalQosFlowInformation		AdditionalQosFlowInformation						OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowLevelQosParameters-ExtIEs} }	OPTIONAL,
	...
}

QosFlowLevelQosParameters-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowListWithCause ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowWithCauseItem

QosFlowWithCauseItem ::= SEQUENCE {
	qosFlowIdentifier		QosFlowIdentifier,
	cause					Cause,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowWithCauseItem-ExtIEs} } OPTIONAL,
	...
}

QosFlowWithCauseItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowModifyConfirmList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowModifyConfirmItem

QosFlowModifyConfirmItem ::= SEQUENCE {
	qosFlowIdentifier		QosFlowIdentifier,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowModifyConfirmItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowModifyConfirmItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowNotifyList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowNotifyItem

QosFlowNotifyItem ::= SEQUENCE {
	qosFlowIdentifier			QosFlowIdentifier,
	notificationCause			NotificationCause,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowNotifyItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowNotifyItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowPerTNLInformation ::= SEQUENCE {
	uPTransportLayerInformation		UPTransportLayerInformation,
	associatedQosFlowList			AssociatedQosFlowList,
	iE-Extensions		ProtocolExtensionContainer { { QosFlowPerTNLInformation-ExtIEs} }	OPTIONAL,
	...
}

QosFlowPerTNLInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowPerTNLInformationList ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivityMinusOne)) OF QosFlowPerTNLInformationItem

QosFlowPerTNLInformationItem ::= SEQUENCE {
	qosFlowPerTNLInformation				QosFlowPerTNLInformation,
	iE-Extensions		ProtocolExtensionContainer { { QosFlowPerTNLInformationItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowPerTNLInformationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowSetupRequestList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowSetupRequestItem

QosFlowSetupRequestItem ::= SEQUENCE {
	qosFlowIdentifier				QosFlowIdentifier,
	qosFlowLevelQosParameters		QosFlowLevelQosParameters,
	e-RAB-ID						E-RAB-ID											OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowSetupRequestItem-ExtIEs} } OPTIONAL,
	...
}

QosFlowSetupRequestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowListWithDataForwarding ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowItemWithDataForwarding

QosFlowItemWithDataForwarding ::= SEQUENCE {
	qosFlowIdentifier			QosFlowIdentifier,
	dataForwardingAccepted		DataForwardingAccepted											OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowItemWithDataForwarding-ExtIEs} }	OPTIONAL,
	...
}

QosFlowItemWithDataForwarding-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowSetupResponseListSURes ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowSetupResponseItemSURes

QosFlowSetupResponseItemSURes ::= SEQUENCE {
	qosFlowIdentifier		QosFlowIdentifier,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowSetupResponseItemSURes-ExtIEs} } OPTIONAL,
	...
}

QosFlowSetupResponseItemSURes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowToBeForwardedList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowToBeForwardedItem

QosFlowToBeForwardedItem ::= SEQUENCE {
	qosFlowIdentifier		QosFlowIdentifier,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowToBeForwardedItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowToBeForwardedItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QoSFlowsUsageReportList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QoSFlowsUsageReport-Item

QoSFlowsUsageReport-Item ::= SEQUENCE {
	qosFlowIdentifier					QosFlowIdentifier,
	rATType								ENUMERATED {nr, eutra, ...},
	qoSFlowsTimedReportList				VolumeTimedReportList,
	iE-Extensions		ProtocolExtensionContainer { {QoSFlowsUsageReport-Item-ExtIEs} } OPTIONAL,
...
}

QoSFlowsUsageReport-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- R

RANNodeName ::= PrintableString (SIZE(1..150, ...))

RANPagingPriority ::= INTEGER (1..256)

RANStatusTransfer-TransparentContainer ::= SEQUENCE {
	dRBsSubjectToStatusTransferList		DRBsSubjectToStatusTransferList,
	iE-Extensions		ProtocolExtensionContainer { {RANStatusTransfer-TransparentContainer-ExtIEs} }	OPTIONAL,
	...
}

RANStatusTransfer-TransparentContainer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

RAN-UE-NGAP-ID ::= INTEGER (0..4294967295)

RATRestrictions ::= SEQUENCE (SIZE(1..maxnoofEPLMNsPlusOne)) OF RATRestrictions-Item

RATRestrictions-Item ::= SEQUENCE {
	pLMNIdentity					PLMNIdentity,
	rATRestrictionInformation		RATRestrictionInformation,
	iE-Extensions		ProtocolExtensionContainer { {RATRestrictions-Item-ExtIEs} }		OPTIONAL,
	...
}

RATRestrictions-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

RATRestrictionInformation ::= BIT STRING (SIZE(8, ...))

RecommendedCellsForPaging ::= SEQUENCE {
	recommendedCellList			RecommendedCellList,
	iE-Extensions		ProtocolExtensionContainer { {RecommendedCellsForPaging-ExtIEs} }	OPTIONAL,
	...
}

RecommendedCellsForPaging-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

RecommendedCellList ::= SEQUENCE (SIZE(1..maxnoofRecommendedCells)) OF RecommendedCellItem

RecommendedCellItem ::= SEQUENCE {
	nGRAN-CGI				NGRAN-CGI,
	timeStayedInCell		INTEGER (0..4095)		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {RecommendedCellItem-ExtIEs} }	OPTIONAL,
	...
}

RecommendedCellItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

RecommendedRANNodesForPaging ::= SEQUENCE {
	recommendedRANNodeList		RecommendedRANNodeList,
	iE-Extensions		ProtocolExtensionContainer { {RecommendedRANNodesForPaging-ExtIEs} }	OPTIONAL,
	...
}

RecommendedRANNodesForPaging-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

RecommendedRANNodeList::= SEQUENCE (SIZE(1..maxnoofRecommendedRANNodes)) OF RecommendedRANNodeItem

RecommendedRANNodeItem ::= SEQUENCE {
	aMFPagingTarget		AMFPagingTarget,
	iE-Extensions		ProtocolExtensionContainer { {RecommendedRANNodeItem-ExtIEs} }	OPTIONAL,
	...
}

RecommendedRANNodeItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

RedirectionVoiceFallback ::= ENUMERATED {
	possible,
	not-possible,
	...
}

ReflectiveQosAttribute ::= ENUMERATED {
	subject-to,
	...
}

ReferenceID ::= INTEGER (1..64, ...)

RelativeAMFCapacity ::= INTEGER (0..255)

ReportArea ::= ENUMERATED {
	cell,
	...
}

RepetitionPeriod ::= INTEGER (0..131071)

ResetAll ::= ENUMERATED {
	reset-all,
	...
}

ResetType ::= CHOICE {
	nG-Interface			ResetAll,
	partOfNG-Interface		UE-associatedLogicalNG-connectionList,
	choice-Extensions		ProtocolIE-SingleContainer { {ResetType-ExtIEs} }
}

ResetType-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

RoutingID ::= OCTET STRING

RRCContainer ::= OCTET STRING

RRCEstablishmentCause ::= ENUMERATED {
	emergency,
	highPriorityAccess,
	mt-Access,
	mo-Signalling,
	mo-Data,
	mo-VoiceCall,
	mo-VideoCall,
	mo-SMS,
	mps-PriorityAccess,
	mcs-PriorityAccess,
	...,
	notAvailable
}

RRCInactiveTransitionReportRequest ::= ENUMERATED {
	subsequent-state-transition-report,
	single-rrc-connected-state-report,
	cancel-report,
	...
}

RRCState ::= ENUMERATED {
	inactive,
	connected,
	...
}

-- S

SCTP-TLAs	::= SEQUENCE (SIZE(1..maxnoofXnTLAs)) OF TransportLayerAddress

SD ::= OCTET STRING (SIZE(3))

SecondaryRATUsageInformation ::= SEQUENCE {
	pDUSessionUsageReport		PDUSessionUsageReport											OPTIONAL,
	qosFlowsUsageReportList		QoSFlowsUsageReportList											OPTIONAL,
	iE-Extension		ProtocolExtensionContainer { {SecondaryRATUsageInformation-ExtIEs} }	OPTIONAL,
	...
}

SecondaryRATUsageInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SecondaryRATDataUsageReportTransfer ::= SEQUENCE {
	secondaryRATUsageInformation		SecondaryRATUsageInformation									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {SecondaryRATDataUsageReportTransfer-ExtIEs} }	OPTIONAL,
	...
}

SecondaryRATDataUsageReportTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SecurityContext ::= SEQUENCE {
	nextHopChainingCount		NextHopChainingCount,
	nextHopNH					SecurityKey,
	iE-Extensions		ProtocolExtensionContainer { {SecurityContext-ExtIEs} }	OPTIONAL,
	...
}

SecurityContext-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SecurityIndication ::= SEQUENCE {
	integrityProtectionIndication			IntegrityProtectionIndication,
	confidentialityProtectionIndication		ConfidentialityProtectionIndication,
	maximumIntegrityProtectedDataRate-UL	MaximumIntegrityProtectedDataRate		OPTIONAL,
-- The above IE shall be present if integrity protection is required or preferred
	iE-Extensions		ProtocolExtensionContainer { {SecurityIndication-ExtIEs} }	OPTIONAL,
	...
}

SecurityIndication-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-MaximumIntegrityProtectedDataRate-DL	CRITICALITY ignore	EXTENSION MaximumIntegrityProtectedDataRate	PRESENCE optional	},
	...
}

SecurityKey	::= BIT STRING (SIZE(256))

SecurityResult ::= SEQUENCE {
	integrityProtectionResult			IntegrityProtectionResult,
	confidentialityProtectionResult		ConfidentialityProtectionResult,
	iE-Extensions		ProtocolExtensionContainer { {SecurityResult-ExtIEs} }	OPTIONAL,
	...
}

SecurityResult-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SerialNumber ::= BIT STRING (SIZE(16))

ServedGUAMIList ::= SEQUENCE (SIZE(1..maxnoofServedGUAMIs)) OF ServedGUAMIItem

ServedGUAMIItem ::= SEQUENCE {
	gUAMI				GUAMI,
	backupAMFName		AMFName													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {ServedGUAMIItem-ExtIEs} }	OPTIONAL,
	...
}

ServedGUAMIItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ServiceAreaInformation ::= SEQUENCE (SIZE(1.. maxnoofEPLMNsPlusOne)) OF ServiceAreaInformation-Item

ServiceAreaInformation-Item ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	allowedTACs			AllowedTACs																OPTIONAL,
	notAllowedTACs		NotAllowedTACs															OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {ServiceAreaInformation-Item-ExtIEs} }		OPTIONAL,
	...
}

ServiceAreaInformation-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


SliceOverloadList ::= SEQUENCE (SIZE(1..maxnoofSliceItems)) OF SliceOverloadItem

SliceOverloadItem ::= SEQUENCE {
	s-NSSAI				S-NSSAI,
	iE-Extensions		ProtocolExtensionContainer { {SliceOverloadItem-ExtIEs} }	OPTIONAL,
	...
}

SliceOverloadItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SliceSupportList ::= SEQUENCE (SIZE(1..maxnoofSliceItems)) OF SliceSupportItem

SliceSupportItem ::= SEQUENCE {
	s-NSSAI				S-NSSAI,
	iE-Extensions		ProtocolExtensionContainer { {SliceSupportItem-ExtIEs} }	OPTIONAL,
	...
}

SliceSupportItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

S-NSSAI ::= SEQUENCE {
	sST					SST,
	sD					SD													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { S-NSSAI-ExtIEs} }	OPTIONAL,
	...
}

S-NSSAI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SONConfigurationTransfer ::= SEQUENCE {
	targetRANNodeID				TargetRANNodeID,
	sourceRANNodeID				SourceRANNodeID,
	sONInformation				SONInformation,
	xnTNLConfigurationInfo		XnTNLConfigurationInfo										OPTIONAL,
-- The above IE shall be present if the SON Information IE contains the SON Information Request IE set to ¡°Xn TNL Configuration Info¡±
	iE-Extensions		ProtocolExtensionContainer { {SONConfigurationTransfer-ExtIEs} }	OPTIONAL,
	...
}

SONConfigurationTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SONInformation ::= CHOICE {
	sONInformationRequest		SONInformationRequest,
	sONInformationReply			SONInformationReply,
	choice-Extensions		ProtocolIE-SingleContainer { {SONInformation-ExtIEs} }
}

SONInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

SONInformationReply ::= SEQUENCE {
	xnTNLConfigurationInfo		XnTNLConfigurationInfo									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {SONInformationReply-ExtIEs} }		OPTIONAL,
	...
}

SONInformationReply-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SONInformationRequest ::= ENUMERATED { 
	xn-TNL-configuration-info,
	...
}

SourceNGRANNode-ToTargetNGRANNode-TransparentContainer ::= SEQUENCE {
	rRCContainer							RRCContainer,
	pDUSessionResourceInformationList		PDUSessionResourceInformationList													OPTIONAL,
	e-RABInformationList					E-RABInformationList																OPTIONAL,
	targetCell-ID							NGRAN-CGI,
	indexToRFSP								IndexToRFSP																			OPTIONAL,
	uEHistoryInformation					UEHistoryInformation,
	iE-Extensions		ProtocolExtensionContainer { {SourceNGRANNode-ToTargetNGRANNode-TransparentContainer-ExtIEs} }	OPTIONAL,
	...
}

SourceNGRANNode-ToTargetNGRANNode-TransparentContainer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SourceOfUEActivityBehaviourInformation ::= ENUMERATED {
	subscription-information,
	statistics,
	...
}

SourceRANNodeID ::= SEQUENCE {
	globalRANNodeID		GlobalRANNodeID,
	selectedTAI			TAI,
	iE-Extensions		ProtocolExtensionContainer { {SourceRANNodeID-ExtIEs} } OPTIONAL,
	...
}

SourceRANNodeID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SourceToTarget-TransparentContainer ::= OCTET STRING
-- This IE includes a transparent container from the source RAN node to the target RAN node. 
-- The octets of the OCTET STRING are encoded according to the specifications of the target system.

SourceToTarget-AMFInformationReroute ::= SEQUENCE {
configuredNSSAI						ConfiguredNSSAI													OPTIONAL,
rejectedNSSAIinPLMN					RejectedNSSAIinPLMN												OPTIONAL,
rejectedNSSAIinTA						RejectedNSSAIinTA													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {SourceToTarget-AMFInformationReroute-ExtIEs} }	OPTIONAL,
	...
}

SourceToTarget-AMFInformationReroute-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- This IE includes information from the source Core node to the target Core node for reroute information provide by NSSF. 
-- The octets of the OCTET STRING are encoded according to the specifications of the Core network.


ConfiguredNSSAI  ::=  OCTET STRING (SIZE(128))

RejectedNSSAIinPLMN ::= OCTET STRING (SIZE(32))

RejectedNSSAIinTA ::= OCTET STRING (SIZE(32))

SST ::= OCTET STRING (SIZE(1))

SupportedTAList ::= SEQUENCE (SIZE(1..maxnoofTACs)) OF SupportedTAItem

SupportedTAItem ::= SEQUENCE {
	tAC									TAC,
	broadcastPLMNList		BroadcastPLMNList,
	iE-Extensions		ProtocolExtensionContainer { {SupportedTAItem-ExtIEs} } OPTIONAL,
	...
}

SupportedTAItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- T

TAC ::= OCTET STRING (SIZE(3))

TAI ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	tAC					TAC,
	iE-Extensions		ProtocolExtensionContainer { {TAI-ExtIEs} } OPTIONAL,
	...
}

TAI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIBroadcastEUTRA ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAIBroadcastEUTRA-Item

TAIBroadcastEUTRA-Item ::= SEQUENCE {
	tAI								TAI,
	completedCellsInTAI-EUTRA		CompletedCellsInTAI-EUTRA,
	iE-Extensions		ProtocolExtensionContainer { {TAIBroadcastEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

TAIBroadcastEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIBroadcastNR ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAIBroadcastNR-Item

TAIBroadcastNR-Item ::= SEQUENCE {
	tAI							TAI,
	completedCellsInTAI-NR		CompletedCellsInTAI-NR,
	iE-Extensions		ProtocolExtensionContainer { {TAIBroadcastNR-Item-ExtIEs} } OPTIONAL,
	...
}

TAIBroadcastNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAICancelledEUTRA ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAICancelledEUTRA-Item

TAICancelledEUTRA-Item ::= SEQUENCE {
	tAI								TAI,
	cancelledCellsInTAI-EUTRA		CancelledCellsInTAI-EUTRA,
	iE-Extensions		ProtocolExtensionContainer { {TAICancelledEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

TAICancelledEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAICancelledNR ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAICancelledNR-Item

TAICancelledNR-Item ::= SEQUENCE {
	tAI							TAI,
	cancelledCellsInTAI-NR		CancelledCellsInTAI-NR,
	iE-Extensions		ProtocolExtensionContainer { {TAICancelledNR-Item-ExtIEs} } OPTIONAL,
	...
}

TAICancelledNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIListForInactive ::= SEQUENCE (SIZE(1..maxnoofTAIforInactive)) OF TAIListForInactiveItem

TAIListForInactiveItem ::= SEQUENCE {
	tAI					TAI,
	iE-Extensions		ProtocolExtensionContainer { {TAIListForInactiveItem-ExtIEs} } OPTIONAL,
	...
}

TAIListForInactiveItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIListForPaging ::= SEQUENCE (SIZE(1..maxnoofTAIforPaging)) OF TAIListForPagingItem

TAIListForPagingItem ::= SEQUENCE {
	tAI					TAI,
	iE-Extensions		ProtocolExtensionContainer { {TAIListForPagingItem-ExtIEs} } OPTIONAL,
	...
}

TAIListForPagingItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIListForRestart ::= SEQUENCE (SIZE(1..maxnoofTAIforRestart)) OF TAI

TAIListForWarning ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAI

TargeteNB-ID ::= SEQUENCE {
	globalENB-ID		GlobalNgENB-ID,
	selected-EPS-TAI	EPS-TAI,
	iE-Extensions		ProtocolExtensionContainer { {TargeteNB-ID-ExtIEs} } OPTIONAL,
	...
}

TargeteNB-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TargetID ::= CHOICE {
	targetRANNodeID		TargetRANNodeID,
	targeteNB-ID		TargeteNB-ID,
	choice-Extensions		ProtocolIE-SingleContainer { {TargetID-ExtIEs} }
}

TargetID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

TargetNGRANNode-ToSourceNGRANNode-TransparentContainer ::= SEQUENCE {
	rRCContainer		RRCContainer,
	iE-Extensions		ProtocolExtensionContainer { {TargetNGRANNode-ToSourceNGRANNode-TransparentContainer-ExtIEs} } OPTIONAL,
	...
}

TargetNGRANNode-ToSourceNGRANNode-TransparentContainer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TargetRANNodeID ::= SEQUENCE {
	globalRANNodeID		GlobalRANNodeID,
	selectedTAI			TAI,
	iE-Extensions		ProtocolExtensionContainer { {TargetRANNodeID-ExtIEs} } OPTIONAL,
	...
}

TargetRANNodeID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TargetToSource-TransparentContainer ::= OCTET STRING
-- This IE includes a transparent container from the target RAN node to the source RAN node. 
-- The octets of the OCTET STRING are encoded according to the specifications of the target system.

TimerApproachForGUAMIRemoval ::= ENUMERATED { 
	apply-timer,
	...
}

TimeStamp ::= OCTET STRING (SIZE(4))

TimeToWait ::= ENUMERATED {v1s, v2s, v5s, v10s, v20s, v60s, ...}

TimeUEStayedInCell ::= INTEGER (0..4095)

TimeUEStayedInCellEnhancedGranularity ::= INTEGER (0..40950)

TNLAddressWeightFactor ::= INTEGER (0..255)

TNLAssociationList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF TNLAssociationItem

TNLAssociationItem ::= SEQUENCE {
	tNLAssociationAddress		CPTransportLayerInformation,
	cause						Cause,
	iE-Extensions		ProtocolExtensionContainer { {TNLAssociationItem-ExtIEs} } OPTIONAL,
	...
}

TNLAssociationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TNLAssociationUsage ::= ENUMERATED { 
	ue,
	non-ue,
	both,
	...
}

TraceActivation ::= SEQUENCE {
	nGRANTraceID						NGRANTraceID,
	interfacesToTrace					InterfacesToTrace,
     traceDepth							TraceDepth,
     traceCollectionEntityIPAddress		TransportLayerAddress,
	iE-Extensions		ProtocolExtensionContainer { {TraceActivation-ExtIEs} }	OPTIONAL,
	...
}

TraceActivation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TraceDepth ::= ENUMERATED { 
	minimum,
	medium,
	maximum,
	minimumWithoutVendorSpecificExtension,
	mediumWithoutVendorSpecificExtension,
	maximumWithoutVendorSpecificExtension,
	...
}

TrafficLoadReductionIndication ::= INTEGER (1..99)

TransportLayerAddress ::= BIT STRING (SIZE(1..160, ...))

TypeOfError ::= ENUMERATED {
	not-understood,
	missing,
	...
}

-- U

UEAggregateMaximumBitRate ::= SEQUENCE {
	uEAggregateMaximumBitRateDL		BitRate,
	uEAggregateMaximumBitRateUL		BitRate,
	iE-Extensions		ProtocolExtensionContainer { {UEAggregateMaximumBitRate-ExtIEs} } OPTIONAL,
	...
}

UEAggregateMaximumBitRate-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UE-associatedLogicalNG-connectionList ::= SEQUENCE (SIZE(1..maxnoofNGConnectionsToReset)) OF UE-associatedLogicalNG-connectionItem

UE-associatedLogicalNG-connectionItem ::= SEQUENCE {
	aMF-UE-NGAP-ID		AMF-UE-NGAP-ID																		OPTIONAL,
	rAN-UE-NGAP-ID		RAN-UE-NGAP-ID																		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UE-associatedLogicalNG-connectionItem-ExtIEs} }	OPTIONAL,
	...
}

UE-associatedLogicalNG-connectionItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...}

UEContextRequest ::= ENUMERATED {requested, ...}

UEHistoryInformation ::= SEQUENCE (SIZE(1..maxnoofCellsinUEHistoryInfo)) OF LastVisitedCellItem

UEIdentityIndexValue ::= CHOICE {
	indexLength10			BIT STRING (SIZE(10)),
	choice-Extensions		ProtocolIE-SingleContainer { {UEIdentityIndexValue-ExtIEs} }
}

UEIdentityIndexValue-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

UE-NGAP-IDs ::= CHOICE {
	uE-NGAP-ID-pair		UE-NGAP-ID-pair,
	aMF-UE-NGAP-ID		AMF-UE-NGAP-ID,
	choice-Extensions		ProtocolIE-SingleContainer { {UE-NGAP-IDs-ExtIEs} }
}

UE-NGAP-IDs-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

UE-NGAP-ID-pair ::= SEQUENCE{
	aMF-UE-NGAP-ID		AMF-UE-NGAP-ID,
	rAN-UE-NGAP-ID		RAN-UE-NGAP-ID,
	iE-Extensions		ProtocolExtensionContainer { {UE-NGAP-ID-pair-ExtIEs} } OPTIONAL,
	...
}

UE-NGAP-ID-pair-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UEPagingIdentity ::= CHOICE {
	fiveG-S-TMSI		FiveG-S-TMSI,
	choice-Extensions		ProtocolIE-SingleContainer { {UEPagingIdentity-ExtIEs} }
	}

UEPagingIdentity-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

UEPresence ::= ENUMERATED {in, out, unknown, ...}

UEPresenceInAreaOfInterestList ::= SEQUENCE (SIZE(1..maxnoofAoI)) OF UEPresenceInAreaOfInterestItem

UEPresenceInAreaOfInterestItem ::= SEQUENCE {
	locationReportingReferenceID		LocationReportingReferenceID,
	uEPresence							UEPresence,
	iE-Extensions		ProtocolExtensionContainer { {UEPresenceInAreaOfInterestItem-ExtIEs} }	OPTIONAL,
	...
}

UEPresenceInAreaOfInterestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UERadioCapability ::= OCTET STRING

UERadioCapabilityForPaging ::= SEQUENCE {
	uERadioCapabilityForPagingOfNR		UERadioCapabilityForPagingOfNR			OPTIONAL,
	uERadioCapabilityForPagingOfEUTRA		UERadioCapabilityForPagingOfEUTRA		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UERadioCapabilityForPaging-ExtIEs} }	OPTIONAL,
	...
}

UERadioCapabilityForPaging-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UERadioCapabilityForPagingOfNR ::= OCTET STRING

UERadioCapabilityForPagingOfEUTRA ::= OCTET STRING

UERetentionInformation ::= ENUMERATED {
	ues-retained,
	...
}

UESecurityCapabilities ::= SEQUENCE {
	nRencryptionAlgorithms					NRencryptionAlgorithms,
	nRintegrityProtectionAlgorithms			NRintegrityProtectionAlgorithms,
	eUTRAencryptionAlgorithms				EUTRAencryptionAlgorithms,
	eUTRAintegrityProtectionAlgorithms		EUTRAintegrityProtectionAlgorithms,

	iE-Extensions		ProtocolExtensionContainer { {UESecurityCapabilities-ExtIEs} }	OPTIONAL,
	...
}

UESecurityCapabilities-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UL-NGU-UP-TNLModifyList ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivity)) OF UL-NGU-UP-TNLModifyItem

UL-NGU-UP-TNLModifyItem ::= SEQUENCE {
	uL-NGU-UP-TNLInformation		UPTransportLayerInformation,
	dL-NGU-UP-TNLInformation		UPTransportLayerInformation,
	iE-Extensions		ProtocolExtensionContainer { {UL-NGU-UP-TNLModifyItem-ExtIEs} } OPTIONAL,
	...
}

UL-NGU-UP-TNLModifyItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UnavailableGUAMIList ::= SEQUENCE (SIZE(1..maxnoofServedGUAMIs)) OF UnavailableGUAMIItem

UnavailableGUAMIItem ::= SEQUENCE {
	gUAMI								GUAMI,
	timerApproachForGUAMIRemoval		TimerApproachForGUAMIRemoval					OPTIONAL,
	backupAMFName						AMFName											OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UnavailableGUAMIItem-ExtIEs} }	OPTIONAL,
	...
}

UnavailableGUAMIItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ULForwarding ::= ENUMERATED {
	ul-forwarding-proposed,
	...
}

UPTransportLayerInformation ::= CHOICE {
	gTPTunnel				GTPTunnel,
	choice-Extensions		ProtocolIE-SingleContainer { {UPTransportLayerInformation-ExtIEs} }
}

UPTransportLayerInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

UPTransportLayerInformationList ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivityMinusOne)) OF UPTransportLayerInformationItem

UPTransportLayerInformationItem ::= SEQUENCE {
	nGU-UP-TNLInformation		UPTransportLayerInformation,
	iE-Extensions		ProtocolExtensionContainer { {UPTransportLayerInformationItem-ExtIEs} } OPTIONAL,
	...
}

UPTransportLayerInformationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


UPTransportLayerInformationPairList ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivityMinusOne)) OF UPTransportLayerInformationPairItem

UPTransportLayerInformationPairItem ::= SEQUENCE {
	uL-NGU-UP-TNLInformation		UPTransportLayerInformation,
	dL-NGU-UP-TNLInformation		UPTransportLayerInformation,
	iE-Extensions		ProtocolExtensionContainer { {UPTransportLayerInformationPairItem-ExtIEs} } OPTIONAL,
	...
}

UPTransportLayerInformationPairItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UserLocationInformation ::= CHOICE {
	userLocationInformationEUTRA	UserLocationInformationEUTRA,
	userLocationInformationNR		UserLocationInformationNR,
	userLocationInformationN3IWF	UserLocationInformationN3IWF,
	choice-Extensions		ProtocolIE-SingleContainer { {UserLocationInformation-ExtIEs} }
}

UserLocationInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

UserLocationInformationEUTRA ::= SEQUENCE {
	eUTRA-CGI			EUTRA-CGI,
	tAI					TAI,
	timeStamp			TimeStamp																OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UserLocationInformationEUTRA-ExtIEs} }	OPTIONAL,
	...
}

UserLocationInformationEUTRA-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-PSCellInformation	CRITICALITY ignore	EXTENSION NGRAN-CGI				PRESENCE optional},
	...
}

UserLocationInformationN3IWF ::= SEQUENCE {
	iPAddress			TransportLayerAddress,
	portNumber			PortNumber,
	iE-Extensions		ProtocolExtensionContainer { {UserLocationInformationN3IWF-ExtIEs} }	OPTIONAL,
	...
}

UserLocationInformationN3IWF-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UserLocationInformationNR ::= SEQUENCE {
	nR-CGI				NR-CGI,
	tAI					TAI,
	timeStamp			TimeStamp															OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UserLocationInformationNR-ExtIEs} }	OPTIONAL,
	...
}

UserLocationInformationNR-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-PSCellInformation	CRITICALITY ignore	EXTENSION NGRAN-CGI				PRESENCE optional},
	...
}

UserPlaneSecurityInformation ::= SEQUENCE {
	securityResult			SecurityResult,
	securityIndication		SecurityIndication,
	iE-Extensions		ProtocolExtensionContainer { {UserPlaneSecurityInformation-ExtIEs} }	OPTIONAL,
	...
}

UserPlaneSecurityInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- V

VolumeTimedReportList ::= SEQUENCE (SIZE(1..maxnoofTimePeriods)) OF VolumeTimedReport-Item

VolumeTimedReport-Item ::= SEQUENCE {
	startTimeStamp				OCTET STRING (SIZE(4)),
	endTimeStamp				OCTET STRING (SIZE(4)),
	usageCountUL				INTEGER (0..18446744073709551615),
	usageCountDL				INTEGER (0..18446744073709551615),
	iE-Extensions		ProtocolExtensionContainer { {VolumeTimedReport-Item-ExtIEs} } OPTIONAL,
...
}

VolumeTimedReport-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- W

WarningAreaCoordinates ::= OCTET STRING (SIZE(1..1024))

WarningAreaList ::= CHOICE {
	eUTRA-CGIListForWarning			EUTRA-CGIListForWarning,
	nR-CGIListForWarning			NR-CGIListForWarning,
	tAIListForWarning				TAIListForWarning,
	emergencyAreaIDList				EmergencyAreaIDList,
	choice-Extensions		ProtocolIE-SingleContainer { {WarningAreaList-ExtIEs} }
}

WarningAreaList-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

WarningMessageContents ::= OCTET STRING (SIZE(1..9600))

WarningSecurityInfo ::= OCTET STRING (SIZE(50))

WarningType ::= OCTET STRING (SIZE(2))

-- X

XnExtTLAs ::= SEQUENCE (SIZE(1..maxnoofXnExtTLAs)) OF XnExtTLA-Item

XnExtTLA-Item ::= SEQUENCE {
	iPsecTLA					TransportLayerAddress		OPTIONAL,
	gTP-TLAs					XnGTP-TLAs					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {XnExtTLA-Item-ExtIEs} } OPTIONAL,
	...
}

XnExtTLA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-SCTP-TLAs		CRITICALITY ignore	EXTENSION SCTP-TLAs		PRESENCE optional },
	...
}

XnGTP-TLAs ::= SEQUENCE (SIZE(1..maxnoofXnGTP-TLAs)) OF TransportLayerAddress

XnTLAs ::= SEQUENCE (SIZE(1..maxnoofXnTLAs)) OF TransportLayerAddress

XnTNLConfigurationInfo ::= SEQUENCE {
	xnTransportLayerAddresses			XnTLAs,
	xnExtendedTransportLayerAddresses	XnExtTLAs										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {XnTNLConfigurationInfo-ExtIEs} }	OPTIONAL,
	...
}

XnTNLConfigurationInfo-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- Y
-- Z

END
-- ASN1STOP

-- ASN1START
-- **************************************************************
--
-- Common definitions
--
-- **************************************************************

NGAP-CommonDataTypes {
itu-t (0) identified-organization (4) etsi (0) mobileDomain (0) 
ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-CommonDataTypes (3) }

DEFINITIONS AUTOMATIC TAGS ::= 

BEGIN

Criticality		::= ENUMERATED { reject, ignore, notify }

Presence		::= ENUMERATED { optional, conditional, mandatory }

PrivateIE-ID	::= CHOICE {
	local				INTEGER (0..65535),
	global				OBJECT IDENTIFIER
}

ProcedureCode		::= INTEGER (0..255)

ProtocolExtensionID	::= INTEGER (0..65535)

ProtocolIE-ID		::= INTEGER (0..65535)

TriggeringMessage	::= ENUMERATED { initiating-message, successful-outcome, unsuccessfull-outcome }

END
-- ASN1STOP

-- ASN1START
-- **************************************************************
--
-- Constant definitions
--
-- **************************************************************

NGAP-Constants { 
itu-t (0) identified-organization (4) etsi (0) mobileDomain (0) 
ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-Constants (4) } 

DEFINITIONS AUTOMATIC TAGS ::= 

BEGIN

-- **************************************************************
--
-- IE parameter types from other modules.
--
-- **************************************************************

IMPORTS

	ProcedureCode,
	ProtocolIE-ID
FROM NGAP-CommonDataTypes;


-- **************************************************************
--
-- Elementary Procedures
--
-- **************************************************************

id-AMFConfigurationUpdate					ProcedureCode ::= 0
id-AMFStatusIndication						ProcedureCode ::= 1
id-CellTrafficTrace							ProcedureCode ::= 2
id-DeactivateTrace							ProcedureCode ::= 3
id-DownlinkNASTransport						ProcedureCode ::= 4
id-DownlinkNonUEAssociatedNRPPaTransport	ProcedureCode ::= 5
id-DownlinkRANConfigurationTransfer			ProcedureCode ::= 6
id-DownlinkRANStatusTransfer				ProcedureCode ::= 7
id-DownlinkUEAssociatedNRPPaTransport		ProcedureCode ::= 8
id-ErrorIndication							ProcedureCode ::= 9
id-HandoverCancel							ProcedureCode ::= 10
id-HandoverNotification						ProcedureCode ::= 11
id-HandoverPreparation						ProcedureCode ::= 12
id-HandoverResourceAllocation				ProcedureCode ::= 13
id-InitialContextSetup						ProcedureCode ::= 14
id-InitialUEMessage							ProcedureCode ::= 15
id-LocationReportingControl					ProcedureCode ::= 16
id-LocationReportingFailureIndication		ProcedureCode ::= 17
id-LocationReport							ProcedureCode ::= 18
id-NASNonDeliveryIndication					ProcedureCode ::= 19
id-NGReset									ProcedureCode ::= 20
id-NGSetup									ProcedureCode ::= 21
id-OverloadStart							ProcedureCode ::= 22
id-OverloadStop								ProcedureCode ::= 23
id-Paging									ProcedureCode ::= 24
id-PathSwitchRequest						ProcedureCode ::= 25
id-PDUSessionResourceModify					ProcedureCode ::= 26
id-PDUSessionResourceModifyIndication		ProcedureCode ::= 27
id-PDUSessionResourceRelease				ProcedureCode ::= 28
id-PDUSessionResourceSetup					ProcedureCode ::= 29
id-PDUSessionResourceNotify					ProcedureCode ::= 30
id-PrivateMessage							ProcedureCode ::= 31
id-PWSCancel								ProcedureCode ::= 32
id-PWSFailureIndication						ProcedureCode ::= 33
id-PWSRestartIndication						ProcedureCode ::= 34
id-RANConfigurationUpdate					ProcedureCode ::= 35
id-RerouteNASRequest						ProcedureCode ::= 36
id-RRCInactiveTransitionReport				ProcedureCode ::= 37
id-TraceFailureIndication					ProcedureCode ::= 38
id-TraceStart								ProcedureCode ::= 39
id-UEContextModification					ProcedureCode ::= 40
id-UEContextRelease							ProcedureCode ::= 41
id-UEContextReleaseRequest					ProcedureCode ::= 42
id-UERadioCapabilityCheck					ProcedureCode ::= 43
id-UERadioCapabilityInfoIndication			ProcedureCode ::= 44
id-UETNLABindingRelease						ProcedureCode ::= 45
id-UplinkNASTransport						ProcedureCode ::= 46
id-UplinkNonUEAssociatedNRPPaTransport		ProcedureCode ::= 47
id-UplinkRANConfigurationTransfer			ProcedureCode ::= 48
id-UplinkRANStatusTransfer					ProcedureCode ::= 49
id-UplinkUEAssociatedNRPPaTransport			ProcedureCode ::= 50
id-WriteReplaceWarning						ProcedureCode ::= 51
id-SecondaryRATDataUsageReport				ProcedureCode ::= 52

-- **************************************************************
--
-- Extension constants
--
-- **************************************************************

maxPrivateIEs							INTEGER ::= 65535
maxProtocolExtensions					INTEGER ::= 65535
maxProtocolIEs							INTEGER ::= 65535

-- **************************************************************
--
-- Lists
--
-- **************************************************************

	maxnoofAllowedAreas					INTEGER ::= 16
	maxnoofAllowedS-NSSAIs				INTEGER ::= 8
	maxnoofBPLMNs						INTEGER ::= 12
	maxnoofCellIDforWarning				INTEGER ::= 65535
	maxnoofCellinAoI					INTEGER ::= 256
	maxnoofCellinEAI					INTEGER ::= 65535
	maxnoofCellinTAI					INTEGER ::= 65535
	maxnoofCellsingNB					INTEGER ::= 16384
	maxnoofCellsinngeNB					INTEGER ::= 256
	maxnoofCellsinUEHistoryInfo			INTEGER ::= 16
	maxnoofCellsUEMovingTrajectory		INTEGER ::= 16
	maxnoofDRBs							INTEGER ::= 32
	maxnoofEmergencyAreaID				INTEGER ::= 65535
	maxnoofEAIforRestart				INTEGER ::= 256
	maxnoofEPLMNs						INTEGER ::= 15
	maxnoofEPLMNsPlusOne				INTEGER ::= 16
	maxnoofE-RABs						INTEGER ::= 256
	maxnoofErrors						INTEGER ::= 256
	maxnoofForbTACs						INTEGER ::= 4096
	maxnoofMultiConnectivity				INTEGER ::= 4
	maxnoofMultiConnectivityMinusOne	INTEGER ::= 3
	maxnoofNGConnectionsToReset			INTEGER ::= 65536
	maxnoofPDUSessions					INTEGER ::= 256
	maxnoofPLMNs						INTEGER ::= 12
	maxnoofQosFlows						INTEGER ::= 64
	maxnoofRANNodeinAoI					INTEGER ::= 64
	maxnoofRecommendedCells				INTEGER ::= 16
	maxnoofRecommendedRANNodes			INTEGER ::= 16
	maxnoofAoI							INTEGER ::= 64
	maxnoofServedGUAMIs					INTEGER ::= 256
	maxnoofSliceItems					INTEGER ::= 1024
	maxnoofTACs							INTEGER ::= 256
	maxnoofTAIforInactive				INTEGER ::= 16
	maxnoofTAIforPaging					INTEGER ::= 16
	maxnoofTAIforRestart				INTEGER ::= 2048
	maxnoofTAIforWarning				INTEGER ::= 65535
	maxnoofTAIinAoI						INTEGER ::= 16
	maxnoofTimePeriods					INTEGER ::= 2
	maxnoofTNLAssociations				INTEGER ::= 32
	maxnoofXnExtTLAs					INTEGER ::= 16
	maxnoofXnGTP-TLAs					INTEGER ::= 16
	maxnoofXnTLAs						INTEGER ::= 2

-- **************************************************************
--
-- IEs
--
-- **************************************************************

	id-AllowedNSSAI											ProtocolIE-ID ::= 0
	id-AMFName												ProtocolIE-ID ::= 1
	id-AMFOverloadResponse									ProtocolIE-ID ::= 2
	id-AMFSetID												ProtocolIE-ID ::= 3
	id-AMF-TNLAssociationFailedToSetupList					ProtocolIE-ID ::= 4
	id-AMF-TNLAssociationSetupList							ProtocolIE-ID ::= 5
	id-AMF-TNLAssociationToAddList							ProtocolIE-ID ::= 6
	id-AMF-TNLAssociationToRemoveList						ProtocolIE-ID ::= 7
	id-AMF-TNLAssociationToUpdateList						ProtocolIE-ID ::= 8
	id-AMFTrafficLoadReductionIndication					ProtocolIE-ID ::= 9
	id-AMF-UE-NGAP-ID										ProtocolIE-ID ::= 10
	id-AssistanceDataForPaging								ProtocolIE-ID ::= 11
	id-BroadcastCancelledAreaList							ProtocolIE-ID ::= 12
	id-BroadcastCompletedAreaList							ProtocolIE-ID ::= 13
	id-CancelAllWarningMessages								ProtocolIE-ID ::= 14
	id-Cause												ProtocolIE-ID ::= 15
	id-CellIDListForRestart									ProtocolIE-ID ::= 16
	id-ConcurrentWarningMessageInd							ProtocolIE-ID ::= 17
	id-CoreNetworkAssistanceInformationForInactive			ProtocolIE-ID ::= 18
	id-CriticalityDiagnostics								ProtocolIE-ID ::= 19
	id-DataCodingScheme										ProtocolIE-ID ::= 20
	id-DefaultPagingDRX										ProtocolIE-ID ::= 21
	id-DirectForwardingPathAvailability						ProtocolIE-ID ::= 22
	id-EmergencyAreaIDListForRestart						ProtocolIE-ID ::= 23
	id-EmergencyFallbackIndicator							ProtocolIE-ID ::= 24
	id-EUTRA-CGI											ProtocolIE-ID ::= 25
	id-FiveG-S-TMSI											ProtocolIE-ID ::= 26
	id-GlobalRANNodeID										ProtocolIE-ID ::= 27
	id-GUAMI												ProtocolIE-ID ::= 28
	id-HandoverType											ProtocolIE-ID ::= 29
	id-IMSVoiceSupportIndicator								ProtocolIE-ID ::= 30
	id-IndexToRFSP											ProtocolIE-ID ::= 31
	id-InfoOnRecommendedCellsAndRANNodesForPaging			ProtocolIE-ID ::= 32
	id-LocationReportingRequestType							ProtocolIE-ID ::= 33
	id-MaskedIMEISV											ProtocolIE-ID ::= 34
	id-MessageIdentifier									ProtocolIE-ID ::= 35
	id-MobilityRestrictionList								ProtocolIE-ID ::= 36
	id-NASC													ProtocolIE-ID ::= 37
	id-NAS-PDU												ProtocolIE-ID ::= 38
	id-NASSecurityParametersFromNGRAN						ProtocolIE-ID ::= 39
	id-NewAMF-UE-NGAP-ID									ProtocolIE-ID ::= 40
	id-NewSecurityContextInd								ProtocolIE-ID ::= 41
	id-NGAP-Message											ProtocolIE-ID ::= 42
	id-NGRAN-CGI											ProtocolIE-ID ::= 43
	id-NGRANTraceID											ProtocolIE-ID ::= 44
	id-NR-CGI												ProtocolIE-ID ::= 45
	id-NRPPa-PDU											ProtocolIE-ID ::= 46
	id-NumberOfBroadcastsRequested							ProtocolIE-ID ::= 47
	id-OldAMF												ProtocolIE-ID ::= 48
	id-OverloadStartNSSAIList								ProtocolIE-ID ::= 49
	id-PagingDRX											ProtocolIE-ID ::= 50
	id-PagingOrigin											ProtocolIE-ID ::= 51
	id-PagingPriority										ProtocolIE-ID ::= 52
	id-PDUSessionResourceAdmittedList						ProtocolIE-ID ::= 53
	id-PDUSessionResourceFailedToModifyListModRes			ProtocolIE-ID ::= 54
	id-PDUSessionResourceFailedToSetupListCxtRes			ProtocolIE-ID ::= 55
	id-PDUSessionResourceFailedToSetupListHOAck				ProtocolIE-ID ::= 56
	id-PDUSessionResourceFailedToSetupListPSReq				ProtocolIE-ID ::= 57
	id-PDUSessionResourceFailedToSetupListSURes				ProtocolIE-ID ::= 58
	id-PDUSessionResourceHandoverList						ProtocolIE-ID ::= 59
	id-PDUSessionResourceListCxtRelCpl						ProtocolIE-ID ::= 60
	id-PDUSessionResourceListHORqd							ProtocolIE-ID ::= 61
	id-PDUSessionResourceModifyListModCfm					ProtocolIE-ID ::= 62
	id-PDUSessionResourceModifyListModInd					ProtocolIE-ID ::= 63
	id-PDUSessionResourceModifyListModReq					ProtocolIE-ID ::= 64
	id-PDUSessionResourceModifyListModRes					ProtocolIE-ID ::= 65
	id-PDUSessionResourceNotifyList							ProtocolIE-ID ::= 66
	id-PDUSessionResourceReleasedListNot					ProtocolIE-ID ::= 67
	id-PDUSessionResourceReleasedListPSAck					ProtocolIE-ID ::= 68
	id-PDUSessionResourceReleasedListPSFail					ProtocolIE-ID ::= 69
	id-PDUSessionResourceReleasedListRelRes					ProtocolIE-ID ::= 70
	id-PDUSessionResourceSetupListCxtReq					ProtocolIE-ID ::= 71
	id-PDUSessionResourceSetupListCxtRes					ProtocolIE-ID ::= 72
	id-PDUSessionResourceSetupListHOReq						ProtocolIE-ID ::= 73
	id-PDUSessionResourceSetupListSUReq						ProtocolIE-ID ::= 74
	id-PDUSessionResourceSetupListSURes						ProtocolIE-ID ::= 75
	id-PDUSessionResourceToBeSwitchedDLList					ProtocolIE-ID ::= 76
	id-PDUSessionResourceSwitchedList						ProtocolIE-ID ::= 77
	id-PDUSessionResourceToReleaseListHOCmd					ProtocolIE-ID ::= 78
	id-PDUSessionResourceToReleaseListRelCmd				ProtocolIE-ID ::= 79
	id-PLMNSupportList										ProtocolIE-ID ::= 80
	id-PWSFailedCellIDList									ProtocolIE-ID ::= 81
	id-RANNodeName											ProtocolIE-ID ::= 82
	id-RANPagingPriority									ProtocolIE-ID ::= 83
	id-RANStatusTransfer-TransparentContainer				ProtocolIE-ID ::= 84
	id-RAN-UE-NGAP-ID										ProtocolIE-ID ::= 85
	id-RelativeAMFCapacity									ProtocolIE-ID ::= 86
	id-RepetitionPeriod										ProtocolIE-ID ::= 87
	id-ResetType											ProtocolIE-ID ::= 88
	id-RoutingID											ProtocolIE-ID ::= 89
	id-RRCEstablishmentCause								ProtocolIE-ID ::= 90
	id-RRCInactiveTransitionReportRequest					ProtocolIE-ID ::= 91
	id-RRCState												ProtocolIE-ID ::= 92
	id-SecurityContext										ProtocolIE-ID ::= 93
	id-SecurityKey											ProtocolIE-ID ::= 94
	id-SerialNumber											ProtocolIE-ID ::= 95
	id-ServedGUAMIList										ProtocolIE-ID ::= 96
	id-SliceSupportList										ProtocolIE-ID ::= 97
	id-SONConfigurationTransferDL							ProtocolIE-ID ::= 98
	id-SONConfigurationTransferUL							ProtocolIE-ID ::= 99
	id-SourceAMF-UE-NGAP-ID									ProtocolIE-ID ::= 100
	id-SourceToTarget-TransparentContainer					ProtocolIE-ID ::= 101
	id-SupportedTAList										ProtocolIE-ID ::= 102
	id-TAIListForPaging										ProtocolIE-ID ::= 103
	id-TAIListForRestart									ProtocolIE-ID ::= 104
	id-TargetID												ProtocolIE-ID ::= 105
	id-TargetToSource-TransparentContainer					ProtocolIE-ID ::= 106
	id-TimeToWait											ProtocolIE-ID ::= 107
	id-TraceActivation										ProtocolIE-ID ::= 108
	id-TraceCollectionEntityIPAddress						ProtocolIE-ID ::= 109
	id-UEAggregateMaximumBitRate							ProtocolIE-ID ::= 110
	id-UE-associatedLogicalNG-connectionList				ProtocolIE-ID ::= 111
	id-UEContextRequest										ProtocolIE-ID ::= 112
	id-UE-NGAP-IDs											ProtocolIE-ID ::= 114
	id-UEPagingIdentity										ProtocolIE-ID ::= 115
	id-UEPresenceInAreaOfInterestList						ProtocolIE-ID ::= 116
	id-UERadioCapability									ProtocolIE-ID ::= 117
	id-UERadioCapabilityForPaging							ProtocolIE-ID ::= 118
	id-UESecurityCapabilities								ProtocolIE-ID ::= 119
	id-UnavailableGUAMIList									ProtocolIE-ID ::= 120
	id-UserLocationInformation								ProtocolIE-ID ::= 121
	id-WarningAreaList										ProtocolIE-ID ::= 122
	id-WarningMessageContents								ProtocolIE-ID ::= 123
	id-WarningSecurityInfo									ProtocolIE-ID ::= 124
	id-WarningType											ProtocolIE-ID ::= 125
	id-AdditionalUL-NGU-UP-TNLInformation					ProtocolIE-ID ::= 126
	id-DataForwardingNotPossible							ProtocolIE-ID ::= 127
	id-DL-NGU-UP-TNLInformation								ProtocolIE-ID ::= 128
	id-NetworkInstance										ProtocolIE-ID ::= 129
	id-PDUSessionAggregateMaximumBitRate					ProtocolIE-ID ::= 130
	id-PDUSessionResourceFailedToModifyListModCfm			ProtocolIE-ID ::= 131
	id-PDUSessionResourceFailedToSetupListCxtFail			ProtocolIE-ID ::= 132
	id-PDUSessionResourceListCxtRelReq						ProtocolIE-ID ::= 133
	id-PDUSessionType										ProtocolIE-ID ::= 134
	id-QosFlowAddOrModifyRequestList						ProtocolIE-ID ::= 135
	id-QosFlowSetupRequestList								ProtocolIE-ID ::= 136
	id-QosFlowToReleaseList									ProtocolIE-ID ::= 137
	id-SecurityIndication									ProtocolIE-ID ::= 138
	id-UL-NGU-UP-TNLInformation								ProtocolIE-ID ::= 139
	id-UL-NGU-UP-TNLModifyList								ProtocolIE-ID ::= 140
	id-WarningAreaCoordinates								ProtocolIE-ID ::= 141
	id-PDUSessionResourceSecondaryRATUsageList				ProtocolIE-ID ::= 142
	id-HandoverFlag											ProtocolIE-ID ::= 143
	id-SecondaryRATUsageInformation							ProtocolIE-ID ::= 144
	id-PDUSessionResourceReleaseResponseTransfer			ProtocolIE-ID ::= 145
	id-RedirectionVoiceFallback								ProtocolIE-ID ::= 146
	id-UERetentionInformation								ProtocolIE-ID ::= 147
	id-S-NSSAI												ProtocolIE-ID ::= 148
	id-PSCellInformation									ProtocolIE-ID ::= 149
	id-LastEUTRAN-PLMNIdentity								ProtocolIE-ID ::= 150
	id-MaximumIntegrityProtectedDataRate-DL					ProtocolIE-ID ::= 151
	id-AdditionalDLForwardingUPTNLInformation				ProtocolIE-ID ::= 152
	id-AdditionalDLUPTNLInformationForHOList				ProtocolIE-ID ::= 153
	id-AdditionalNGU-UP-TNLInformation						ProtocolIE-ID ::= 154
	id-AdditionalDLQosFlowPerTNLInformation					ProtocolIE-ID ::= 155
	id-SecurityResult										ProtocolIE-ID ::= 156
	id-ENDC-SONConfigurationTransferDL						ProtocolIE-ID ::= 157
	id-ENDC-SONConfigurationTransferUL						ProtocolIE-ID ::= 158
	id-OldAssociatedQosFlowList-ULendmarkerexpected			ProtocolIE-ID ::= 159
	id-CNTypeRestrictionsForEquivalent						ProtocolIE-ID ::= 160
	id-CNTypeRestrictionsForServing							ProtocolIE-ID ::= 161
	id-NewGUAMI												ProtocolIE-ID ::= 162
	id-ULForwarding											ProtocolIE-ID ::= 163
	id-ULForwardingUP-TNLInformation						ProtocolIE-ID ::= 164
	id-CNAssistedRANTuning									ProtocolIE-ID ::= 165
	id-CommonNetworkInstance								ProtocolIE-ID ::= 166
	id-NGRAN-TNLAssociationToRemoveList						ProtocolIE-ID ::= 167
	id-TNLAssociationTransportLayerAddressNGRAN				ProtocolIE-ID ::= 168
	id-EndpointIPAddressAndPort								ProtocolIE-ID ::= 169
	id-LocationReportingAdditionalInfo						ProtocolIE-ID ::= 170
	id-SourceToTarget-AMFInformationReroute					ProtocolIE-ID ::= 171
	id-AdditionalULForwardingUPTNLInformation				ProtocolIE-ID ::= 172
	id-SCTP-TLAs											ProtocolIE-ID ::= 173
	id-SelectedPLMNIdentity									ProtocolIE-ID ::= 174


END
-- ASN1STOP

-- ASN1START
-- **************************************************************
--
-- Container definitions
--
-- **************************************************************

NGAP-Containers {
itu-t (0) identified-organization (4) etsi (0) mobileDomain (0) 
ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-Containers (5) }

DEFINITIONS AUTOMATIC TAGS ::= 

BEGIN

-- **************************************************************
--
-- IE parameter types from other modules.
--
-- **************************************************************

IMPORTS

	Criticality,
	Presence,
	PrivateIE-ID,
	ProtocolExtensionID,
	ProtocolIE-ID
FROM NGAP-CommonDataTypes

	maxPrivateIEs,
	maxProtocolExtensions,
	maxProtocolIEs
FROM NGAP-Constants;

-- **************************************************************
--
-- Class Definition for Protocol IEs
--
-- **************************************************************

NGAP-PROTOCOL-IES ::= CLASS {
	&id				ProtocolIE-ID					UNIQUE,
	&criticality	Criticality,
	&Value,
	&presence		Presence
}
WITH SYNTAX {
	ID				&id
	CRITICALITY		&criticality
	TYPE			&Value
	PRESENCE		&presence
}

-- **************************************************************
--
-- Class Definition for Protocol IEs
--
-- **************************************************************

NGAP-PROTOCOL-IES-PAIR ::= CLASS {
	&id					ProtocolIE-ID				UNIQUE,
	&firstCriticality	Criticality,
	&FirstValue,
	&secondCriticality	Criticality,
	&SecondValue,
	&presence			Presence
}
WITH SYNTAX {
	ID						&id
	FIRST CRITICALITY		&firstCriticality
	FIRST TYPE				&FirstValue
	SECOND CRITICALITY		&secondCriticality
	SECOND TYPE				&SecondValue
	PRESENCE				&presence
}

-- **************************************************************
--
-- Class Definition for Protocol Extensions
--
-- **************************************************************

NGAP-PROTOCOL-EXTENSION ::= CLASS {
	&id				ProtocolExtensionID			UNIQUE,
	&criticality	Criticality,
	&Extension,
	&presence		Presence
}
WITH SYNTAX {
	ID				&id
	CRITICALITY		&criticality
	EXTENSION		&Extension
	PRESENCE		&presence
}

-- **************************************************************
--
-- Class Definition for Private IEs
--
-- **************************************************************

NGAP-PRIVATE-IES ::= CLASS {
	&id				PrivateIE-ID,
	&criticality	Criticality,
	&Value,
	&presence		Presence
}
WITH SYNTAX {
	ID				&id
	CRITICALITY		&criticality
	TYPE			&Value
	PRESENCE		&presence
}

-- **************************************************************
--
-- Container for Protocol IEs
--
-- **************************************************************

ProtocolIE-Container {NGAP-PROTOCOL-IES : IEsSetParam} ::= 
	SEQUENCE (SIZE (0..maxProtocolIEs)) OF
	ProtocolIE-Field {{IEsSetParam}}

ProtocolIE-SingleContainer {NGAP-PROTOCOL-IES : IEsSetParam} ::= 
	ProtocolIE-Field {{IEsSetParam}}

ProtocolIE-Field {NGAP-PROTOCOL-IES : IEsSetParam} ::= SEQUENCE {
	id				NGAP-PROTOCOL-IES.&id				({IEsSetParam}),
	criticality		NGAP-PROTOCOL-IES.&criticality		({IEsSetParam}{@id}),
	value			NGAP-PROTOCOL-IES.&Value			({IEsSetParam}{@id})
}

-- **************************************************************
--
-- Container for Protocol IE Pairs
--
-- **************************************************************

ProtocolIE-ContainerPair {NGAP-PROTOCOL-IES-PAIR : IEsSetParam} ::= 
	SEQUENCE (SIZE (0..maxProtocolIEs)) OF
	ProtocolIE-FieldPair {{IEsSetParam}}

ProtocolIE-FieldPair {NGAP-PROTOCOL-IES-PAIR : IEsSetParam} ::= SEQUENCE {
	id					NGAP-PROTOCOL-IES-PAIR.&id					({IEsSetParam}),
	firstCriticality	NGAP-PROTOCOL-IES-PAIR.&firstCriticality	({IEsSetParam}{@id}),
	firstValue			NGAP-PROTOCOL-IES-PAIR.&FirstValue			({IEsSetParam}{@id}),
	secondCriticality	NGAP-PROTOCOL-IES-PAIR.&secondCriticality	({IEsSetParam}{@id}),
	secondValue			NGAP-PROTOCOL-IES-PAIR.&SecondValue			({IEsSetParam}{@id})
}

-- **************************************************************
--
-- Container Lists for Protocol IE Containers
--
-- **************************************************************

ProtocolIE-ContainerList {INTEGER : lowerBound, INTEGER : upperBound, NGAP-PROTOCOL-IES : IEsSetParam} ::=
	SEQUENCE (SIZE (lowerBound..upperBound)) OF
	ProtocolIE-SingleContainer {{IEsSetParam}}

ProtocolIE-ContainerPairList {INTEGER : lowerBound, INTEGER : upperBound, NGAP-PROTOCOL-IES-PAIR : IEsSetParam} ::=
	SEQUENCE (SIZE (lowerBound..upperBound)) OF
	ProtocolIE-ContainerPair {{IEsSetParam}}

-- **************************************************************
--
-- Container for Protocol Extensions
--
-- **************************************************************

ProtocolExtensionContainer {NGAP-PROTOCOL-EXTENSION : ExtensionSetParam} ::= 
	SEQUENCE (SIZE (1..maxProtocolExtensions)) OF
	ProtocolExtensionField {{ExtensionSetParam}}

ProtocolExtensionField {NGAP-PROTOCOL-EXTENSION : ExtensionSetParam} ::= SEQUENCE {
	id					NGAP-PROTOCOL-EXTENSION.&id				({ExtensionSetParam}),
	criticality			NGAP-PROTOCOL-EXTENSION.&criticality	({ExtensionSetParam}{@id}),
	extensionValue		NGAP-PROTOCOL-EXTENSION.&Extension		({ExtensionSetParam}{@id})
}

-- **************************************************************
--
-- Container for Private IEs
--
-- **************************************************************

PrivateIE-Container {NGAP-PRIVATE-IES : IEsSetParam } ::= 
	SEQUENCE (SIZE (1..maxPrivateIEs)) OF
	PrivateIE-Field {{IEsSetParam}}

PrivateIE-Field {NGAP-PRIVATE-IES : IEsSetParam} ::= SEQUENCE {
	id					NGAP-PRIVATE-IES.&id				({IEsSetParam}),
	criticality			NGAP-PRIVATE-IES.&criticality		({IEsSetParam}{@id}),
	value				NGAP-PRIVATE-IES.&Value				({IEsSetParam}{@id})
}

END
-- ASN1STOP